   PPVPN-PIB PIB-DEFINITIONS ::= BEGIN 
   
   IMPORTS 
       ibrpib
               FROM TUBS-SMI
       Unsigned32, Integer32, MODULE-IDENTITY, MODULE-COMPLIANCE, 
       OBJECT-TYPE, OBJECT-GROUP, pib, TEXTUAL-CONVENTION 
               FROM COPS-PR-SPPI 
       InstanceId, ReferenceId, Prid, TagId, TagReferenceId 
               FROM COPS-PR-SPPI-TC 
       zeroDotZero 
            FROM SNMPv2-SMI 
       TruthValue, DisplayString
               FROM SNMPv2-TC 
       RoleCombination, AttrIdentifier 
               FROM FRAMEWORK-TC-PIB
       InetAddress, InetAddressType
               FROM INET-ADDRESS-MIB
       SnmpAdminString
               FROM SNMP-FRAMEWORK-MIB
       InterfaceIndexOrZero
               FROM IF-MIB;
   
   
   ppvpn2547PolicyPib  MODULE-IDENTITY 
       SUBJECT-CATEGORIES { all } -- PPVPN COPS Client Type 
                                  -- to be assigned by IANA 
       LAST-UPDATED "200203081800Z" 
       ORGANIZATION "IETF PPVPN WG" 
       CONTACT-INFO " 
                      Yacine El Mghazli
                      Alcatel R&I
                      Route de Nozay
                      F-91460 Marcoussis - FRANCE
                      Phone: +33 1 69 63 41 87
                      Email: yacine.el_mghazli@alcatel.fr"
       DESCRIPTION 
            "The PIB module containing a set of provisioning classes 
            that describe provider provisioned virtual private networks 
            (PPVPN) policies for BGP/MPLS VPN. It includes general 
            classes that may be extended by other PIB specifications as 
            well as a set of PIB classes related to PPVPNs." 
       REVISION "200203081800Z" 
       DESCRIPTION 
            "Initial version, published as RFC xxxx." 
       ::= { ibrpib 18 } -- xxx to be assigned by IANA 
   
   
-- BGP/MPLS VPN specific Textual Conventions.
   
   Ppvpn2547RouteDistinguisher ::= TEXTUAL-CONVENTION
      STATUS        current
      DESCRIPTION
          "Syntax for a route distinguisher."
      SYNTAX  OCTET STRING(SIZE (0..256))
   
   Ppvpn2547RouteTarget ::= TEXTUAL-CONVENTION
      STATUS        current
      DESCRIPTION
          "Syntax for a route target."
      SYNTAX  OCTET STRING(SIZE (0..256))
   
   
-- BGP/MPLS VPN PIB module
   
   ppvpn2547CapabilityClasses 
      OBJECT IDENTIFIER ::= { ppvpn2547PolicyPib 1 } 
   ppvpn2547PolicyClasses 
      OBJECT IDENTIFIER ::= { ppvpn2547PolicyPib 2 } 
   ppvpn2547PibConformance 
      OBJECT IDENTIFIER ::= { ppvpn2547PolicyPib 3 } 
   
   
-- Capabilities Group

-- 
-- BGP/MPLS VPN PE Routing Capabilities
-- 
   
   ppvpn2547RoutingCapsTable OBJECT-TYPE 
       SYNTAX         SEQUENCE OF Ppvpn2547RoutingCapsEntry 
       PIB-ACCESS     notify 
       STATUS         current 
       DESCRIPTION 
           "This class represents routing capabilities of a device
            (PE)."
       ::= { ppvpn2547CapabilityClasses 1 } 
   
   ppvpn2547RoutingCapsEntry OBJECT-TYPE 
      SYNTAX         Ppvpn2547RoutingCapsEntry 
      STATUS         current 
      DESCRIPTION 
          "An instance of the ppvpn2547RoutingCaps class." 
      PIB-INDEX { ppvpn2547RoutingCapsPrid } 
      ::= { ppvpn2547RoutingCapsTable 1 } 
   
   Ppvpn2547RoutingCapsEntry ::= SEQUENCE { 
           ppvpn2547RoutingCapsPrid           InstanceId,
           ppvpn2547RoutingCapsDistProtocol   BITS,
           ppvpn2547RoutingCapsMaxRoutes      Unsigned32,
   
           ppvpn2547RoutingCapsMaxVrfs        Unsigned32
   }
   
   ppvpn2547RoutingCapsPrid OBJECT-TYPE 
       SYNTAX         InstanceId 
       STATUS         current 
       DESCRIPTION 
           "An arbitrary integer index that uniquely identifies an 
           instance of the class." 
       ::= { ppvpn2547RoutingCapsEntry 1 } 
   
   ppvpn2547RoutingCapsDistProtocol OBJECT-TYPE 
       SYNTAX         BITS { none  (0),
                             ebgp  (1),
                             ospf  (2),
                             rip   (3),
                             isis  (4),
                             other (5)
       }
       STATUS         current 
       DESCRIPTION 
           "Denotes the route distribution protocol supported by the PE 
            across the PE-CE links. Note that more than one routing 
            protocol may be enabled at the same time."
       ::= { ppvpn2547RoutingCapsEntry 2 } 
   
   ppvpn2547RoutingCapsMaxRoutes OBJECT-TYPE 
       SYNTAX        Unsigned32
       STATUS        current
       DESCRIPTION
          "Denotes maximum number of routes which this PE is 
           able to hold."
       ::= { ppvpn2547RoutingCapsEntry 3 } 
   
   ppvpn2547RoutingCapsMaxVrfs OBJECT-TYPE 
       SYNTAX        Unsigned32
       STATUS        current
       DESCRIPTION
          "Denotes maximum number of VRF which this PE is 
           able to hold."
       ::= { ppvpn2547RoutingCapsEntry 4 } 
   
   
-- 
-- PE Interface Capabilities 
-- 
   
   ppvpn2547IfCapsTable OBJECT-TYPE 
       SYNTAX         SEQUENCE OF Ppvpn2547IfCapsEntry 
       PIB-ACCESS     notify 
       STATUS         current 
       DESCRIPTION 
         " This class represents interfaces capabilities of a device 
   
           (PE) in terms of MPLS support." 
       ::= { ppvpn2547CapabilityClasses 2 } 
   
   ppvpn2547IfCapsEntry OBJECT-TYPE 
       SYNTAX         Ppvpn2547IfCapsEntry 
       STATUS         current 
       DESCRIPTION 
         "An instance of the ppvpn2547IfCaps class." 
       PIB-INDEX { ppvpn2547IfCapsPrid } 
       UNIQUENESS {}
   ::= { ppvpn2547IfCapsTable 1 } 
   
   Ppvpn2547IfCapsEntry ::= SEQUENCE { 
           ppvpn2547IfCapsPrid           InstanceId,
           ppvpn2547IfCapsMplsSupport    INTEGER,
           ppvpn2547IfCapsLabelEdgeType  INTEGER
   } 
   
   ppvpn2547IfCapsPrid OBJECT-TYPE 
       SYNTAX         InstanceId 
       STATUS         current 
       DESCRIPTION 
           "An arbitrary integer index that uniquely identifies an 
           instance of the class." 
       ::= { ppvpn2547IfCapsEntry 1 } 
   
   ppvpn2547IfCapsMplsSupport OBJECT-TYPE 
       SYNTAX         INTEGER { nonMpls    (0),
                                mpls       (1),
                                mplsTunnel (2)
       }
       STATUS         current 
       DESCRIPTION 
           " Denotes the interface type in accordance with [IFMIB] which 
             states that the interfaces tables contains information on 
             the managed resource's interfaces and each sub-layer bellow 
             the internetwork layer interface is considered as an  
             interface." 
       ::= { ppvpn2547IfCapsEntry 2 } 
   
   ppvpn2547IfCapsLabelEdgeType OBJECT-TYPE 
       SYNTAX         INTEGER { providerEdge (1),
                                customerEdge (2) 
       }
       STATUS         current 
       DESCRIPTION 
           " Either the providerEdge(0) or customerEdge(1) bit MUST be 
             set. Denotes if the interface is an exterior interface 
            (customerEdge) or a interior interface (providerEdge), 
            regarding to the provider network."
       ::= { ppvpn2547IfCapsEntry 3 } 
   
   
   
-- BGP/MPLS VPN Policy Classes  
    
-- 
-- BGP/MPLS VPN VRF Table 
-- 
   
   ppvpn2547VrfTable OBJECT-TYPE 
       SYNTAX       SEQUENCE OF Ppvpn2547VrfEntry 
       PIB-ACCESS   install 
       STATUS       current 
       DESCRIPTION 
          "This class specifies BGP/MPLS VPN VRF Table associated 
           information. Entries in this table define VRF instances 
           associated with MPLS/VPN interfaces. Note that multiple 
           interfaces can belong to the same VRF instance." 
       ::= { ppvpn2547PolicyClasses 1 } 
   
   ppvpn2547VrfEntry OBJECT-TYPE 
       SYNTAX       Ppvpn2547VrfEntry 
       STATUS       current 
       DESCRIPTION 
          "An entry in this table is created by the provider for
           every VRF capable of supporting MPLS/BGP VPN." 
       PIB-INDEX {  ppvpn2547VrfPrid } 
       UNIQUENESS { ppvpn2547VrfId,
                    ppvpn2547VrfRoles,
                    ppvpn2547VrfIfName,
                    ppvpn2547VrfRD }
       ::= { ppvpn2547VrfTable 1 } 
    
   Ppvpn2547VrfEntry ::= SEQUENCE  { 
       ppvpn2547VrfPrid        InstanceId, 
       ppvpn2547VrfRoles       RoleCombination,
       ppvpn2547VrfIfName      SnmpAdminString,
       ppvpn2547VrfId          TagReferenceId, 
       ppvpn2547VrfDescription SnmpAdminString,
       ppvpn2547VrfRD          Ppvpn2547RouteDistinguisher,
       ppvpn2547VrfMaxRoutes   Unsigned32
   }
   
   ppvpn2547VrfPrid OBJECT-TYPE 
       SYNTAX       InstanceId 
       STATUS       current 
       DESCRIPTION 
          "An arbitrary integer index that uniquely identifies an 
           instance of the class." 
       ::= { ppvpn2547VrfEntry 1 } 
    
   ppvpn2547VrfRoles OBJECT-TYPE 
       SYNTAX       RoleCombination 
       STATUS       current 
       DESCRIPTION 
          "The interfaces to which the VRF is attached to, 
   
   
           specified in terms of roles.  There must exist an entry 
           in the frwkIfRoleComboTable [FR-PIB] specifying 
           this role combination, together with the interface 
           capability set specified by ppvpn2547IfName, prior to 
           association with an instance of this class." 
       ::= { ppvpn2547VrfEntry 2 }

   ppvpn2547VrfIfName OBJECT-TYPE 
       SYNTAX       SnmpAdminString 
       STATUS       current 
       DESCRIPTION 
          "The interface capability set to which the VRF is attached to.
           The interface capability name specified by this attribute 
           must exist in the frwkIfCapSetTable [FR-PIB] prior to 
           association with an instance of this class." 
       ::= { ppvpn2547VrfEntry 3 } 
   
   ppvpn2547VrfId OBJECT-TYPE 
       SYNTAX       TagReferenceId 
       STATUS       current 
       DESCRIPTION 
          "Identifies a VRF instance." 
       ::= { ppvpn2547VrfEntry 4 } 
   
   ppvpn2547VrfDescription OBJECT-TYPE
       SYNTAX        SnmpAdminString
       STATUS        current
       DESCRIPTION
           "The human-readable description of this VRF."
       ::= { ppvpn2547VrfEntry 5 }
   
   ppvpn2547VrfRD OBJECT-TYPE
       SYNTAX        Ppvpn2547RouteDistinguisher
       STATUS        current
       DESCRIPTION
           "The route distinguisher for this VRF."
       ::= { ppvpn2547VrfEntry 6 }
   
   ppvpn2547VrfMaxRoutes OBJECT-TYPE
       SYNTAX        Unsigned32
       STATUS        current
       DESCRIPTION
           "Denotes maximum number of routes which this VRF is 
            configured to hold."
       ::= { ppvpn2547VrfEntry 7 }
   
   
-- 
-- BGP/MPLS VPN Route Target Table
-- 
   
   ppvpn2547RouteTargetTable OBJECT-TYPE
       SYNTAX        SEQUENCE OF Ppvpn2547RouteTargetEntry
   
       PIB-ACCESS    install
       STATUS        current
       DESCRIPTION
           "This table specifies per-VRF route target association. Each 
           entry identifies a connectivity policy supported as part of a 
           VPN."
   ::= { ppvpn2547PolicyClasses 2 }
   
   ppvpn2547RouteTargetEntry OBJECT-TYPE
       SYNTAX        Ppvpn2547RouteTargetEntry
       STATUS        current
       DESCRIPTION
           "An entry in this table is created for each route target 
           configured for a VRF supporting a MPLS/BGP VPN instance. The 
           precedence attribute provides an ordering per-VRF instance."
      PIB-INDEX  { ppvpn2547RouteTargetPrid}
      UNIQUENESS { ppvpn2547RouteTargetVrfId,
                   ppvpn2547RouteTargetType,
--                   ppvpn2547RouteTargetPrecedence,
                   ppvpn2547RouteTargetRT
      }
   ::= { ppvpn2547RouteTargetTable 1 } 
    
Ppvpn2547RouteTargetEntry ::= SEQUENCE {
     ppvpn2547RouteTargetPrid       InstanceId, 
     ppvpn2547RouteTargetType       INTEGER,
     ppvpn2547RouteTargetVrfId      TagId,
--     ppvpn2547RouteTargetPrecedence Unsigned32,
     ppvpn2547RouteTargetRT         Ppvpn2547RouteTarget,
     ppvpn2547RouteTargetDescr      DisplayString
   }
   
   ppvpn2547RouteTargetPrid OBJECT-TYPE 
       SYNTAX       InstanceId 
       STATUS       current 
       DESCRIPTION 
           "An arbitrary integer index that uniquely identifies an 
           instance of the class." 
       ::= { ppvpn2547RouteTargetEntry 1 }
   
   ppvpn2547RouteTargetType OBJECT-TYPE
       SYNTAX        INTEGER { import(1),
                               export(2),
                               both(3) }
       STATUS        current
       DESCRIPTION
           "The route target distribution type."
       ::= { ppvpn2547RouteTargetEntry 2 }
   
   ppvpn2547RouteTargetVrfId OBJECT-TYPE
       SYNTAX        TagId
       STATUS        current
       DESCRIPTION
   
           " A VRF is composed of an import RT list and a export RT 
           list. Each RT belonging to the same VRF uses the same VRF ID. 
           Hence, a VRF Id identifies which this RT is a part of. This 
           needs to be the value of ppvpn2547VrfId attribute for an 
           existing instance of ppvpn2547VrfEntry."
   ::= { ppvpn2547RouteTargetEntry 3 }
   
   ppvpn2547RouteTargetRT OBJECT-TYPE
       SYNTAX        Ppvpn2547RouteTarget
       STATUS        current
       DESCRIPTION
           "The route target value."
       ::= { ppvpn2547RouteTargetEntry 4 }
   
   ppvpn2547RouteTargetDescr OBJECT-TYPE
       SYNTAX        DisplayString
       STATUS        current
       DESCRIPTION
           "Description of the route target."
       ::= { ppvpn2547RouteTargetEntry 5 }
   
   
-- 
-- BGP/MPLS VPN Interface Table
-- 
   
   ppvpn2547IfTable  OBJECT-TYPE
       SYNTAX        SEQUENCE OF Ppvpn2547IfEntry
       PIB-ACCESS    install
       STATUS        current
       DESCRIPTION
           "This table specifies per-interface configuration information 
            related to PE-CE links."
       ::= { ppvpn2547PolicyClasses 3 }
   
   ppvpn2547IfEntry OBJECT-TYPE
       SYNTAX        Ppvpn2547IfEntry
       STATUS        current
       DESCRIPTION
           "An entry in this table is created for every interface type 
           supporting MPLS/BGP VPN. Each entry in this table is meant to 
           correspond to an entry in the Interfaces Table."
       PIB-INDEX { ppvpn2547IfPrid }
       UNIQUENESS { ppvpn2547IfRoles,
                    ppvpn2547IfName }
       ::= { ppvpn2547IfTable 1 }
   
   Ppvpn2547IfEntry ::= SEQUENCE {
           ppvpn2547IfPrid               InstanceId,
           ppvpn2547IfRoles              RoleCombination,
           ppvpn2547IfName               SnmpAdminString,
           ppvpn2547IfVpnClassification  INTEGER,
           ppvpn2547IfRouteDistProtocol  BITS
   
   }
   
   ppvpn2547IfPrid OBJECT-TYPE 
       SYNTAX       InstanceId 
       STATUS       current 
       DESCRIPTION 
          "An arbitrary integer index that uniquely identifies an 
           instance of the class." 
       ::= { ppvpn2547IfEntry 1 }
   
   ppvpn2547IfName OBJECT-TYPE 
       SYNTAX       SnmpAdminString 
       STATUS       current 
       DESCRIPTION 
          "The interface capability set to configure. The interface 
           capability name specified by this attribute must exist in the 
           frwkIfCapSetTable [FR-PIB] prior to association with an 
           instance of this class." 
       ::= { ppvpn2547IfEntry 2 } 
   
   
   ppvpn2547IfRoles OBJECT-TYPE 
       SYNTAX       RoleCombination 
       STATUS       current
       DESCRIPTION 
          "The interfaces to which the VRF is attached to, 
           specified in terms of roles.  There must exist an entry 
           in the frwkIfRoleComboTable [FR-PIB] specifying 
           this role combination, together with the interface 
           capability set specified by ppvpn2547IfName, prior to 
           association with an instance of this class." 
       ::= { ppvpn2547IfEntry 3 }
   
   ppvpn2547IfVpnClassification OBJECT-TYPE
       SYNTAX        INTEGER { carrierOfCarrier (1),
                               enterprise (2),
                               interProvider (3)
       }
       STATUS        current
       DESCRIPTION
           "Denotes whether this link participates in a carrier-of-
           carrier's, enterprise, or inter-provider scenario."
       ::= { ppvpn2547IfEntry 4 }
   
   ppvpn2547IfRouteDistProtocol OBJECT-TYPE
       SYNTAX        BITS { none  (0),
                            ebgp  (1),
                            ospf  (2),
                            rip   (3),
                            isis  (4),
                            other (5)
       }
       STATUS        current
   
       DESCRIPTION
           "Denotes the route distribution protocol across the PE-CE 
           link. Note that more than one routing protocol may be enabled 
           at the same time."
       ::= { ppvpn2547IfEntry 5 }
   
   
-- 
-- BGP/MPLS VPN BGP Peer Address Table
-- 
    
   ppvpn2547BgpPeerTable OBJECT-TYPE
       SYNTAX        SEQUENCE OF Ppvpn2547BgpPeerEntry
       PIB-ACCESS    install
       STATUS        current
       DESCRIPTION
           "Each entry in this table specifies a per-interface 
            MPLS/BGP neighbor."
       ::= { ppvpn2547PolicyClasses 5 }
   
   ppvpn2547BgpPeerEntry OBJECT-TYPE
       SYNTAX        Ppvpn2547BgpPeerEntry
       STATUS        current
       DESCRIPTION
           "An entry in this table is created by an LSR for
            every VRF capable of supporting MPLS/BGP VPN. The
            indexing provides an ordering of VRFs per-VPN
            interface."
       PIB-INDEX  { ppvpn2547BgpPeerPrid }
       UNIQUENESS { ppvpn2547BgpPeerVrfId,
                    ppvpn2547BgpPeerAddrType,
                    ppvpn2547BgpPeerAddr
       }
       ::= { ppvpn2547BgpPeerTable 1 }
   
   Ppvpn2547BgpPeerEntry ::= SEQUENCE {
           ppvpn2547BgpPeerPrid         InstanceId,
           ppvpn2547BgpPeerVrfId        TagId, 
           ppvpn2547BgpPeerRole         INTEGER,
           ppvpn2547BgpPeerAddrType     InetAddressType,
           ppvpn2547BgpPeerAddr         InetAddress
   }
   
   ppvpn2547BgpPeerPrid OBJECT-TYPE
       SYNTAX        InstanceId
       STATUS        current
       DESCRIPTION
            "An arbitrary integer index that uniquely identifies an 
            instance of the class."
       ::= { ppvpn2547BgpPeerEntry 1 }
   
   ppvpn2547BgpPeerVrfId OBJECT-TYPE
       SYNTAX        TagId
   
       STATUS        current
       DESCRIPTION
           "Each BGP neighbor to the same VRF uses the same VRF ID. 
           Hence, a VRF Id identifies which VRF this device is the 
           neighbor. This needs to be the value of ppvpn2547VrfId
           attribute for an existing instance of ppvpn2547VrfEntry."
   ::= { ppvpn2547BgpPeerEntry 2 }
   
   ppvpn2547BgpPeerRole  OBJECT-TYPE
       SYNTAX        INTEGER { ce(1), 
                               pe(2) 
       }
       STATUS        current
       DESCRIPTION
           "Denotes the role played by this BGP neighbor
            with respect to this VRF."
       ::= { ppvpn2547BgpPeerEntry 3 }
   
   ppvpn2547BgpPeerAddrType  OBJECT-TYPE
       SYNTAX        InetAddressType
       STATUS        current
       DESCRIPTION
           "Denotes the address family of the PE address."
       ::= { ppvpn2547BgpPeerEntry 4 }
    
   ppvpn2547BgpPeerAddr  OBJECT-TYPE
       SYNTAX        InetAddress
       STATUS        current
       DESCRIPTION
       "Denotes the EBGP neighbor address."
   ::= { ppvpn2547BgpPeerEntry 5 }
   
   
-- 
-- VRF Routing Table
-- 
   
   ppvpn2547RouteTable  OBJECT-TYPE
       SYNTAX        SEQUENCE OF Ppvpn2547RouteEntry
       PIB-ACCESS    install
       STATUS        current
       DESCRIPTION
           "This table specifies per-VRF MPLS/BGP VPN routing 
           information. Entries in this table define VRF routing entries 
           associated with the specified MPLS/VPN interfaces. Note
           that this table contains both BGP and IGP routes, as both may
           appear in the same VRF." 
       ::= { ppvpn2547PolicyClasses 4 }
   
   ppvpn2547RouteEntry OBJECT-TYPE
       SYNTAX        Ppvpn2547RouteEntry 
       STATUS        current
       DESCRIPTION
           "An entry in this table is created by an LSR for every route
   
            present configured (either dynamically or statically) within
            the context of a specific VRF capable of supporting MPLS/BGP
            VPN. The indexing provides an ordering of VRFs per-VPN
            interface."
       PIB-INDEX { ppvpn2547RoutePrid }
       UNIQUENESS { ppvpn2547RouteVrfId,
                    ppvpn2547RouteDest,
                    ppvpn2547RouteMask,
                    ppvpn2547RouteTos,
                    ppvpn2547RouteNextHop }
          ::= { ppvpn2547RouteTable 1 }
   
   Ppvpn2547RouteEntry ::= SEQUENCE {
           ppvpn2547RoutePrid               InstanceId,
           ppvpn2547RouteVrfId              TagId,
           ppvpn2547RouteDest               InetAddress,
           ppvpn2547RouteDestAddrType       InetAddressType,
           ppvpn2547RouteMask               InetAddress,
           ppvpn2547RouteMaskAddrType       InetAddressType,
           ppvpn2547RouteTos                Unsigned32,
           ppvpn2547RouteNextHop            InetAddress,
           ppvpn2547RouteNextHopAddrType    InetAddressType,
           ppvpn2547RouteIfIndex            InterfaceIndexOrZero,
           ppvpn2547RouteType               INTEGER,
           ppvpn2547RouteProto              INTEGER,
           ppvpn2547RouteInfo               OBJECT IDENTIFIER,
           ppvpn2547RouteNextHopAS          Unsigned32,
           ppvpn2547RouteMetric1            Integer32,
           ppvpn2547RouteMetric2            Integer32,
           ppvpn2547RouteMetric3            Integer32,
           ppvpn2547RouteMetric4            Integer32,
           ppvpn2547RouteMetric5            Integer32 
   }
   
   ppvpn2547RoutePrid OBJECT-TYPE
       SYNTAX        InstanceId
       STATUS        current
       DESCRIPTION
            "An arbitrary integer index that uniquely identifies an 
            instance of the class."
       ::= { ppvpn2547RouteEntry 1 }
   
   ppvpn2547RouteVrfId OBJECT-TYPE
       SYNTAX        TagId
       STATUS        current
       DESCRIPTION
           "Each route belonging to the same VRF uses the same VRF ID. 
           Hence, a VRF Id identifies which routing table this route is 
           a part of. This needs to be the value of ppvpn2547VrfId 
           attribute for an existing instance of ppvpn2547VrfEntry."
   ::= { ppvpn2547RouteEntry 2 }
   
   ppvpn2547RouteDest  OBJECT-TYPE
   
      SYNTAX        InetAddress 
      STATUS        current
      DESCRIPTION
          "The destination IP address of this route.
           This object may not take a Multicast (Class D)
           address value.
           Any assignment (implicit or otherwise) of an
           instance of this object to a value x must be
           rejected if the bit-wise logical-AND of x with
           the value of the corresponding instance of the
           ppvpn2547RouteMask object is not equal to x."
      ::= { ppvpn2547RouteEntry 3 }
   
   ppvpn2547RouteDestAddrType  OBJECT-TYPE
      SYNTAX        InetAddressType
      STATUS        current
      DESCRIPTION
          "The address type of the ppvpn2547RouteDest
           entry."
      ::= { ppvpn2547RouteEntry 4 }
   
   ppvpn2547RouteMask  OBJECT-TYPE
       SYNTAX        InetAddress 
       STATUS        current
       DESCRIPTION
           "Indicate the mask to be logical-ANDed with the
           destination  address  before  being compared to
           the value  in  the  ppvpn2547RouteDest field.
           For those  systems  that  do  not support
           arbitrary subnet masks, an agent constructs the
           value of the ppvpn2547RouteMask by reference
           to the IP Address Class.
           Any assignment (implicit or otherwise) of an
           instance of this object to a value x must be
           rejected if the bit-wise logical-AND of x with
           the value of the corresponding instance of the
           ppvpn2547RouteDest object is not equal to
           ppvpn2547RouteDest."
       ::= { ppvpn2547RouteEntry 5 }
   
   ppvpn2547RouteMaskAddrType  OBJECT-TYPE
       SYNTAX        InetAddressType 
       STATUS        current
       DESCRIPTION
           "The address type of ppvpn2547RouteMask."
       ::= { ppvpn2547RouteEntry 6 }
   
   ppvpn2547RouteTos  OBJECT-TYPE
       SYNTAX        Unsigned32 
       STATUS        current
       DESCRIPTION
          "The IP TOS Field is used to specify the policy to
          be applied to this route.  The encoding of IP TOS
   
   
          is as specified  by  the  following convention.
          Zero indicates the default path if no more
          specific policy applies.
   
          +-----+-----+-----+-----+-----+-----+-----+-----+
          |                 |                       |     |
          |   PRECEDENCE    |    TYPE OF SERVICE    |  0  |
          |                 |                       |     |
          +-----+-----+-----+-----+-----+-----+-----+-----+
   
                     IP TOS                IP TOS
                Field     Policy      Field     Policy
                Contents    Code      Contents    Code
                0 0 0 0  ==>   0      0 0 0 1  ==>   2
                0 0 1 0  ==>   4      0 0 1 1  ==>   6
                0 1 0 0  ==>   8      0 1 0 1  ==>  10
                0 1 1 0  ==>  12      0 1 1 1  ==>  14
                1 0 0 0  ==>  16      1 0 0 1  ==>  18
                1 0 1 0  ==>  20      1 0 1 1  ==>  22
                1 1 0 0  ==>  24      1 1 0 1  ==>  26
                1 1 1 0  ==>  28      1 1 1 1  ==>  30."
      ::= { ppvpn2547RouteEntry 7 }
   
   ppvpn2547RouteNextHop  OBJECT-TYPE
       SYNTAX        InetAddress 
       STATUS        current
       DESCRIPTION
           "On remote routes, the address of the next
           system en route; Otherwise, 0.0.0.0. ."
       ::= { ppvpn2547RouteEntry 8 }
   
   ppvpn2547RouteNextHopAddrType  OBJECT-TYPE
       SYNTAX        InetAddressType 
       STATUS        current
       DESCRIPTION
           "The address type of the ppvpn2547RouteNextHopAddrType
           object."
       ::= { ppvpn2547RouteEntry 9 }
   
   ppvpn2547RouteIfIndex  OBJECT-TYPE
       SYNTAX        InterfaceIndexOrZero 
       STATUS        current
       DESCRIPTION
           "The ifIndex value that identifies the local
           interface  through  which  the next hop of this
           route should be reached. If this value is set to 0,
           this indicates that no interface is associated with 
           this route."
       ::= { ppvpn2547RouteEntry 10 }
   
   ppvpn2547RouteType  OBJECT-TYPE
       SYNTAX  INTEGER { other  (1), -- not specified
                         reject (2), -- route to discard traffic
   
                         local  (3), -- local interface
                         remote (4)  -- remote destination
                       } 
       STATUS        current
       DESCRIPTION
           "The type of route.  Note that local(3)  refers
           to a route for which the next hop is the final
           destination; remote(4) refers to a route for
           that the next  hop is not the final destination.
           Routes which do not result in traffic forwarding or
           rejection should not be displayed even if the
           implementation keeps them stored internally.
           Reject (2) refers to a route which, if matched,
           discards the message as unreachable. This is used
           in some protocols as a means of correctly aggregating
           routes."
      ::= { ppvpn2547RouteEntry 11 }
   
   ppvpn2547RouteProto  OBJECT-TYPE
       SYNTAX INTEGER { other     (1),  -- not specified
                        local     (2),  -- local interface
                        netmgmt   (3),  -- static route
                        icmp      (4),  -- result of ICMP Redirect
   
                        -- the following are all dynamic
                        -- routing protocols
   
                        egp        (5),  -- Exterior Gateway Protocol
                        ggp        (6),  -- Gateway-Gateway Protocol
                        hello      (7),  -- FuzzBall HelloSpeak
                        rip        (8),  -- Berkeley RIP or RIP-II
                        isIs       (9),  -- Dual IS-IS
                        esIs       (10), -- ISO 9542
                        ciscoIgrp  (11), -- Cisco IGRP
                        bbnSpfIgp  (12), -- BBN SPF IGP
                        ospf       (13), -- Open Shortest Path First
                        bgp        (14), -- Border Gateway Protocol
                        idpr       (15), -- InterDomain Policy Routing
                        ciscoEigrp (16)  -- Cisco EIGRP
                      } 
       STATUS        current
       DESCRIPTION
           "The routing mechanism via which this route was
           learned.  Inclusion of values for gateway rout-
           ing protocols is not  intended  to  imply  that
           hosts should support those protocols."
       ::= { ppvpn2547RouteEntry 12 }
   
   ppvpn2547RouteInfo               OBJECT-TYPE
       SYNTAX        OBJECT IDENTIFIER 
       STATUS        current
       DESCRIPTION
           "A reference to MIB definitions specific to the
   
           particular routing protocol which is responsi-
           ble for this route, as determined by the  value
           specified  in the route's ppvpn2547RouteProto
           value. If this information is not present, its
           value SHOULD be set to the OBJECT IDENTIFIER
           { 0 0 }, which is a syntactically valid object
           identif-ier, and any implementation conforming
           to ASN.1 and the Basic Encoding Rules must be
           able to generate and recognize this value."
       ::= { ppvpn2547RouteEntry 13 }
   
   ppvpn2547RouteNextHopAS          OBJECT-TYPE
       SYNTAX        Unsigned32 
       STATUS        current
       DESCRIPTION
           "The Autonomous System Number of the Next Hop.
           The semantics of this object are determined by
           the routing-protocol specified in the route's
           ppvpn2547RouteProto value. When this object is
           unknown or not relevant its value should be set
           to zero."
       ::= { ppvpn2547RouteEntry 14 }
   
   ppvpn2547RouteMetric1  OBJECT-TYPE
       SYNTAX        Integer32 
       STATUS        current
       DESCRIPTION
           "The primary routing metric for this route.
           The semantics of this metric are determined by
           the routing-protocol specified in  the  route's
           ppvpn2547RouteProto value. If this metric is not
           used, its value should be set to -1."
       ::= { ppvpn2547RouteEntry 15 }
   
   ppvpn2547RouteMetric2  OBJECT-TYPE
       SYNTAX        Integer32
       STATUS        current
       DESCRIPTION
           "An alternate routing metric for this route.
           The semantics of this metric are determined by
           the routing-protocol specified in  the  route's
           ppvpn2547RouteProto value. If this metric is not
           used, its value should be set to -1."
       ::= { ppvpn2547RouteEntry 16 }
   
   ppvpn2547RouteMetric3  OBJECT-TYPE
       SYNTAX        Integer32
       STATUS        current
       DESCRIPTION
           "An alternate routing metric for this route.
           The semantics of this metric are determined by
           the routing-protocol specified in  the  route's
           ppvpn2547RouteProto value. If this metric is not
   
           used, its value should be set to -1."
       ::= { ppvpn2547RouteEntry 17 }
   
   ppvpn2547RouteMetric4  OBJECT-TYPE
       SYNTAX        Integer32
       STATUS        current
       DESCRIPTION
           "An alternate routing metric for this route.
           The semantics of this metric are determined by
           the routing-protocol specified in  the  route's
           ppvpn2547RouteProto value. If this metric is not
           used, its value should be set to -1."
       ::= { ppvpn2547RouteEntry 18 }
   
   ppvpn2547RouteMetric5  OBJECT-TYPE
       SYNTAX        Integer32
       STATUS        current
       DESCRIPTION
           "An alternate routing metric for this route.
           The semantics of this metric are determined by
           the routing-protocol specified in  the  route's
           ppvpn2547RouteProto value. If this metric is not
           used, its value should be set to -1."
       ::= { ppvpn2547RouteEntry 19 }
   
   
   -- 
   -- Conformance Section 
   -- 
    

    
   ppvpn2547PibCompliances 
       OBJECT IDENTIFIER ::= { ppvpn2547PibConformance 1 } 
   ppvpn2547PibGroups 
       OBJECT IDENTIFIER ::= { ppvpn2547PibConformance 2 } 
   
   ppvpn2547PibCompliance MODULE-COMPLIANCE 
       STATUS  current 
       DESCRIPTION 
               "Describes the requirements for conformance to the 
               PPVPN BGP/MPLS VPN Policy PIB." 
        
       MODULE  -- this module 
           MANDATORY-GROUPS { 
               ppvpn2547PibVrfGroup, 
               ppvpn2547PibRouteTargetGroup, 
               ppvpn2547PibIfGroup, 
               ppvpn2547PibBgpPeerGroup,
               ppvpn2547PibRouteGroup
           }
       ::= { ppvpn2547PibCompliances 1 } 
   
   ppvpn2547PibVrfGroup OBJECT-GROUP
       OBJECTS { ppvpn2547VrfRoles,
   
                 ppvpn2547VrfIfName,
                 ppvpn2547VrfId,
                 ppvpn2547VrfDescription,
                 ppvpn2547VrfRD,
                 ppvpn2547VrfMaxRoutes 
       } 
       STATUS current 
       DESCRIPTION 
          "The VRF Group defines the PIB Objects that describe a VRF." 
       ::= { ppvpn2547PibGroups 1 }

   ppvpn2547PibRouteTargetGroup OBJECT-GROUP
       OBJECTS { ppvpn2547RouteTargetType,
                 ppvpn2547RouteTargetVrfId,
--                 ppvpn2547RouteTargetPrecedence,
                 ppvpn2547RouteTargetRT,
                 ppvpn2547RouteTargetDescr
       } 
       STATUS current 
       DESCRIPTION 
          "The Route Target Group defines the PIB Objects  that describe 
          a Route Target." 
       ::= { ppvpn2547PibGroups 2 }

   ppvpn2547PibIfGroup OBJECT-GROUP
       OBJECTS { ppvpn2547IfRoles,
                 ppvpn2547IfName,
                 ppvpn2547IfVpnClassification,
                 ppvpn2547IfRouteDistProtocol  
       } 
       STATUS current 
       DESCRIPTION 
          "The Interface Group defines  the  PIB  Objects  that 
          describe a Interface." 
       ::= { ppvpn2547PibGroups 3 }

   ppvpn2547PibBgpPeerGroup OBJECT-GROUP
       OBJECTS { ppvpn2547BgpPeerVrfId,
                 ppvpn2547BgpPeerRole,
                 ppvpn2547BgpPeerAddrType,
                 ppvpn2547BgpPeerAddr         
       } 
       STATUS current 
       DESCRIPTION 
          "The BGP Peer Group defines  the  PIB  Objects  that 
          describe a BGP Peer." 
       ::= { ppvpn2547PibGroups 4 }
   
   ppvpn2547PibRouteGroup OBJECT-GROUP
       OBJECTS { ppvpn2547RouteVrfId,
                 ppvpn2547RouteDest,
                 ppvpn2547RouteDestAddrType,
   
                 ppvpn2547RouteMask,
                 ppvpn2547RouteMaskAddrType,
                 ppvpn2547RouteTos,
                 ppvpn2547RouteNextHop,
                 ppvpn2547RouteNextHopAddrType,
                 ppvpn2547RouteIfIndex,

                 ppvpn2547RouteType,
                 ppvpn2547RouteProto,
                 ppvpn2547RouteInfo,
                 ppvpn2547RouteNextHopAS,
                 ppvpn2547RouteMetric1,
                 ppvpn2547RouteMetric2,
                 ppvpn2547RouteMetric3,
                 ppvpn2547RouteMetric4,
                 ppvpn2547RouteMetric5
       } 
       STATUS current 
       DESCRIPTION 
          "The Route Group defines the PIB Objects that 
          describe a Route." 
       ::= { ppvpn2547PibGroups 5 }

END
