   FEEDBACK-FRAMEWORK-PIB PIB-DEFINITIONS ::= BEGIN   
         
      IMPORTS   
          ibrpib FROM TUBS-SMI
          Unsigned32, Unsigned64,     
          Integer32, Integer64, MODULE-IDENTITY, OBJECT-TYPE, pib
                  FROM COPS-PR-SPPI   
          TruthValue, TEXTUAL-CONVENTION   
                  FROM SNMPv2-TC   
          InstanceId, ReferenceId, TagReferenceId, TagId, Prid
                  FROM COPS-PR-SPPI-TC
          RoleCombination   
                  FROM POLICY-DEVICE-AUX-MIB
          Counter64, ExtUTCTime
                  FROM SNMPv2-SMI
          IfDirection
                  FROM DIFFSERV-MIB;
         
      feedbackPolFrameworkPib  MODULE-IDENTITY   
          SUBJECT-CATEGORIES  { all }  
          LAST-UPDATED "200011171000Z"   
          ORGANIZATION "IETF RAP WG"   
          CONTACT-INFO "   
                        Diana Rawlins   
                        WorldCom   
                        901 International Parkway   
                        Richardson, TX 75081   
                        Phone: 972 729 1044   
                        Email: diana.rawlins@wcom.com   
         
                       Amol Kulkarni   
                       JF3-206            
                       2111 NE 25th Ave   
                       Hillsboro, Oregon 97124   
                       Phone: 503-712-1168  
                       Email: amol.kulkarni@intel.com   
                      
                       Kwok Ho Chan  
                       Nortel Networks, Inc.  
                       600 Technology Park Drive  
                       Billerica, MA 01821 USA  
                       Phone: 978-288-8175  
                       Email: khchan@nortelnetworks.com  
                       Martin Bokaemper 
                       Unisphere Networks 
                       700 Silver Seven Road 
                       Kanata, ON, K2V 1C3, Canada 
                       Phone: 613-591-2735 
                       Email: mbokaemper@unispherenetworks.com"  
         
         
      DESCRIPTION   
              "The PIB module containing the base set of policy rule  
              classes that are required for support of all policy 
              usage  monitoring, tracking and reporting policies" 
         
            ::= { ibrpib 7 }  -- to be assigned by IANA
   --   
   -- The feedback report group  
   --   
         
   frwkFeedbackGroupClasses    
                  OBJECT IDENTIFIER ::= { feedbackPolFrameworkPib  1 }   
 
   --  
   --  Feedback Action Table  
   --  
     
   frwkFeedbackActionTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackActionEntry   
        PIB-ACCESS      install   
        STATUS          current   
        DESCRIPTION   
                 "This class contains a single PRI that indicates   
                 that the PEP is to resume the sending of   
                 feedback type reports."  
     
           ::= { frwkFeedbackGroupClasses  1}   
         
   frwkFeedbackActionEntry OBJECT-TYPE   
        SYNTAX  FrwkFeedbackActionEntry   
        STATUS  current   
        DESCRIPTION   
                   "An instance of this class can indicates a action 
                    the PEP is to take regarding the usage policies."   
        PIB-INDEX { frwkFeedbackActionId} 
  
           ::= { frwkFeedbackActionTable 1}   
         
   FrwkFeedbackActionEntry ::= SEQUENCE {   
           frwkFeedbackActionId                 InstanceId,   
           frwkFeedbackActionIndicator          INTEGER, 
           frwkFeedbackActionSpecificPri        INTEGER, 
           frwkFeedbackActionList               TagReferenceId
        }   

   frwkFeedbackActionId  OBJECT-TYPE  
        SYNTAX        InstanceId
        STATUS        current  
        DESCRIPTION  
           " An arbitrary integer index that uniquely identifies an   
            instance of the frwkFeedbackActionTable class."  
     
        ::= { frwkFeedbackActionEntry 1}  
     
   frwkFeedbackActionIndicator OBJECT-TYPE   
        SYNTAX  INTEGER {  
                   suspendUsageMonitoringAndReports(0),
                   suspendReportsOnly(1),
                   resumeUsageAndReporting(2),
                   solicitUsageReportNow(3)
        }   
        STATUS  current   
        DESCRIPTION   
                  "The value indicates if the PEP is to send cached   
                   usage policies via feedback type report messages.  
                   The enumeration values are:   
                   (0)  SUSPEND USAGE MONITORING_AND_REPORTS   
                   (1)  SUSPEND_REPORTS_ONLY  
                   (2)  RESUME_USAGE AND REPORTING 
                   (3)  SOLICIT USAGE REPORT NOW "   
         
          ::= { frwkFeedbackActionEntry 2 }   
 
   frwkFeedbackActionSpecificPri OBJECT-TYPE   
           SYNTAX        TruthValue 
           STATUS        current   
           DESCRIPTION   
                   "A value of 0 indicates that the  
                   frwkFeedbackActionListId attribute should be 
                   ignored, and the action applied to all policies. A 
                  value of 1 indicates that the action entry has a 
                  specific list of policies to which it is to be 
                  applied." 
           ::= { frwkFeedbackActionEntry 3}   
    
   frwkFeedbackActionList OBJECT-TYPE   
           SYNTAX        TagReferenceId
           PIB-TAG       { frwkFeedbackActionListGroup }
           STATUS        current   
           DESCRIPTION   
                     "Identifies a list of  
                      frwkFeedbackActionListTable instances  
                      associated with the action described by 
                      this instance" 
           ::= { frwkFeedbackActionEntry 4}   
      
   --  
   --  Feedback Action List Table  
      
   frwkFeedbackActionListTable OBJECT-TYPE    
           SYNTAX          SEQUENCE OF FrwkFeedbackActionListEntry 
           PIB-ACCESS      install    
           STATUS          current    
           DESCRIPTION   
                         "This class contains the PRIDs of the  
                         linkage instance which are to be impacted by  
                         the frwkFeedbackActionIndicator for this 
                         list."  
           ::= { frwkFeedbackGroupClasses  2}    
    
   frwkFeedbackActionListEntry OBJECT-TYPE    
           SYNTAX          FrwkFeedbackActionListEntry 
           STATUS          current    
           DESCRIPTION    
                    "This class identifies a set of linkage instances  
                     for which the  PDP is suspending, resuming or  
                     soliciting usage feedback." 
      
           PIB-INDEX {frwkFeedbackActionListId }   
           UNIQUENESS { frwkFeedbackActionListGroup, 
                        frwkFeedbackActionListPRID  
                      }   
           ::= { frwkFeedbackActionListTable 1}    
         
   FrwkFeedbackActionListEntry::= SEQUENCE {   
              frwkFeedbackActionListId          InstanceId,   
              frwkFeedbackActionListGroup       TagId, 
              frwkFeedbackActionListPRID        Prid  
        }   
    
   frwkFeedbackActionListId OBJECT-TYPE   
           SYNTAX       InstanceId   
           STATUS       current   
           DESCRIPTION   
                     "Arbitrary integer index that uniquely  
                     identifies an instance of the class."   
    
           ::= { frwkFeedbackActionListEntry 1 }   
    
   frwkFeedbackActionListGroup OBJECT-TYPE   
           SYNTAX       TagId   
           STATUS       current   
           DESCRIPTION   
                       "Represents the binding between the Action 
                      table entry and the Action List table entries" 
           ::= { frwkFeedbackActionListEntry 2 }   
    
   frwkFeedbackActionListPRID   OBJECT-TYPE   
           SYNTAX       Prid   
           STATUS       current   
           DESCRIPTION   
                         "The PRID of the linkage instance(s) belonging  
                          to the list of instances identified by the 
                          list id upon which the suspend, resume or  
                          solicit action is directed." 
    
           ::= { frwkFeedbackActionListEntry 3 }   
    
   -- 
   -- The Feedback Selection Usage Combination Capability Table 
   --  
 
   frwkFeedbackSelUsageComboCapsTable OBJECT-TYPE 
        SYNTAX           SEQUENCE OF FrwkFeedbackSelUsageComboCapsEntry 
        PIB-ACCESS       notify 
        STATUS           current 
        DESCRIPTION 
                "This table defines the valid combinations of the 
                 selection criteria PRCs, the usage PRCs and the 
                threshold PRCs that the PEP supports." 
         ::= { frwkFeedbackGroupClasses 3} 
 
 
   frwkFeedbackSelUsageComboCapsEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackSelUsageComboCapsEntry   
        STATUS          current   
        DESCRIPTION   
                 "The attributes of this class identify valid  
                  combinations of selection criteria, usage and 
                  threshold PRCs for feedback supported by the PEP 
                  device."  
        PIB-INDEX {frwkFeedbackSelUsageComboCapId}  
        UNIQUENESS { frwkFeedbackSelUsageComboCapId,   
                    frwkFeedbackSelUsageComboCapSelection,  
                    frwkFeedbackSelUsageComboCapUsage, 
                    frwkFeedbackSelUsageComboCapThreshold 
                 }  
        ::= {frwkFeedbackSelUsageComboCapsTable 1}   
     
   FrwkFeedbackSelUsageComboCapsEntry ::= SEQUENCE {  
          frwkFeedbackSelUsageComboCapId         InstanceId,  
          frwkFeedbackSelUsageComboCapSelection  OBJECT IDENTIFIER,  
          frwkFeedbackSelUsageComboCapUsage      OBJECT IDENTIFIER, 
          frwkFeedbackSelUsageComboCapThreshold  OBJECT IDENTIFIER  
   }  
 
   frwkFeedbackSelUsageComboCapId OBJECT-TYPE  
        SYNTAX        InstanceId  
        STATUS        current  
        DESCRIPTION  
           " An arbitrary integer index that uniquely identifies an   
             instance of the frwkFeedbackSelUsageComboCapsEntry  
             class."  
        ::= { frwkFeedbackSelUsageComboCapsEntry 1}  
     
   frwkFeedbackSelUsageComboCapSelection OBJECT-TYPE  
        SYNTAX        OBJECT IDENTIFIER  
        STATUS        current  
        DESCRIPTION  
           "The PRC of the selection class that is supported by  
            the device in the combination defined by this instance."  
        ::= { frwkFeedbackSelUsageComboCapsEntry 2} 
 
   frwkFeedbackSelUsageComboCapUsage OBJECT-TYPE  
        SYNTAX        OBJECT IDENTIFIER  
        STATUS        current  
        DESCRIPTION  
           "The PRC of the usage policy class that is supported by  
            the device in combination  with the selection PRC and the 
            threshold PRC defined in this instance."  
        ::= { frwkFeedbackSelUsageComboCapsEntry 3} 
  
  
   frwkFeedbackSelUsageComboCapThreshold OBJECT-TYPE  
           SYNTAX        OBJECT IDENTIFIER  
           STATUS        current  
           DESCRIPTION  
              "The PRC of the threshold class that is supported by  
               the device in the combination defined by this instance."  
           ::= { frwkFeedbackSelUsageComboCapsEntry 4} 
 
   --   
   -- The Feedback Report Linkage Table  
   --   
     
   frwkFeedbackLinkTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackLinkEntry   
        PIB-ACCESS      install   
        STATUS          current   
        DESCRIPTION   
                 "This class associates the selection criteria with the  
                  usage policy. It also permit the defining of the max  
                  interval used for reporting the usage instance."  
     
        ::= { frwkFeedbackGroupClasses  4}   
 
   frwkFeedbackLinkEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackLinkEntry   
        STATUS          current   
        DESCRIPTION   
                 "This class associates the selection criteria with the  
                  usage policy. It also permits the defining of the max  
                  interval used for reporting the usage instance."  
        PIB-INDEX {frwkFeedbackLinkId}  
        UNIQUENESS { frwkFeedbackLinkId,   
                    frwkFeedbackLinkSel,  
                    frwkFeedbackLinkUsage }  
        ::= {frwkFeedbackLinkTable 1}   
     
   FrwkFeedbackLinkEntry ::= SEQUENCE {  
          frwkFeedbackLinkId         InstanceId,  
          frwkFeedbackLinkSel        Prid,  
          frwkFeedbackLinkUsage      OBJECT IDENTIFIER,  
          frwkFeedbackLinkInterval   Integer32, 
          frwkFeedbackLinkThreshold  Prid, 
          frwkFeedbackLinkFlags       BITS 
   }  
     
   frwkFeedbackLinkId OBJECT-TYPE  
        SYNTAX        InstanceId  
        STATUS        current  
        DESCRIPTION  
           " An arbitrary integer index that uniquely identifies an   
             instance of the frwkFeedbackLinkTable class."  
        ::= { frwkFeedbackLinkEntry 1}  
     
   frwkFeedbackLinkSel OBJECT-TYPE  
        SYNTAX       Prid  
        STATUS       current  
        DESCRIPTION  
            "The PRID of the selection criteria instance that   
             defines the conditions to use by the PEP for   
             monitoring the usage."  
     
        ::= { frwkFeedbackLinkEntry 2}  
     
   frwkFeedbackLinkUsage OBJECT-TYPE  
        SYNTAX      OBJECT IDENTIFIER  
        STATUS      current  
        DESCRIPTION  
             "The PRC of the usage policy class that the PEP uses to  
             monitor, record and report."  
     
        ::= { frwkFeedbackLinkEntry 3}  
     
   frwkFeedbackLinkInterval  OBJECT-TYPE       
        SYNTAX   Integer32  
        STATUS   current  
        DESCRIPTION   
                "Maximum interval in units of the value of the 
                Accounting Timer specified by the PDP in the client 
                accept message. A frwkFeedbackLinkInterval of 1 is 
                equal to the value of the Accounting Timer. This value 
                must be 1 or greater. "  
     
        ::= { frwkFeedbackLinkEntry 4}  
 
   frwkFeedbackLinkThreshold  OBJECT-TYPE       
        SYNTAX   Prid  
        STATUS   current  
        DESCRIPTION   
                "The PRID of the threshold class instance. This 
                instance specifies the threshold values for the usage 
                policy."  
        ::= { frwkFeedbackLinkEntry 5}  
 
  frwkFeedbackLinkFlags  OBJECT-TYPE       
        SYNTAX   BITS { 
                         periodic(0), 
                         threshold(1), 
                         changeOnly(2)
                 } 
        STATUS   current  
        DESCRIPTION   
               "This value indicates the reporting basis of the usage 
                policy. The feed back may be generated on demand, on a 
                periodic basis regardless of a change in value from the 
                previous report, on a periodic basis if a change in 
                value has occurred, or the usage is reported when an 
                identified threshold value in the usage instance has 
                been reached.  
                If the 'periodic' flag is set, the PEP will provide 
                unsolicited reports at the rate specified in 
                frwkFeedbackLinkInterval. 
                If the 'periodic' flag is not set, reports will only be 
                generated when solicited by the PDP. 
                The 'threshold' and 'changeOnly' flags make the 
                periodic reports conditional - these flags only make 
                sense in combination with the 'periodic' flag." 
                                   
           ::= { frwkFeedbackLinkEntry 6} 
    
  
   -- 
   -- All actual usage classes are in the separate 
   -- FrwkFeedbackUsageClasses group 
   -- 
    
   frwkFeedbackUsageClasses 
       OBJECT IDENTIFIER ::= { feedbackPolFrameworkPib  2 } 
   
 
   --   
   -- The generic traffic (byte & packet count) usage class   
   --   
     
   frwkFeedbackTrafficUsageTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackTrafficUsageEntry   
        PIB-ACCESS      report-only   
        STATUS          current   
        DESCRIPTION   
                 "This class defines the usage attributes that the PEP 
                  is to monitor for plain traffic handling elements 
                  like filters. All packets and the bytes contained in 
                  these packets are counted. It also contains the PRID 
                  of the linkage instance associating the selection 
                  criteria instance with the usage instance."  
     
        ::= { frwkFeedbackUsageClasses  1}   
     
   frwkFeedbackTrafficUsageEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackTrafficUsageEntry   
        STATUS          current   
        DESCRIPTION   
                 "Defines the attributes the PEP is to monitor,  
                  record and report."  
        PIB-INDEX {frwkFeedbackTrafficUsageId}  
        UNIQUENESS { frwkFeedbackTrafficUsageLinkPRID }  
     
        ::= {frwkFeedbackTrafficUsageTable 1}   
     
   FrwkFeedbackTrafficUsageEntry ::= SEQUENCE {  
         frwkFeedbackTrafficUsageId              InstanceId,  
         frwkFeedbackTrafficUsageLinkPRID        Prid,  
         frwkFeedbackTrafficUsagePacketCount     Counter64,    
         frwkFeedbackTrafficUsageByteCount       Counter64    
          
   }  
      
   frwkFeedbackTrafficUsageId   OBJECT-TYPE  
        SYNTAX       InstanceId  
        STATUS       current  
        DESCRIPTION  
                  "Arbitrary integer index that uniquely identifies  
                   an instance of the class."  
        ::= { frwkFeedbackTrafficUsageEntry 1 }  
     
   frwkFeedbackTrafficUsageLinkPRID  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of the Linkage policy instance used to base 
                   this usage policy instance upon."  
     
        ::= { frwkFeedbackTrafficUsageEntry 2 }  
     
   frwkFeedbackTrafficUsagePacketCount OBJECT-TYPE    
        SYNTAX       Counter64 
        STATUS       current    
        DESCRIPTION    
                  "The count of packets handled by the associated 
                   element during the reporting interval."    
             
        ::= {frwkFeedbackTrafficUsageEntry 3}    
             
   frwkFeedbackTrafficUsageByteCount OBJECT-TYPE    
        SYNTAX       Counter64 
        STATUS       current    
        DESCRIPTION    
                   "The byte count of packets handled by the associated 
                    element." 
        ::= { frwkFeedbackTrafficUsageEntry 4}    
             
     
 
   --   
   -- The traffic usage class, qualified for an interface   
   --   
     
   frwkFeedbackIfTrafficUsageTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackIfTrafficUsageEntry   
        PIB-ACCESS      report-only   
        STATUS          current   
        DESCRIPTION   
                "A usage PRC similar to the basic TrafficUsage class 
                that also contains a reference to an interface. This 
                class should be used with a selection criteria that 
                matches an element that is assigned to multiple 
                interfaces. The interface field can be used to 
                associate the instances of this class with the specific 
                element's assignment."  
        ::= { frwkFeedbackUsageClasses  2 }   
     
   frwkFeedbackIfTrafficUsageEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackIfTrafficUsageEntry   
        STATUS          current   
        DESCRIPTION   
                 "Defines the attributes the PEP is to monitor,  
                  record and report."  
        PIB-INDEX {frwkFeedbackIfTrafficUsageId}  
        UNIQUENESS { frwkFeedbackIfTrafficUsageLinkPRID, 
                     frwkFeedbackIfTrafficUsageInterface }  
     
        ::= {frwkFeedbackIfTrafficUsageTable 1}   
     
   FrwkFeedbackIfTrafficUsageEntry ::= SEQUENCE {  
         frwkFeedbackIfTrafficUsageId              InstanceId,  
         frwkFeedbackIfTrafficUsageLinkPRID        Prid, 
         frwkFeedbackIfTrafficUsageInterface       Prid, 
         frwkFeedbackIfTrafficUsagePacketCount     Counter64,    
         frwkFeedbackIfTrafficUsageByteCount       Counter64    
          
   }  
      
   frwkFeedbackIfTrafficUsageId   OBJECT-TYPE  
        SYNTAX       InstanceId  
        STATUS       current  
        DESCRIPTION  
                  "Arbitrary integer index that uniquely identifies  
                   an instance of the class."  
        ::= { frwkFeedbackIfTrafficUsageEntry 1 }  
     
   frwkFeedbackIfTrafficUsageLinkPRID  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of the Linkage policy instance used to base 
                   this usage policy instance upon."  
        ::= { frwkFeedbackIfTrafficUsageEntry 2 }  
     
   frwkFeedbackIfTrafficUsageInterface  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of a frwkIfRoleCombo instance, uniquely 
                   identifying a specific interface." 
        ::= { frwkFeedbackIfTrafficUsageEntry 3 }  
 
   frwkFeedbackIfTrafficUsagePacketCount OBJECT-TYPE    
        SYNTAX       Counter64 
        STATUS       current    
        DESCRIPTION    
                "The count of packets handled by the associated element 
                during the reporting interval."    
        ::= { frwkFeedbackIfTrafficUsageEntry 4 }    
             
   frwkFeedbackIfTrafficUsageByteCount OBJECT-TYPE    
        SYNTAX       Counter64 
        STATUS       current    
        DESCRIPTION    
                   "The byte count of packets  
                    handled by the associated element." 
        ::= { frwkFeedbackIfTrafficUsageEntry 5 }    
 
 
 
   -- 
   -- The Threshold class that accompanies the above Usage PRCs 
   -- 
    
   frwkFeedbackTrafficThresholdTable OBJECT-TYPE   
           SYNTAX         SEQUENCE OF FrwkFeedbackTrafficThresholdEntry   
           PIB-ACCESS     install   
           STATUS         current   
           DESCRIPTION   
                 "This class defines the threshold attributes 
                  corresponding to usage attributes specified in 
                  frwkFeedbackTrafficUsageTable, 
                  frwkFeedbackIfTrafficUsageTable and other similar 
                  usage classes. 
                  The usage object is considered to match the threshold 
                  condition if the following expression evaluates to 
                  'TRUE': 
                  { 
                    byteCond = (ByteThreshold != NULL) ? 
                            (ByteThreshold > ByteCounter) : FALSE; 
                    packetCond (PacketThreshold != NULL) ? 
                            (PacketThreshold > PacketCounter) : FALSE; 
                    return ( byteCond || packetCond ); 
                  }"  
        
           ::= { frwkFeedbackUsageClasses  3}   
        
      frwkFeedbackTrafficThresholdEntry OBJECT-TYPE   
           SYNTAX          FrwkFeedbackTrafficThresholdEntry   
           STATUS          current   
           DESCRIPTION   
                    "Defines the attributes to hold threshold values."  
           PIB-INDEX {frwkFeedbackTrafficThresholdId}  
    
           ::= {frwkFeedbackTrafficThresholdTable 1}   
        
      FrwkFeedbackTrafficThresholdEntry ::= SEQUENCE {  
            frwkFeedbackTrafficThresholdId          InstanceId,  
            frwkFeedbackTrafficThresholdPacketThreshold     Integer64,    
            frwkFeedbackTrafficThresholdByteThreshold       Integer64       
      }  
    
   frwkFeedbackTrafficThresholdId   OBJECT-TYPE  
           SYNTAX       InstanceId  
           STATUS       current  
           DESCRIPTION  
                     "Arbitrary integer index that uniquely identifies  
                      an instance of the class."  
           ::= { frwkFeedbackTrafficThresholdEntry 1 } 
    
   frwkFeedbackTrafficThresholdPacketThreshold   OBJECT-TYPE  
           SYNTAX       Integer64  
           STATUS       current  
           DESCRIPTION  
                     "The threshold, in terms of packets, that must be 
                      exceeded to trigger a report in the next 
                      reporting interval."  
           ::= { frwkFeedbackTrafficThresholdEntry 2 } 
    
   frwkFeedbackTrafficThresholdByteThreshold   OBJECT-TYPE  
           SYNTAX       Integer64  
           STATUS       current  
           DESCRIPTION  
                     "The threshold, in terms of bytes, that must be 
                      exceeded to trigger a report in the next 
                      reporting interval."  
           ::= { frwkFeedbackTrafficThresholdEntry 3 } 
    
    
   -- 
   -- All Selection classes are in the separate 
   -- FrwkFeedbackSelectionClasses group 
   -- 
    
   frwkFeedbackSelectionClasses 
       OBJECT IDENTIFIER ::= { feedbackPolFrameworkPib  3 } 
 
   -- 
   -- The Set WatchPoint Table  
   --   
     
   frwkFeedbackSetWatchPointTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackSetWatchPointEntry   
        PIB-ACCESS      install   
        STATUS          current   
        DESCRIPTION   
                 "This class defines a selection criteria that 
                  identifies a specific processing point to watch 
                  for the desired usage. This selection criteria 
                  may be useful in PIBs that are designed using a 
                  datapath approach where the policies are linked 
                  and can be reused within the PIB."  
     
        ::= { frwkFeedbackSelectionClasses  1}   
     
   frwkFeedbackSetWatchPointEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackSetWatchPointEntry   
        STATUS          current   
        DESCRIPTION   
                 "Defines the attributes the of the selection  
                  criteria identifying a specific policy 
                  where to monitor the associated usage."  
        PIB-INDEX { frwkFeedbackSetWatchPointId }  
 
     
        ::= {frwkFeedbackSetWatchPointTable 1}   
     
   FrwkFeedbackSetWatchPointEntry ::= SEQUENCE {  
         frwkFeedbackSetWatchPointId                  InstanceId,  
         frwkFeedbackSetWatchPointPolicyPRID          Prid
    
   }  
      
   frwkFeedbackSetWatchPointId   OBJECT-TYPE  
        SYNTAX       InstanceId  
        STATUS       current  
        DESCRIPTION  
                  "Arbitrary integer index that uniquely identifies  
                   an instance of the class."  
        ::= { frwkFeedbackSetWatchPointEntry 1 }  
     
   frwkFeedbackSetWatchPointPolicyPRID  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of the enforcement policy instance where 
                   the associated usage is to be monitored."  
     
        ::= { frwkFeedbackSetWatchPointEntry 2 }  
     
 
    -- 
    -- DPE Selection Class 
    --  
 
    frwkFeedbackDPESelectionTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackDPESelectionEntry   
        PIB-ACCESS      install 
        STATUS          current   
        DESCRIPTION   
                "This class defines a selection criteria that 
                identifies a specific data path element to collect 
                usage information" 
   
        ::= { frwkFeedbackSelectionClasses  2}   
     
    frwkFeedbackDPESelectionEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackDPESelectionEntry   
        STATUS          current 
        DESCRIPTION   
                 "Defines the attributes the of the selection  
                  criteria identifying a specific policy 
                  where to monitor the associated usage."  
        PIB-INDEX { frwkFeedbackDPESelectionId }  
        UNIQUENESS { frwkFeedbackDPESelectionDataPathElement, 
                     frwkFeedbackDPESelectionInterface, 
                     frwkFeedbackDPESelectionIfDirection }  
     
        ::= {frwkFeedbackDPESelectionTable 1}   
     
   FrwkFeedbackDPESelectionEntry ::= SEQUENCE {  
                     frwkFeedbackDPESelectionId             InstanceId, 
                     frwkFeedbackDPESelectionDataPathElement      Prid, 
                     frwkFeedbackDPESelectionInterface            Prid, 
                     frwkFeedbackDPESelectionIfDirection   IfDirection 
   }  
      
   frwkFeedbackDPESelectionId   OBJECT-TYPE  
        SYNTAX       InstanceId  
        STATUS       current  
        DESCRIPTION  
                  "Arbitrary integer index that uniquely identifies  
                   an instance of the class."  
        ::= { frwkFeedbackDPESelectionEntry 1 }  
     
 
   frwkFeedbackDPESelectionDataPathElement  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of the element in the data path that we 
                   want to collect usage information from. This element 
                   must be part of the data path assigned to the 
                   interface/direction combination referenced in this 
                   object."  
        ::= { frwkFeedbackDPESelectionEntry 2 }  
 
   frwkFeedbackDPESelectionInterface  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of a frwkIfRoleCombo instance, uniquely 
                   identifying a specific interface" 
        ::= { frwkFeedbackDPESelectionEntry 3 }  
 
   frwkFeedbackDPESelectionIfDirection  OBJECT-TYPE  
        SYNTAX      IfDirection 
        STATUS      current  
        DESCRIPTION  
                  "The direction (ingress/egress) that to which the DPE 
                   is attached that we want to match."  
        ::= { frwkFeedbackDPESelectionEntry 4 }  
 
 
    -- 
    -- DPE Selection Query Class 
    --  
 
    frwkFeedbackDPESelectionQueryTable OBJECT-TYPE   
        SYNTAX          SEQUENCE OF FrwkFeedbackDPESelectionQueryEntry   
        PIB-ACCESS      install 
        STATUS          current   
        DESCRIPTION   
                "This class defines a selection criteria that 
                identifies a set of assignments of a data path element 
                based on an entry in the Data Path Table 
                Each matched assignment will collect and report usage 
                independently, so this selection criteria should be 
                combined with a Usage PRC that includes an interface 
                reference." 
   
        ::= { frwkFeedbackSelectionClasses  3}   
     
    frwkFeedbackDPESelectionQueryEntry OBJECT-TYPE   
        SYNTAX          FrwkFeedbackDPESelectionQueryEntry   
        STATUS          current 
        DESCRIPTION   
                 "Defines the attributes the of the selection  
                  criteria identifying a specific policy 
                  where to monitor the associated usage."  
        PIB-INDEX { frwkFeedbackDPESelectionQueryId }  
        UNIQUENESS { frwkFeedbackDPESelectionQueryDataPath, 
                     frwkFeedbackDPESelectionQueryDataPathElement }  
     
        ::= {frwkFeedbackDPESelectionQueryTable 1}   
     
   FrwkFeedbackDPESelectionQueryEntry ::= SEQUENCE {  
                     frwkFeedbackDPESelectionQueryId        InstanceId, 
                     frwkFeedbackDPESelectionQueryDataPath        Prid, 
                     frwkFeedbackDPESelectionQueryDataPathElement Prid 
   }  
      
   frwkFeedbackDPESelectionQueryId   OBJECT-TYPE  
        SYNTAX       InstanceId  
        STATUS       current  
        DESCRIPTION  
                  "Arbitrary integer index that uniquely identifies  
                   an instance of the class."  
        ::= { frwkFeedbackDPESelectionQueryEntry 1 }  
     
   frwkFeedbackDPESelectionQueryDataPath  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of a Data Path instance, identifying a 
                   group of data path assignments." 
        ::= { frwkFeedbackDPESelectionQueryEntry 2 }  
 
   frwkFeedbackDPESelectionQueryDataPathElement  OBJECT-TYPE  
        SYNTAX      Prid  
        STATUS      current  
        DESCRIPTION  
                  "The PRID of the element in the data path that we 
                   want to collect usage information from. This element 
                   must be part of the data path referenced from the 
                   frwkFeedbackDPESelectionQueryDataPath field."  
        ::= { frwkFeedbackDPESelectionQueryEntry 3 }  
 
   END 
