# -*- text -*-
# Copyright (C) 2015 The FreeRADIUS Server project and contributors
##############################################################################
#
#	Alcatel Broadband Access Server dictionary.
#
#	$Id: d1952902b4e514456185dfcac4017e57a2d49dac $
#
##############################################################################

VENDOR		Alcatel				3041

BEGIN-VENDOR	Alcatel

ATTRIBUTE	AAT-Client-Primary-DNS			5	ipaddr
ATTRIBUTE	AAT-Client-Primary-WINS-NBNS		6	ipaddr
ATTRIBUTE	AAT-Client-Secondary-WINS-NBNS		7	ipaddr
ATTRIBUTE	AAT-Client-Secondary-DNS		8	ipaddr
ATTRIBUTE	AAT-PPP-Address				9	ipaddr
ATTRIBUTE	AAT-PPP-Netmask				10	ipaddr
ATTRIBUTE	AAT-Primary-Home-Agent			12	string
ATTRIBUTE	AAT-Secondary-Home-Agent		13	string
ATTRIBUTE	AAT-Home-Agent-Password			14	string
ATTRIBUTE	AAT-Home-Network-Name			15	string
ATTRIBUTE	AAT-Home-Agent-UDP-Port			16	integer
ATTRIBUTE	AAT-IP-Direct				17	ipaddr
ATTRIBUTE	AAT-FR-Direct				18	integer
ATTRIBUTE	AAT-FR-Direct-Profile			19	string
ATTRIBUTE	AAT-FR-Direct-DLCI			20	integer
ATTRIBUTE	AAT-ATM-Direct				21	string
ATTRIBUTE	AAT-IP-TOS				22	integer
ATTRIBUTE	AAT-IP-TOS-Precedence			23	integer
ATTRIBUTE	AAT-IP-TOS-Apply-To			24	integer
ATTRIBUTE	AAT-MCast-Client			27	integer
ATTRIBUTE	AAT-Modem-Port-No			28	integer
ATTRIBUTE	AAT-Modem-Slot-No			29	integer
ATTRIBUTE	AAT-Modem-Shelf-No			30	integer
ATTRIBUTE	AAT-Filter				60	string
ATTRIBUTE	AAT-Vrouter-Name			61	string
ATTRIBUTE	AAT-Require-Auth			62	integer
ATTRIBUTE	AAT-IP-Pool-Definition			63	string
ATTRIBUTE	AAT-Assign-IP-Pool			64	integer
ATTRIBUTE	AAT-Data-Filter				65	string
ATTRIBUTE	AAT-Source-IP-Check			66	integer
ATTRIBUTE	AAT-Modem-Answer-String			67	string
ATTRIBUTE	AAT-Auth-Type				68	integer
ATTRIBUTE	AAT-Qos					70	integer
ATTRIBUTE	AAT-Qoa					71	integer
ATTRIBUTE	AAT-Client-Assign-DNS			72	integer
ATTRIBUTE	AAT-ATM-VPI				128	integer
ATTRIBUTE	AAT-ATM-VCI				129	integer
ATTRIBUTE	AAT-Input-Octets-Diff			130	integer
ATTRIBUTE	AAT-Output-Octets-Diff			131	integer
ATTRIBUTE	AAT-User-MAC-Address			132	string
ATTRIBUTE	AAT-ATM-Traffic-Profile			133	string

VALUE	AAT-MCast-Client		Multicast-No		0
VALUE	AAT-MCast-Client		Multicast-Yes		1

VALUE	AAT-Require-Auth		Not-Require-Auth	0
VALUE	AAT-Require-Auth		Require-Auth		1

VALUE	AAT-FR-Direct			No			0
VALUE	AAT-FR-Direct			Yes			1

VALUE	AAT-Source-IP-Check		Source-IP-Check-No	0
VALUE	AAT-Source-IP-Check		Source-IP-Check-Yes	1

VALUE	AAT-IP-TOS			IP-TOS-Normal		0
VALUE	AAT-IP-TOS			IP-TOS-Disabled		1
VALUE	AAT-IP-TOS			IP-TOS-Cost		2
VALUE	AAT-IP-TOS			IP-TOS-Reliability	4
VALUE	AAT-IP-TOS			IP-TOS-Throughput	8
VALUE	AAT-IP-TOS			IP-TOS-Latency		16

VALUE	AAT-IP-TOS-Apply-To		IP-TOS-Apply-To-Incoming 1024
VALUE	AAT-IP-TOS-Apply-To		IP-TOS-Apply-To-Both	3072
VALUE	AAT-IP-TOS-Apply-To		IP-TOS-Apply-To-Outgoing 2048

VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Normal 0
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-One 32
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Two 64
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Three 96
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Four 128
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Five 160
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Six 192
VALUE	AAT-IP-TOS-Precedence		IP-TOS-Precedence-Pri-Seven 224

VALUE	AAT-Auth-Type			AAT-Auth-None		0
VALUE	AAT-Auth-Type			AAT-Auth-Default	1
VALUE	AAT-Auth-Type			AAT-Auth-Any		2
VALUE	AAT-Auth-Type			AAT-Auth-PAP		3
VALUE	AAT-Auth-Type			AAT-Auth-CHAP		4
VALUE	AAT-Auth-Type			AAT-Auth-MS-CHAP	5

VALUE	AAT-Client-Assign-DNS		DNS-Assign-No		0
VALUE	AAT-Client-Assign-DNS		DNS-Assign-Yes		1

END-VENDOR	Alcatel
