IP-TE-PIB PIB-DEFINITIONS ::= BEGIN 
 
IMPORTS 
     ibrpib
            FROM TUBS-SMI
     Unsigned32, Integer32, MODULE-IDENTITY, 
     MODULE-COMPLIANCE, OBJECT-TYPE, OBJECT-GROUP,
     TEXTUAL-CONVENTION 
            FROM COPS-PR-SPPI 
     InstanceId, ReferenceId, Prid, TagId 
            FROM COPS-PR-SPPI-TC 

     InetAddress, InetAddressType 
            FROM INET-ADDRESS-MIB 
     Count
            FROM ACCOUNTING-FRAMEWORK-PIB
     TruthValue, TEXTUAL-CONVENTION  
            FROM SNMPv2-TC 
     RoleCombination
            FROM FRAMEWORK-TC-PIB 
     SnmpAdminString 
            FROM SNMP-FRAMEWORK-MIB; 
 
 
ipTePib     MODULE-IDENTITY 
 
     SUBJECT-CATEGORIES { all }     -- IP TE client-type to be  
                                   -- assigned by IANA 
     LAST-UPDATED   "200106180900Z" 
     ORGANIZATION   "France Telecom" 
     CONTACT-INFO   " 
                    Christian Jacquenet 
                    France Telecom R & D 
                    42, rue des Coutures 
                    BP 6243 
                    14066 CAEN CEDEX 04 
                    France 
                    Phone: +33 2 31 75 94 28 
                    E-Mail: christian.jacquenet@francetelecom.com" 
     DESCRIPTION 
            "The PIB module containing a set of policy rule classes 
             that describe IP Traffic Engineering policies to be 
             enforced within and between domains." 
    REVISION        "200111061600Z" 
    DESCRIPTION 
            "Initial version." 
 
     ::= { ibrpib 23 } -- tbd to be assigned by IANA 
 
ipTeFwdClasses      OBJECT IDENTIFIER ::= { ipTePib 1 } 
ipTeMetricsClasses  OBJECT IDENTIFIER ::= { ipTePib 2 } 
ipTeStatsClasses    OBJECT IDENTIFIER ::= { ipTePib 3 } 
 
-- 
-- Forwarding classes. The information contained in these classes 
-- is meant to provide a detailed description of the traffic  
-- engineered routes. One table has been specified so far, but there 
-- is room for depicting specific kinds of routes, like MPLS LSP  
-- paths, for example. 
-- 
-- 
 
 
--  

-- The ipTeRouteTable 
-- 
 
ipTeRouteTable      OBJECT-TYPE 
  
       SYNTAX        SEQUENCE OF IpTeRouteEntry  
       PIB-ACCESS   notify  
       STATUS        current  
       DESCRIPTION  
             "This table describes the traffic engineered routes 
             that are installed in the forwarding tables of the 
             routers."  
     
       ::= { ipTeFwdClasses 1 }  
     
ipTeRouteEntry      OBJECT-TYPE 
  
       SYNTAX        IpTeRouteEntry  
       STATUS        current  
       DESCRIPTION  
             "A particular traffic engineered route to a particular 
             destination."  
     
       PIB-INDEX    { ipTeRoutePrid }  
       UNIQUENESS   { ipTeRouteDest,  
                       ipTeRouteMask,  
                       ipTeRoutePhbId, 
                       ipTeRouteNextHopAddress,
                      ipTeRouteNextHopMask }    
     
       ::= { ipTeRouteTable 1 }  
     
IpTeRouteEntry ::= SEQUENCE {  
            ipTeRoutePrid                  InstanceId, 
            ipTeRouteDestAddrType          InetAddressType,  
            ipTeRouteDest                  InetAddress,  
            ipTeRouteMask                  Unsigned32,  
            ipTeRouteNextHopAddrType       InetAddressType,        
            ipTeRouteNextHopAddress        InetAddress, 
            ipTeRouteNextHopMask           Unsigned32, 
            ipTeRoutePhbId                 Integer32, 
            ipTeRouteOrigin                 Integer32,   
            ipTeRouteIfIndex               Unsigned32  
}  
     
ipTeRoutePrid              OBJECT-TYPE 
      
     SYNTAX                InstanceId 
     STATUS                current 
     DESCRIPTION     
             "An integer index that uniquely identifies this route 
             entry among all the route entries." 

 
     ::= { ipTeRouteEntry 1 } 
 
ipTeRouteDestAddrType       OBJECT-TYPE 
      
     SYNTAX                InetAddressType 
     STATUS                current 
     DESCRIPTION 
             "The address type enumeration value ([16]) used to 
             specify the type of a route's destination IP address." 
              
    ::= { ipTeRouteEntry 2 } 
 
ipTeRouteDest       OBJECT-TYPE 
  
     SYNTAX         InetAddress  
     STATUS         current  
     DESCRIPTION  
             "The IP address to match against the packet's 
             destination address."  
   
     ::= { ipTeRouteEntry 3 }  
     
ipTeRouteMask       OBJECT-TYPE 
  
     SYNTAX         Unsigned32 (0..128)  
     STATUS         current  
     DESCRIPTION  
             "Indicates the length of a mask for the matching of the 
             destination IP address. Masks are constructed by 
             setting bits in sequence from the most-significant bit 
             downwards for ipTeRouteMask bits length. All other bits 
             in the mask, up to the number needed to fill the length 
             of the address ipTeRouteDest are cleared to zero.  A 
             zero bit in the mask then means that the corresponding 
             bit in the address always matches."
     
     ::= { ipTeRouteEntry 4 }  
 
ipTeRouteNextHopAddrType    OBJECT-TYPE 
      
     SYNTAX                InetAddressType 
     STATUS                current 
     DESCRIPTION 
             "The address type enumeration value used to specify the 
             type of the next hop's IP address." 
              
    ::= { ipTeRouteEntry 5 } 
 
ipTeRouteNextHopAddress     OBJECT-TYPE 
  
     SYNTAX                 InetAddress  

     STATUS                 current  
     DESCRIPTION  
             "On remote routes, the address of the next router en 
             route; Otherwise, 0.0.0.0."  
     
     ::= { ipTeRouteEntry 6 }  
     
ipTeRouteNextHopMask        OBJECT-TYPE 
  
     SYNTAX                Unsigned32 (0..128)  
     STATUS                current  
     DESCRIPTION  
             "Indicates the length of a mask for the matching of the 
             next hop's IP address. Masks are constructed by setting 
             bits in sequence from the most-significant bit 
             downwards for ipTeRouteNextHopMask bits length. All 
             other bits in the mask, up to the number needed to fill 
             the length of the address ipTeRouteNextHop are cleared 
             to zero.  A zero bit in the mask then means that the 
             corresponding bit in the address always matches." 
     
     ::= { ipTeRouteEntry 7 }  
     
ipTeRoutePhbId      OBJECT-TYPE 
  
     SYNTAX          Integer32 (-1 | 0..63) 
     STATUS          current  
     DESCRIPTION  
             "The binary encoding that uniquely identifies a Per Hop 
             Behaviour (PHB, [17]) or a set of PHBs associated to 
             the DiffServ Code Point (DSCP, [15]) marking of the IP 
             datagrams that will be conveyed along this traffic 
             engineered route. A value of -1 indicates that a 
             specific PHB ID value has not been defined, and thus, 
             all PHB ID values are considered a match." 
   
     ::= { ipTeRouteEntry 8 }  
     
ipTeRouteOrigin     OBJECT-TYPE 
 
     SYNTAX INTEGER { 
                    ospf (0),
                    is-is (1),
                    bgp (2),
                    static (3),
                    other (4)
            } 
     STATUS         current 
     DESCRIPTION     
             "The value indicates the origin of the route. Either 
             the route has been computed by OSPF, by IS-IS, 
             announced by BGP4, is static, or else." 

              
     ::= { ipTeRouteEntry 9 } 
 
ipTeRouteIfIndex    OBJECT-TYPE 
  
     SYNTAX          Unsigned32 (0..65535)  
     STATUS          current  
     DESCRIPTION  
             "The ifIndex value that identifies the local interface 
             through which the next hop of this route is 
             accessible."  
     
     ::= { ipTeRouteEntry 10 } 
 
-- 
-- 
-- Traffic engineering metrics classes.  
-- 
-- The information stored in the following tables is meant to provide 
-- the description of the metric values that will be taken into  
-- account by intra- and inter-domain routing protocols for the  
-- computation and the selection of traffic-engineered routes. So  
-- far, two tables have been identified: one which is based upon the 
-- traffic engineering extensions of OSPF, the other which is based  
-- upon the contents of a specific BGP4 attribute. Next versions of  
-- the draft will include IS-IS specific information, as well as  
-- extensions of the BGP4-specific provisioning information for the  
-- "basic" enforcement of a BGP4 routing policy. 
-- 
-- 
 
-- 
-- The ospfTeMetricsTable 
-- 
 
ospfTeMetricsTable  OBJECT-TYPE 
  
     SYNTAX         SEQUENCE OF OspfTeMetricsEntry  
     PIB-ACCESS     install-notify  
     STATUS          current  
     DESCRIPTION  
             "This class describes the link and traffic engineering 
             metrics that will be used by OSPF for TE route 
             calculation purposes."  
     
       ::= { ipTeMetricsClasses 1 }  
     
ospfTeMetricsEntry  OBJECT-TYPE  
        
     SYNTAX          OspfTeMetricsEntry  
     STATUS          current  
     DESCRIPTION  

             "The collection of OSPF metrics assigned to the router 
             on a per interface and per DSCP basis."  
     
     PIB-INDEX      { ospfTeMetricsPrid }  
     UNIQUENESS     { ospfTeMetricsIfMetricValue,  
                       ospfTeMetricsDscpValue,  
                       ospfTeMetricsSubTlvLinkType, 
                       ospfTeMetricsSubTlvLinkId, 
                       ospfTeMetricsSubTlvLocalIfAddress, 
                       ospfTeMetricsSubTlvRemoteIfAddress, 
                       ospfTeMetricsSubTlvTeMetric, 
                       ospfTeMetricsSubTlvMaxBandwidth, 
                       ospfTeMetricsSubTlvMaxRsvBandwidth, 
                       ospfTeMetricsSubTlvUnrsvBandwidth, 
                       ospfTeMetricsIfIndex }  
     
     ::= { ospfTeMetricsTable 1 }  
     
OspfTeMetricsEntry ::= SEQUENCE {  
       
            ospfTeMetricsPrid                      InstanceId,  
            ospfTeMetricsIfMetricValue            Unsigned32,  
            ospfTeMetricsDscpValue                Integer32, 
            ospfTeMetricsTopTlvAddressType        InetAddressType, 
            ospfTeMetricsTopTlvRouterAddress       InetAddress, 
            ospfTeMetricsTopTlvRouterAddrMask      Unsigned32,  
            ospfTeMetricsSubTlvLinkType           INTEGER, 
            ospfTeMetricsSubTlvLinkIdAddressType   InetAddressType, 
            ospfTeMetricsSubTlvLinkId             InetAddress, 
            ospfTeMetricsSubTlvLinkIdMask         Unsigned32, 
            ospfTeMetricsSubTlvLocalIfAddressType  InetAddressType, 
            ospfTeMetricsSubTlvLocalIfAddress      InetAddress, 
            ospfTeMetricsSubTlvLocalIfAddrMask     Unsigned32, 
            ospfTeMetricsSubTlvRemoteIfAddressType InetAddressType, 
            ospfTeMetricsSubTlvRemoteIfAddress     InetAddress, 
            ospfTeMetricsSubTlvRemoteIfAddrMask    Unsigned32, 
            ospfTeMetricsSubTlvTeMetric           Unsigned32,     
            ospfTeMetricsSubTlvMaxBandwidth        Unsigned32,     
            ospfTeMetricsSubTlvMaxRsvBandwidth     Unsigned32,     
            ospfTeMetricsSubTlvUnrsvBandwidth      Unsigned32,        
            ospfTeMetricsIfIndex                  Unsigned32  
     }  
     
ospfTeMetricsPrid          OBJECT-TYPE 
      
     SYNTAX                InstanceId 
     STATUS                current 
     DESCRIPTION     
        "An integer index that uniquely identifies this instance of 
        the ospfTeMetrics class." 
 
     ::= { ospfTeMetricsEntry 1 } 

 
ospfTeMetricsIfMetricValue          OBJECT-TYPE  
        
     SYNTAX         Unsigned32 (1..65535)  
     STATUS         current  
     DESCRIPTION  
         "The link metric assigned on a per-DSCP and per-interface 
         basis, as defined in this instance of the 
         ospfTeMetricsTable."  
   
     ::= { ospfTeMetricsEntry 2 }  
     
ospfTeMetricsDscpValue              OBJECT-TYPE 
  
     SYNTAX         Integer32 (-1 | 0..63) 
     STATUS         current  
     DESCRIPTION     
        "The DSCP value associated to the link metric value, as 
        defined in the ospfTeMetricsIfMetricValue object. A value of 
        -1 indicates that a specific DSCP value has not been defined 
        and thus all DSCP values are considered a match." 
     
     ::= { ospfTeMetricsEntry 3 } 
 
ospfTeMetricsTopTlvAddressType      OBJECT-TYPE 
      
     SYNTAX         InetAddressType 
     STATUS         current 
     DESCRIPTION 
        "The address type enumeration value used to specify the IP 
        address of the advertising router. This IP address is always 
        reachable, and is typically implemented as a 'loopback'
        address." 
              
     ::= { ospfTeMetricsEntry 4 }  
     
ospfTeMetricsTopTlvRouterAddress    OBJECT-TYPE  
        
     SYNTAX        InetAddress  
     STATUS        current  
     DESCRIPTION     
        "The IP address (typically a 'loopback' address) of the 
        advertising router." 
   
     ::= { ospfTeMetricsEntry 5 } 
 
ospfTeMetricsTopTlvRouterAddrMask   OBJECT-TYPE     
      
     SYNTAX        Unsigned32 (0..128)  
     STATUS        current  
     DESCRIPTION  


        "Indicates the length of a mask for the matching of the 
        advertising router's IP address. Masks are constructed by 
        setting bits in sequence from the most-significant bit 
        downwards for ospfTeMetricsTopTlvRouterAddrMask bits length. 
        All other bits in the mask, up to the number needed to fill 
        the length of the address ospfTeMetricsTopTlvRouterAddress 
        are cleared to zero.  A zero bit in the mask then means that 
        the corresponding bit in the address always matches."  
 
     ::= { ospfTeMetricsEntry 6 } 
     
ospfTeMetricsSubTlvLinkType         OBJECT-TYPE  
        
     SYNTAX        INTEGER { 
                           point-to-Point (1),
                           multiaccess (2)  
                    } 
     STATUS        current  
     DESCRIPTION     
        "The type of the link, either point-to-point or multi-
        access, as defined in [8]."  
     
     ::= { ospfTeMetricsEntry 7 } 
 
ospfTeMetricsSubTlvLinkIdAddressType OBJECT-TYPE 
      
     SYNTAX         InetAddressType 
     STATUS         current 
     DESCRIPTION 
        "The address type enumeration value used to identify the 
        other end of the link, described as an IP address." 
              
     ::= { ospfTeMetricsEntry 8 }  
 
ospfTeMetricsSubTlvLinkId           OBJECT-TYPE  
        
     SYNTAX         InetAddress  
     STATUS         current  
     DESCRIPTION     
        "The identification of the other end of the link, described 
        as an IP address."  
     
     ::= { ospfTeMetricsEntry 9 } 
 
ospfTeMetricsSubTlvLinkIdMask         OBJECT-TYPE 
 
     SYNTAX        Unsigned32 (0..128)  
     STATUS        current  
     DESCRIPTION  
         "Indicates the length of a mask for the matching of the 
         other end of the link, described as an IP address. Masks 
         are constructed by setting bits in sequence from the most-

         significant bit downwards for ospfTeMetricsSubTlvLinkMask 
         bits length. All other bits in the mask, up to the number 
         needed to fill the length of the address 
         ospfTeMetricsSubTlvLinkId are cleared to zero.  A zero bit 
         in the mask then means that the corresponding bit in the 
         address always matches."  
 
     ::= { ospfTeMetricsEntry 10 } 
 
ospfTeMetricsSubTlvLocalIfAddressType       OBJECT-TYPE 
      
     SYNTAX         InetAddressType 
     STATUS         current 
     DESCRIPTION 
        "The address type enumeration value used to specify the IP 
        address of the interface corresponding to this instance of 
        the ospfTeMetricsSubTlvLinkType object." 
              
     ::= { ospfTeMetricsEntry 11 } 
 
ospfTeMetricsSubTlvLocalIfAddress           OBJECT-TYPE  
        
     SYNTAX         InetAddress  
     STATUS         current  
     DESCRIPTION     
        "Specifies the IP address of the interface of the 
        advertising router which is connected to the link described 
        as an instance of the ospfTeMetricsSubTlvLinkType object."  
      
     ::= { ospfTeMetricsEntry 12 } 
 
ospfTeMetricsSubTlvLocalIfAddrMask          OBJECT-TYPE 
 
     SYNTAX        Unsigned32 (0..128)  
     STATUS        current  
     DESCRIPTION  
        "Indicates the length of a mask for the matching of the IP 
        address of the interface corresponding to this instance of 
        the ospfTeMetricsSubTlvLinkType object. Masks are 
        constructed by setting bits in sequence from the most-
        significant bit downwards for 
        ospfTeMetricsSubTlvLocalIfAddrMask bits length. All other 
        bits in the mask, up to the number needed to fill the length 
        of the address ospfTeMetricsSubTlvLocalIfAddress are cleared 
        to zero.  A zero bit in the mask then means that the 
        corresponding bit in the address always matches."  
 
     ::= { ospfTeMetricsEntry 13 } 
 
      
ospfTeMetricsSubTlvRemoteIfAddressType      OBJECT-TYPE 
      

     SYNTAX         InetAddressType 
     STATUS         current 
     DESCRIPTION 
        "The address type enumeration value used to specify the IP 
        address(es) of the neighbour's interface corresponding to 
        this instance of the ospfTeMetricsSubTlvLinkType object." 
              
     ::= { ospfTeMetricsEntry 14 } 
 
ospfTeMetricsSubTlvRemoteIfAddress   OBJECT-TYPE  
        
     SYNTAX         InetAddress  
     STATUS         current  
     DESCRIPTION     
        "Specifies the IP address of the neighbour's interface that 
        is attached to this instance of the 
        ospfTeMetricsSubTlvLinkType object."  
        
     ::= { ospfTeMetricsEntry 15 } 
 
ospfTeMetricsSubTlvRemoteIfAddrMask  OBJECT-TYPE  
 
     SYNTAX        Unsigned32 (0..128)  
     STATUS        current  
     DESCRIPTION  
        "Indicates the length of a mask for the matching of the IP 
        address of the neighbor's interface corresponding to this 
        instance of the ospfTeMetricsSubTlvLinkType object. Masks 
        are constructed by setting bits in sequence from the most-
        significant bit downwards for 
        ospfTeMetricSubTlvRemoteIfAddrMaskbits length. All other 
        bits in the mask, up to the number needed to fill the length 
        of the address ospfTeMetricSubTlvRemoteIfAddress are cleared 
        to zero.  A zero bit in the mask then means that the 
        corresponding bit in the address always matches."  
 
     ::= { ospfTeMetricsEntry 16 } 
 
 
ospfTeMetricsSubTlvTeMetric          OBJECT-TYPE  
        
     SYNTAX         Unsigned32 (1..65535) 
     STATUS         current  
     DESCRIPTION     
        "The link metric that has been assigned for traffic 
        engineering purposes. This metric may be different from the 
        ospfTeMetricsLinkMetricValue object of the ospfTeMetrics 
        class."  
        
     ::= { ospfTeMetricsEntry 17 } 

ospfTeMetricsSubTlvMaxBandwidth     OBJECT-TYPE

        
     SYNTAX          Unsigned32 (0..4294967295) 
     UNITS          "bytes per second" 
     STATUS          current  
     DESCRIPTION     
        "Specifies the maximum bandwidth that can be used on this 
        instance of the ospfTeMetricsSubTlvLinkType object in this 
        direction (from the advertising router), expressed in bytes 
        per second."  
     
     ::= { ospfTeMetricsEntry 18 } 
 
ospfTeMetricsSubTlvMaxRsvBandwidth   OBJECT-TYPE  
        
     SYNTAX         Unsigned32 (0..4294967295) 
     UNITS          "bytes per second" 
     STATUS          current  
     DESCRIPTION     
        "Specifies the maximum bandwidth that may be reserved on 
        this instance of the ospfTeMetricsSubTlvLinkType object in 
        this direction (from the advertising router), expressed in 
        bytes per second."  
     
     ::= { ospfTeMetricsEntry 19 } 
 
ospfTeMetricsSubTlvUnrsvBandwidth    OBJECT-TYPE  
        
     SYNTAX         Unsigned32 (0..4294967295) 
     UNITS          "bytes per second" 
     STATUS         current  
     DESCRIPTION     
        "Specifies the amount of bandwidth that has not been 
        reserved on this instance of the ospfTeMetricsSubTlvLinkType 
        object in this direction yet (from the advertising router), 
        expressed in bytes per second."  
     
     ::= { ospfTeMetricsEntry 20 } 
     
ospfTeMetricsIfIndex                 OBJECT-TYPE  
        
     SYNTAX         Unsigned32 (0..65535)  
     STATUS         current  
     DESCRIPTION  
        "The ifIndex value that identifies the local interface that 
        has been assigned a (set of) metrics."  
        
     ::= { ospfTeMetricsEntry 21 } 
 
-- 
-- The bgpTeTable 
-- 
 

bgpTeTable          OBJECT-TYPE 
  
     SYNTAX         SEQUENCE OF BgpTeEntry  
     PIB-ACCESS     install-notify  
     STATUS          current  
     DESCRIPTION  
             "This class describes the QoS information that MAY be 
             conveyed in BGP4 UPDATE messages for the purpose of 
             enforcing an inter-domain traffic engineering policy."  
     
       ::= { ipTeMetricsClasses 2 }  
     
bgpTeEntry          OBJECT-TYPE  
        
     SYNTAX          BgpTeEntry  
     STATUS          current  
     DESCRIPTION  
             "The collection of QoS information to be exchanged by 
             BGP peers, as far as the announcement of traffic 
             engineered routes between domains is concerned."  
     
     PIB-INDEX      { bgpTePrid }  
     UNIQUENESS     { bgpTeNlriAddress, 
                      bgpTeNextHopAddress, 
                      bgpTeReservedRate, 
                      bgpTeAvailableRate, 
                      bgpTeLossRate, 
                      bgpTePhbId, 
                      bgpTeMinOneWayDelay, 
                      bgpTeMaxOneWayDelay, 
                      bgpTeAverageOneWayDelay, 
                      bgpTeInterPacketDelay }  
     
     ::= { bgpTeTable 1 } 
 
BgpTeEntry ::= SEQUENCE {  
       
            bgpTePrid                       InstanceId, 
            bgpTeNlriAddressType           InetAddressType, 
            bgpTeNlriAddress               InetAddress, 
            bgpTeNlriAddressMask           Unsigned32, 
            bgpTeNextHopAddressType        InetAddressType, 
            bgpTeNextHopAddress            InetAddress, 
            bgpTeNextHopMask               Unsigned32, 
            bgpTeReservedRate              Unsigned32,  
            bgpTeAvailableRate             Unsigned32, 
            bgpTeLossRate                  Unsigned32, 
            bgpTePhbId                     Integer32,      
            bgpTeMinOneWayDelay            Unsigned32, 
            bgpTeMaxOneWayDelay            Unsigned32,  
            bgpTeAverageOneWayDelay         Unsigned32, 
            bgpTeInterPacketDelay          Unsigned32 

     }  
     
bgpTePrid                  OBJECT-TYPE 
      
     SYNTAX                InstanceId 
     STATUS                current 
     DESCRIPTION     
         "An integer index that uniquely identifies this instance of 
         the bgpTe class." 
 
     ::= { bgpTeEntry 1 } 
 
bgpTeNlriAddressType        OBJECT-TYPE 
      
     SYNTAX                InetAddressType 
     STATUS                current 
     DESCRIPTION 
             "The address type enumeration value ([18]) used to 
             specify the type of a route's destination IP address." 
              
    ::= { bgpTeEntry 2 } 
 
bgpTeNlriAddress           OBJECT-TYPE 
  
     SYNTAX                InetAddress  
     STATUS                current  
     DESCRIPTION  
             "The IP address to match against the NLRI field of the 
             QOS_NLRI attribute of the BGP4 UPDATE message."  
   
     ::= { bgpTeEntry 3 }  
     
bgpTeNlriAddressMask        OBJECT-TYPE 
  
     SYNTAX                Unsigned32 (0..128)  
     STATUS                current  
     DESCRIPTION  
             "Indicates the length of a mask for the matching of the 
             NLRI field of the QOS_NLRI attribute of the BGP4 UPDATE 
             message. Masks are constructed by setting bits in 
             sequence from the most-significant bit downwards for 
             bgpTeNlriMask bits length. All other bits in the mask, 
             up to the number needed to fill the length of the 
             address bgpTeNlri are cleared to zero.  A zero bit in 
             the mask then means that the corresponding bit in the 
             address always matches."
     
     ::= { bgpTeEntry 4 }  
 
bgpTeNextHopAddressType     OBJECT-TYPE 
      
     SYNTAX                InetAddressType 

     STATUS                current 
     DESCRIPTION 
             "The address type enumeration value used to specify the 
             type of the next hop's IP address." 
              
    ::= { bgpTeEntry 5 } 
 
bgpTeNextHopAddress         OBJECT-TYPE 
  
     SYNTAX                 InetAddress  
     STATUS                 current  
     DESCRIPTION  
             "On remote routes, the address of the next router en 
             route; Otherwise, 0.0.0.0."  
     
     ::= { bgpTeEntry 6 }  
     
bgpTeNextHopMask           OBJECT-TYPE 
  
     SYNTAX                Unsigned32 (0..128)  
     STATUS                current  
     DESCRIPTION  
        "Indicates the length of a mask for the matching of the next 
        hop's IP address. Masks are constructed by setting bits in 
        sequence from the most-significant bit downwards for 
        bgpTeNextHopMask bits length. All other bits in the mask, up 
        to the number needed to fill the length of the address 
        bgpTeNextHopAddress are cleared to zero.  A zero bit in the 
        mask then means that the corresponding bit in the address 
        always matches." 
     
     ::= { bgpTeEntry 7 } 
 
bgpTeReservedRate          OBJECT-TYPE  
        
     SYNTAX                 Unsigned32 (0..4294967295) 
     UNITS                 "kilobits per second" 
     STATUS                 current  
     DESCRIPTION     
        "Specifies the reserved rate that cannot be used on this 
        instance of the bgpTeNlriAddress object in this direction 
        (from the advertising BGP peer), expressed in kilobits per 
        second."  
     
     ::= { bgpTeEntry 8 } 
 
bgpTeAvailableRate         OBJECT-TYPE  
        
     SYNTAX                 Unsigned32 (0..4294967295) 
     UNITS                 "kilobits per second" 
     STATUS                 current  
     DESCRIPTION     

        "Specifies the available rate that may be reserved on this 
        instance of the bgpTeNlriAddress object in this direction 
        (from the advertising BGP peer), expressed in kilobits per 
        second."  
     
     ::= { bgpTeEntry 9 } 
 
bgpTeLossRate              OBJECT-TYPE  
        
     SYNTAX                 Unsigned32 (0..4294967295) 
     STATUS                 current  
     DESCRIPTION     
        "Specifies the packet loss ratio that has been observed on 
        this route instantiated by the bgpTeNlriAddress object."  
     
     ::= { bgpTeEntry 10 }  
     
bgpTePhbId                 OBJECT-TYPE 
  
     SYNTAX                 Integer32 (-1 | 0..63) 
     STATUS                 current  
     DESCRIPTION  
             "The binary encoding that uniquely identifies a Per Hop 
             Behaviour (PHB) or a set of PHBs associated to the 
             DiffServ Code Point marking of the IP datagrams that 
             are to be conveyed along this traffic engineered route. 
             A value of -1 indicates that a specific PHB ID value 
             has not been defined, and thus, all PHB ID values are 
             considered a match." 
   
     ::= { bgpTeEntry 11 } 
 
bgpTeMinOneWayDelay        OBJECT-TYPE 
 
     SYNTAX                 Unsigned32 (0..4294967295) 
     UNITS                 "milliseconds" 
     STATUS                 current  
     DESCRIPTION     
        "Specifies the minimum one-way delay that has been observed 
        on this route instantiated by the bgpTeNlriAddress object, 
        expressed in milliseconds."  
     
     ::= { bgpTeEntry 12 } 
 
bgpTeMaxOneWayDelay        OBJECT-TYPE 
 
     SYNTAX                 Unsigned32 (0..4294967295) 
     UNITS                 "milliseconds" 
     STATUS                 current  
     DESCRIPTION     



        "Specifies the maximum one-way delay that has been observed 
        on this route instantiated by the bgpTeNlriAddress object, 
        expressed in milliseconds."  
     
     ::= { bgpTeEntry 13 } 
 
bgpTeAverageOneWayDelay     OBJECT-TYPE 
 
     SYNTAX                 Unsigned32 (0..4294967295) 
     UNITS                 "milliseconds" 
     STATUS                 current  
     DESCRIPTION     
        "Specifies the average one-way delay that has been observed 
        on this route instantiated by the bgpTeNlriAddress object, 
        expressed in milliseconds."  
     
     ::= { bgpTeEntry 14 } 
 
bgpTeInterPacketDelay       OBJECT-TYPE 
 
     SYNTAX                 Unsigned32 (0..4294967295) 
     UNITS                 "milliseconds" 
     STATUS                 current  
     DESCRIPTION     
        "Specifies the inter-packet delay variation that has been 
        observed on this route instantiated by the bgpTeNlriAddress 
        object."  
     
     ::= { bgpTeEntry 15 } 
 
-- 
-- Traffic engineering statistics classes. The information contained 
-- in the yet-to-be defined tables aim at reporting statistics about 
-- COPS control traffic, engineered traffic and potential errors. The 
-- next version of the draft will provide a first table that will be 
-- based upon the use of the "count" clause. 
-- 
-- 
 
END 
