# -*- text -*-
#
#	Attributes and values defined in RFC 4679.
#	http://www.ietf.org/rfc/rfc4679.txt
#
#	$Id$
#

VENDOR		ADSL-Forum			3561

BEGIN-VENDOR	ADSL-Forum

#
#  The first two attributes are prefixed with "ADSL-" because of
#  conflicting names in dictionary.redback.
#
ATTRIBUTE	ADSL-Agent-Circuit-Id			1	string
ATTRIBUTE	ADSL-Agent-Remote-Id			2	string
ATTRIBUTE	Actual-Data-Rate-Upstream		129	integer
ATTRIBUTE	Actual-Data-Rate-Downstream		130	integer
ATTRIBUTE	Minimum-Data-Rate-Upstream		131	integer
ATTRIBUTE	Minimum-Data-Rate-Downstream		132	integer
ATTRIBUTE	Attainable-Data-Rate-Upstream		133	integer
ATTRIBUTE	Attainable-Data-Rate-Downstream		134	integer
ATTRIBUTE	Maximum-Data-Rate-Upstream		135	integer
ATTRIBUTE	Maximum-Data-Rate-Downstream		136	integer
ATTRIBUTE	Minimum-Data-Rate-Upstream-Low-Power	137	integer
ATTRIBUTE	Minimum-Data-Rate-Downstream-Low-Power	138	integer
ATTRIBUTE	Maximum-Interleaving-Delay-Upstream	139	integer
ATTRIBUTE	Actual-Interleaving-Delay-Upstream	140	integer
ATTRIBUTE	Maximum-Interleaving-Delay-Downstream	141	integer
ATTRIBUTE	Actual-Interleaving-Delay-Downstream	142	integer

#
#  This next attribute has a weird encoding.
#
#  Octet[0] - 0x01	AAL5
#  Octet[0] - 0x02	Ethernet

#  Octet[1] - 0x00	Not Available
#  Octet[1] - 0x01	Untagged Ethernet
#  Octet[1] - 0x02	Single-Tagged Ethernet

#  Octet[2] - 0x00	Not available
#  Octet[2] - 0x01	PPPoA LLC
#  Octet[2] - 0x02	PPPoA Null
#  Octet[2] - 0x03	IPoA LLC
#  Octet[2] - 0x04	IPoA NULL
#  Octet[2] - 0x05	Ethernet over AAL5 LLC with FCS
#  Octet[2] - 0x06	Ethernet over AAL5 LLC without FCS
#  Octet[2] - 0x07	Ethernet over AAL5 Null with FCS
#  Octet[2] - 0x08	Ethernet over AAL5 Null without FCS
#
ATTRIBUTE	Access-Loop-Encapsulation		144	octets # 3

#
#  If this attribute exists, it means that IFW has been performed
#  for the subscribers session.
#
ATTRIBUTE	IWF-Session				252	octets # 0

END-VENDOR ADSL-Forum
