# -*- text -*-
# Copyright (C) 2015 The FreeRADIUS Server project and contributors
#
#	3com SuperStack Firewall dictionary
#	Bought from Sonicwall, apparently, from Enterprise number 8741.
#
#		$Id: 2898ff656afb26c302ec2c613f29223689f03859 $
#

VENDOR		3com				43

#
#	These attributes contain the access-level value.
#
BEGIN-VENDOR	3com

ATTRIBUTE	3Com-User-Access-Level			1	integer

#	Read-only access to basic network tools (ping, etc)
VALUE	3Com-User-Access-Level		3Com-Visitor		0

#	Read-only access to manageable (not security) parameters
VALUE	3Com-User-Access-Level		3Com-Monitor		1

# 	Read-write access to manageable (not security) parameters
VALUE	3Com-User-Access-Level		3Com-Manager		2

#	Read-write access to all manageable parameters
VALUE	3Com-User-Access-Level		3Com-Administrator	3

ATTRIBUTE	3Com-VLAN-Name				2	string
ATTRIBUTE	3Com-Mobility-Profile			3	string
ATTRIBUTE	3Com-Encryption-Type			4	string
ATTRIBUTE	3Com-Time-Of-Day			5	string
ATTRIBUTE	3Com-SSID				6	string

#	String formatted as: YY/MM/DD-HH:MM
#	NOT as a "date" attribute!
ATTRIBUTE	3Com-End-Date				7	string

#	Commented out, because the 3Com documentation
#	gives it the same number as End-Date, above.
#ATTRIBUTE	3Com-Start-Date				7	string

#	URL where the user is redirected after WebAAA
ATTRIBUTE	3Com-URL				8	string

ATTRIBUTE	3Com-Connect_Id				26	integer
ATTRIBUTE	3Com-NAS-Startup-Timestamp		59	integer
ATTRIBUTE	3Com-Ip-Host-Addr			60	string
ATTRIBUTE	3Com-Product-ID				255	string

END-VENDOR	3com
