PARTITION-PIB PIB-DEFINITIONS ::= BEGIN 
 
IMPORTS 
    ibrpib
            FROM TUBS-SMI
    Unsigned32, Integer32, 
    MODULE-IDENTITY, OBJECT-TYPE, TEXTUAL-CONVENTION
            FROM COPS-PR-SPPI
    InstanceId 
            FROM COPS-PR-SPPI-TC
    TruthValue
            FROM SNMPv2-TC
    InetAddress
            FROM INET-ADDRESS-MIB;
 
switchPartitionPib  MODULE-IDENTITY 
    SUBJECT-CATEGORIES { all } 
    LAST-UPDATED "200201010000Z"  -- modified
    ORGANIZATION "IETF" 
    CONTACT-INFO " 
          Todd A. Anderson 
          Intel 
          2111 NE 25th Avenue 
          Hillsboro, OR 97124 USA 
          Phone: +1 503 712 1760 
          Email: todd.a.anderson@intel.com 
 
          Avri Doria 
          Nortel Networks 
          600 Technology Park Drive 
          Billerica  MA 01821 
          Phone: +1 401 663 5024 
          Email: avri@nortelnetworks.com 
 
          Jiang Yong 
          Telia Research AB 
          123 86 Farsta 
          Sweden 
          Phone: +46 (0) 8 713 81 25 
          Email: yong.b.jiang@telia.se 
 
          Jerry Sydir                     
          CPlane Inc.                     
          5150 El Camino Real Suite B-31 
          Los Altos, CA 94022 
          Phone: +1(650) 938-8066 x102 
          sydir@cplane.com 
 
          Balaji Srinivasan                     
          CPlane Inc.                     
          5150 El Camino Real Suite B-31 
          Los Altos, CA 94022 
          phone: +1(650) 938-8066 x103 
          balaji@cplane.com" 
    DESCRIPTION 
"The PIB module specifies a set of policy rule classes  
for partitioning a single switch into a set of virtual  
switches." 
    ::= { ibrpib 19 } 
 
vSConfig  OBJECT IDENTIFIER ::= { switchPartitionPib 1 } 
 
PortDirection ::= TEXTUAL-CONVENTION 
    STATUS        current 
    DESCRIPTION 
      "The following type is used to specify the direction of the 
      label ranges and the bandwidth in the physical port of the  
      switch as well as  the virtual port of the virtual switch." 
    SYNTAX  INTEGER { 
        incoming(1), 
        outgoing(2) 
    } 
 
RatioString ::= TEXTUAL-CONVENTION 
   STATUS       current 
   DESCRIPTION 
     "This data type is used to model a floating number,  
     specifically here the cell loss ratio and a  
     probability number. It is required to be of the form  
     m:n, where m and n are both integers and represent a  
     floating number m divided by n." 
   SYNTAX       OCTET STRING (SIZE(3)) 
 
VectorString ::= TEXTUAL-CONVENTION 
   STATUS       current 
   DESCRIPTION 
     "This data type is used to model a 2-dimentional  
     number (x,y). Here it is used to specify the vpi/vci  
     range for an ATM interface. 2 vectors, (minVpi,  
     minVci) and (maxVpi, maxVci), make up a label range.  
     It is required to have the format x:y" 
   SYNTAX       OCTET STRING (SIZE(3..8)) 
 
PortType ::= TEXTUAL-CONVENTION 
        STATUS          current 
        DESCRIPTION  
          "This data type is used to model the port type of the  
          switch" 
        SYNTAX          INTEGER { 
          atm(1), 
          frameRelay(2), 
          ethernetSwitch(3), 
          mpls(4), 
          ipRouting(5) 
        } 
 
-- 
--================================================================ 
--This table performParamTable is used to represent the 
--performance targets associated with the equivalent bandwidths  
--for each port. This table allows the bandwidth, buffer space,  
--and queue schedulers assigned to a VS to be  simply abstracted  
--using a single parameter: the Equivalent bandwidth per port 
--assigned to the VS. Each entry in the VS interface bandwidth  
--table uses its serviceParamIndex to point to a row in this  
--table. Then the equivalent bandwidth points to a performance  
--target set by the service descriptor parameters. The performance  
--target is most common in the form of a loss target but also a  
--delay target can be used.  
--================================================================ 
performParamTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF PerformParamEntry 
   PIB-ACCESS install
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured performance targets  
               for this switch" 
   ::= { switchPartitionPib 2 } 
 
performParamEntry OBJECT-TYPE 
   SYNTAX PerformParamEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives each performance target  
               parameters" 
   PIB-INDEX { performParamIndex } 
   ::= { performParamTable 1 } 
 
PerformParamEntry ::= 
   SEQUENCE { 
      performParamIndex       InstanceId, 
      performPLR              RatioString, 
      performMaxDelay         INTEGER, 
      performDelayOverProb    RatioString 
   } 
 
performParamIndex OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Identifies each performance target" 
   ::= { performParamEntry 1 } 
 
performPLR OBJECT-TYPE 
   SYNTAX RatioString 
   PIB-ACCESS install
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This indicates the packet loss ratio " 
   ::= { performParamEntry 2 } 
 
performMaxDelay OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install
   STATUS current -- war vorher: mandatory 
   DESCRIPTION " This indicates the maximum packet delay " 
   ::= { performParamEntry 3 } 
 
performDelayOverProb OBJECT-TYPE 
   SYNTAX RatioString 
   PIB-ACCESS install
   STATUS current -- war vorher: mandatory 
   DESCRIPTION " This indicates the possibility that the packet   
               delay is bigger than the maximum delay allowed" 
   ::= { performParamEntry 4 } 
 
--=================================== 
--End of performParamTable 
--=================================== 
 
vSConfigTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSConfigEntry 
   PIB-ACCESS install
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Each row in this table describes a virtual switch  
               that has been created on this switch" 
   ::= { vSConfig 1 } 
 
vSConfigEntry OBJECT-TYPE 
   SYNTAX VSConfigEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Describes a virtual switch" 
   PIB-INDEX { vSConfigVSID } 
   ::= { vSConfigTable 1 } 
 
VSConfigEntry ::=  
   SEQUENCE { 
      vSConfigVSID              InstanceId, 
      vSAdminStatus             INTEGER, 
      vSOperStatus              INTEGER, 
      vSNumPorts                INTEGER, 
      vSNumRoutingEntries       INTEGER 
} 
 
vSConfigVSID OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Identifies the virtual switch within this switch" 
   ::= { vSConfigEntry 1 } 
 
vSAdminStatus OBJECT-TYPE 
   SYNTAX INTEGER { 
             up(1), 
             down(2), 
             testing(3) 
   } 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The administrative state of the virtual switch. A 
                virtual switch's administrative status can not be  
                'up' until all the necessary parameters for this  
                virtual switch have been specified" 
   ::={ vSConfigEntry 2 } 
 
vSOperStatus OBJECT-TYPE 
   SYNTAX INTEGER { 
             up(1), 
             down(2) 
          } 
   PIB-ACCESS notify
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The current operational state of the virtual  
               switch" 
   ::={ vSConfigEntry 3 } 
 
vSNumPorts OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The number of virtual ports in this virtual  
               switch" 
   ::= {vSConfigEntry 4 } 
 
vSNumRoutingEntries OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION  
     "The number of routing table entries allocated to  
     this virtual switch.  This value is ignored if the  
     switch has only per port routing tables (i.e., no  
     switch-wide routing table)" 
   ::= {vSConfigEntry 5 } 
 
--=============================== 
-- END OF VSConfigTable 
--=============================== 
 
vSCtrlConfigTable OBJECT-TYPE 
  SYNTAX SEQUENCE OF VSCtrlConfigEntry 
  PIB-ACCESS install 
  STATUS current -- war vorher: mandatory 
  DESCRIPTION "This table gives the per controller configured for  
              the VS" 
  ::={vSConfig 2} 
 
vSCtrlConfigEntry OBJECT-TYPE 
  SYNTAX VSCtrlConfigEntry 
  STATUS current -- war vorher: mandatory 
  DESCRIPTION "Configuration for each controller for the VS" 
  PIB-INDEX { vSCtrlConfigVSID } 
  ::= {vSCtrlConfigTable 1} 
 
VSCtrlConfigEntry ::= 
  SEQUENCE { 
      vSCtrlConfigVSID            InstanceId, 
      vSCtrlID                    INTEGER, 
      vSSciType                   INTEGER, 
      vSSciTransportType          INTEGER, 
      vSSciTCPPortNumber          INTEGER, 
      vSSciPortInterfaceNum       INTEGER, 
      vSSciVpiNumber              INTEGER, 
      vSSciVciNumber              INTEGER 
} 
 
vSCtrlConfigVSID OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Identifies the virtual switch within this switch" 
   ::= { vSCtrlConfigEntry 1 } 
 
vSCtrlID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Identifies the virtual switch controller across  
               the SCI" 
   ::= { vSCtrlConfigEntry 2 } 
 
vSSciType OBJECT-TYPE 
   SYNTAX INTEGER { 
            gsmp(1), 
            megacop(2), 
            cops-pr(3) 
          } 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The switch control protocol used to control this 
                virtual switch" 
   ::= { vSCtrlConfigEntry 3 } 
 
vSSciTransportType OBJECT-TYPE 
   SYNTAX INTEGER { 
       ethernet(1), 
       tcp(2), 
       atm(3) 
   } 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Transport protocol used to transport SCI PDUs" 
   ::= { vSCtrlConfigEntry 4 } 
 
vSSciTCPPortNumber OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The local port number used to access the virtual  
               switch. Meaningful only when the transport type is  
               TCP" 
   ::= { vSCtrlConfigEntry 5 } 
 
vSSciPortInterfaceNum OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This is the physical interface over which control 
                messages are exchanged. " 
   ::= { vSCtrlConfigEntry 6 } 
 
vSSciVpiNumber OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The VPI on which the control messages are  
               exchanged. Meaningful only when the SCI transport  
               is ATM" 
   ::= { vSCtrlConfigEntry 7 } 
 
vSSciVciNumber OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The VCI on which the control messages are  
               exchanged. Meaningful only when the SCI transport  
               is ATM" 
   ::= { vSCtrlConfigEntry 8 } 
 
--=============================== 
--END OF VSCtrlConfigTable 
--=============================== 
 
vSPortConfigTable OBJECT-TYPE 
   SYNTAX    SEQUENCE OF VSPortConfigEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory
   DESCRIPTION "Resource configuration for the virtual ports" 
   ::= { vSConfig 3 } 
 
vSPortConfigEntry OBJECT-TYPE 
   SYNTAX VSPortConfigEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port resource configured  
               for the virtual switch" 
   PIB-INDEX { vSPortConfigVSID } 
   UNIQUENESS { vSPortConfigVSID, vSPortConfigPortID } 
   ::= { vSPortConfigTable 1 } 
 
VSPortConfigEntry ::= 
   SEQUENCE { 
      vSPortConfigVSID             InstanceId, 
      vSPortConfigPortID           INTEGER, 
      vSPhysicalPortNumber         INTEGER, 
      vSPortConfigPortNumBWs       INTEGER, 
      vSPortConfigNumLabelRanges   INTEGER, 
      vSPortNumRoutingEntries      INTEGER 
} 
 
vSPortConfigVSID OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This is the virtual switch ID of the virtual  
               switch" 
   ::= { vSPortConfigEntry 1 } 
 
vSPortConfigPortID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This is the virtual port id in the current virtual          
               switch" 
   ::= { vSPortConfigEntry 2 } 
 
vSPhysicalPortNumber OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The physical port number that is mapped to virtual  
               port" 
   ::= { vSPortConfigEntry 3 } 
 
vSPortConfigPortNumBWs OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Number of equivalent bandwidth pointing to  
               different performance targets (packet loss ratio  
               and delay) in both incoming and outgoing directions  
               for this port." 
   ::= { vSPortConfigEntry 4 } 
 
vSPortConfigNumLabelRanges OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Number of label ranges for this port. The label  
               can be of different types depending on the  
               interface service type." 
   ::= { vSPortConfigEntry 5} 
 
vSPortNumRoutingEntries OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The number of routing table entries allocated to   
               this virtual port from the physical port.  This  
               value is used only if the switch has per port  
               routing tables" 
   ::= {vSPortConfigEntry 6 } 
 
--================================ 
-- END OF VSPortConfigTable  
--================================ 
 
 
-- 
--================================================================ 
-- The table VSConfigBWTable gives the equivalent bandwidth  
--pointing to different service category for input and output at  
--the virtual ports. The table has 3 indices; virtual switch ID,  
--port ID and Bandwidth ID 
--================================================================ 
 
vSPortConfigBWTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSPortConfigBWEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured bandwidth information  
                for the various virtual ports" 
   ::= { vSConfig 4 } 
 
vSPortConfigBWEntry OBJECT-TYPE 
   SYNTAX VSPortConfigBWEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the configured bandwidth  
               information for the various virtual ports" 
   PIB-INDEX { vSPortConfigBWVSID } 
   UNIQUENESS { vSPortConfigBWVSID, 
                vSPortConfigBWPortID, 
                vSPortConfigBWID } 
   ::= { vSPortConfigBWTable 1 } 
 
VSPortConfigBWEntry ::= 
   SEQUENCE { 
      vSPortConfigBWVSID               InstanceId, 
      vSPortConfigBWPortID             INTEGER, 
      vSPortConfigBWID                 INTEGER, 
      vSPortConfigEqiBW                INTEGER, 
      vSPortConfigIndex                OBJECT IDENTIFIER, 
      vSPortConfigBWPortDirection      PortDirection 
} 
 
vSPortConfigBWVSID OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This is the virtual switch ID of the virtual  
               switch" 
   ::= { vSPortConfigBWEntry 1 } 
 
vSPortConfigBWPortID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This is the virtual port id in the current virtual  
               switch" 
   ::= { vSPortConfigBWEntry 2 } 
 
vSPortConfigBWID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This is the equivalent bandwidth ID in the current 
                virtual switch" 
   ::= { vSPortConfigBWEntry 3 } 
 
vSPortConfigEqiBW OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the equivalent bandwidth assigned 
                to this VS " 
   ::= { vSPortConfigBWEntry 4 } 
 
vSPortConfigIndex OBJECT-TYPE 
   SYNTAX OBJECT IDENTIFIER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION " Indicates an entry in the performParamTable 
                 which represents the performance target 
                 associated to by this equivalent bandwidth " 
   ::= { vSPortConfigBWEntry 5 } 
 
vSPortConfigBWPortDirection OBJECT-TYPE 
   SYNTAX PortDirection 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the direction for which this equivalent 
                bandwidth is valid" 
   ::= { vSPortConfigBWEntry 6 } 
 
--================================== 
-- END OF VSPortConfigBWTable  
--================================== 
 
 
-- 
--================================================================ 
-- The VSLabelRangeConfigTable gives the label ranges for input  
-- and output at the virtual ports. 
-- The tables have 3 indices; virtual switch ID, port ID and Range  
-- ID 
--================================================================ 
 
vSPortConfigLabelRangeTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSPortConfigLabelRangeEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured label range  
               information for the various virtual ports" 
   ::= { vSConfig 5 } 
 
vSPortConfigLabelRangeEntry OBJECT-TYPE 
   SYNTAX VSPortConfigLabelRangeEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port label ranges  
               configured for the virtual switch." 
   PIB-INDEX { vSPortConfigLabelRangeID } 
   UNIQUENESS { 
                vSPortConfigLabelRangeID } 
   ::= { vSPortConfigLabelRangeTable 1 } 
 
VSPortConfigLabelRangeEntry ::= 
   SEQUENCE { 
      vSPortConfigLabelRangeID          InstanceId, 
      vSPortConfigPortDirection         PortDirection, 
      vSPortConfigLabelRangeType        INTEGER, 
      vSPortConfigLabelRangeIndex       INTEGER 
}  
 
vSPortConfigLabelRangeID OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Identifies the label range" 
   ::= { vSPortConfigLabelRangeEntry 1 } 
 
vSPortConfigPortDirection OBJECT-TYPE 
   SYNTAX PortDirection 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the direction for which this range is  
               valid" 
   ::= { vSPortConfigLabelRangeEntry 2 } 
 
vSPortConfigLabelRangeType OBJECT-TYPE 
   SYNTAX INTEGER  
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the type of protocol for this label  
               range." 
   ::= { vSPortConfigLabelRangeEntry 3 } 
 
vSPortConfigLabelRangeIndex OBJECT-TYPE 
   SYNTAX INTEGER  
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "The index into the protocol-dependent label  
                range table for this virtual switch." 
   ::= { vSPortConfigLabelRangeEntry 4 } 
 
--==================================== 
-- END OF VSPortConfigLabelRangeTable   
--==================================== 
 
 
-- 
--================================================================ 
-- The table VSAtmLabelRangeTable is used to give the VPI/VCI 
-- label ranges at the ATM virtual switch level.  
--================================================================ 
 
vSAtmLabelRangeTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSAtmLabelRangeEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured ATM label range  
               information for the various switch ports on this  
               virtual switch." 
   ::= { vSConfig 6 } 
 
vSAtmLabelRangeEntry OBJECT-TYPE 
   SYNTAX VSAtmLabelRangeEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port ATM label ranges and 
                capabilities." 
   PIB-INDEX { vSAtmLabelRangeIndex } 
   ::= { vSAtmLabelRangeTable 1 } 
 
VSAtmLabelRangeEntry ::= 
   SEQUENCE { 
      vSAtmLabelRangeIndex              InstanceId, 
      vSAtmLabelRangeMinVpiVci          VectorString, 
      vSAtmLabelRangeMaxVpiVci          VectorString, 
      vSAtmLabelRangeAllowsVP           TruthValue, 
      vSAtmLabelRangeAllowsP2MP         TruthValue, 
      vSAtmLabelRangeAllowsMP2P         TruthValue, 
      vSAtmLabelRangeMaxMulticast       INTEGER 
} 
 
vSAtmLabelRangeIndex OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Index into this table." 
   ::= { vSAtmLabelRangeEntry 1 } 
 
vSAtmLabelRangeMinVpiVci OBJECT-TYPE 
   SYNTAX VectorString 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Lower bound of the vpi and vci range." 
   ::= { vSAtmLabelRangeEntry 2 } 
 
vSAtmLabelRangeMaxVpiVci OBJECT-TYPE 
   SYNTAX VectorString 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Upper bound of the vpi and vci range." 
   ::= { vSAtmLabelRangeEntry 3 } 
 
vSAtmLabelRangeAllowsVP OBJECT-TYPE 
   SYNTAX TruthValue 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates whether this label range can be used for  
               VP connections." 
   ::= { vSAtmLabelRangeEntry 4 } 
 
vSAtmLabelRangeAllowsP2MP OBJECT-TYPE 
   SYNTAX TruthValue 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates whether this label range can be used to  
               create point-to-multipoint connections." 
   ::= { vSAtmLabelRangeEntry 5 } 
 
vSAtmLabelRangeAllowsMP2P OBJECT-TYPE 
   SYNTAX TruthValue 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates whether this label range can be used to  
               create multipoint-to-point connections." 
   ::= { vSAtmLabelRangeEntry 6 } 
 
vSAtmLabelRangeMaxMulticast OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the maximum number of multicast  
               connections that can be created within this range." 
   ::= { vSAtmLabelRangeEntry 7 } 
 
--==================================== 
-- END OF VSAtmLabelRangeTable   
--==================================== 
 
 
-- 
--================================================================ 
-- The table VSFrLabelRangeTable is used to give the DLCI label  
-- ranges on a Frame Relay interface for a virtual switch. 
--================================================================ 
 
vSFrLabelRangeTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSFrLabelRangeEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured label range  
               information for the various frame relay ports." 
   ::= { vSConfig 7 } 
 
vSFrLabelRangeEntry OBJECT-TYPE 
   SYNTAX VSFrLabelRangeEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port label ranges" 
   PIB-INDEX { vSFrLabelRangeIndex } 
   ::= { vSFrLabelRangeTable 1 } 
 
VSFrLabelRangeEntry ::= 
   SEQUENCE { 
      vSFrLabelRangeIndex             InstanceId, 
      vSFrLabelRangeMinDLCI           INTEGER, 
      vSFrLabelRangeMaxDLCI           INTEGER 
} 
 
vSFrLabelRangeIndex OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Index into this table." 
   ::= { vSFrLabelRangeEntry 1 } 
 
 
vSFrLabelRangeMinDLCI OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Lower bound of the DLCI range for this Frame Relay  
                interface." 
   ::= { vSFrLabelRangeEntry 2 } 
 
vSFrLabelRangeMaxDLCI OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Upper bound of the DLCI range for this Frame Relay 
                interface." 
   ::= { vSFrLabelRangeEntry 3 } 
 
 
--==================================== 
-- END OF VSFrLabelRangeTable   
--==================================== 
 
-- 
--================================================================ 
-- The table VSVlanLabelRangeTable is used to give the VLAN ID  
-- label ranges on a VLAN-aware Ethernet interface for a virtual  
-- switch. 
--================================================================ 
 
vSVlanLabelRangeTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSVlanLabelRangeEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured label range  
               information for the VLAN-aware Ethernet ports." 
   ::= { vSConfig 8 } 
 
vSVlanLabelRangeEntry OBJECT-TYPE 
   SYNTAX VSVlanLabelRangeEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port VLAN ID ranges" 
   PIB-INDEX { vSVlanLabelRangeIndex } 
   ::= { vSVlanLabelRangeTable 1 } 
 
VSVlanLabelRangeEntry ::= 
   SEQUENCE { 
      vSVlanLabelRangeIndex           InstanceId, 
      vSVlanLabelRangeMinID           INTEGER, 
      vSVlanLabelRangeMaxID           INTEGER 
} 
 
vSVlanLabelRangeIndex OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Index into this table." 
   ::= { vSVlanLabelRangeEntry 1 } 
 
vSVlanLabelRangeMinID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Lower bound of the VLAN ID range on this VLAN- 
               aware Ethernet switch interface." 
   ::= { vSVlanLabelRangeEntry 2 } 
 
vSVlanLabelRangeMaxID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Upper bound of the VLAN ID range on this VLAN-     
               aware Ethernet switch interface." 
   ::= { vSVlanLabelRangeEntry 3 } 
 
--==================================== 
-- END OF VSVlanLabelRangeTable   
--==================================== 
 
-- 
--================================================================ 
-- The table mplsLabelRangeTable is used to give the label ranges 
-- on a MPLS interface. 
--================================================================ 
 
vSMplsLabelRangeTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSMplsLabelRangeEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured label range  
               information for MPLS ports." 
   ::= { vSConfig 9 } 
 
vSMplsLabelRangeEntry OBJECT-TYPE 
   SYNTAX VSMplsLabelRangeEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port MPLS ranges." 
   PIB-INDEX { vSMplsLabelRangeIndex } 
   ::= { vSMplsLabelRangeTable 1 } 
 
VSMplsLabelRangeEntry ::= 
   SEQUENCE { 
      vSMplsLabelRangeIndex           InstanceId, 
      vSMplsLabelRangeMinID           INTEGER, 
      vSMplsLabelRangeMaxID           INTEGER 
} 
 
vSMplsLabelRangeIndex OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Index into this table." 
   ::= { vSMplsLabelRangeEntry 1 } 
 
 
vSMplsLabelRangeMinID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Lower bound of the MPLS label range." 
   ::= { vSMplsLabelRangeEntry 2 } 
 
vSMplsLabelRangeMaxID OBJECT-TYPE 
   SYNTAX INTEGER 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Upper bound of the MPLS label range." 
   ::= { vSMplsLabelRangeEntry 3 } 
 
--==================================== 
-- END OF VSMplsLabelRangeTable   
--==================================== 
 
--================================================================ 
-- The table VSIpLabelRangeTable is used to give the IP ranges on  
-- an IP interface for a virtual switch. 
--================================================================ 
 
vSIpLabelRangeTable OBJECT-TYPE 
   SYNTAX SEQUENCE OF VSIpLabelRangeEntry 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Table giving the configured IP ranges for IP  
               ports." 
   ::= { vSConfig 10 } 
 
vSIpLabelRangeEntry OBJECT-TYPE 
   SYNTAX VSIpLabelRangeEntry 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "This table gives the per port IP ranges." 
   PIB-INDEX { vSIpLabelRangeIndex } 
   ::= { vSIpLabelRangeTable 1 } 
 
VSIpLabelRangeEntry ::= 
   SEQUENCE { 
      vSIpLabelRangeIndex        InstanceId, 
      vSIpLabelRangeIP           InetAddress, 
      vSIpLabelRangeIPMask       InetAddress 
} 
 
vSIpLabelRangeIndex OBJECT-TYPE 
   SYNTAX InstanceId 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Index into this table." 
   ::= { vSIpLabelRangeEntry 1 } 
 
vSIpLabelRangeIP OBJECT-TYPE 
   SYNTAX InetAddress 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the IP address for a particular network."
   ::= { vSIpLabelRangeEntry 2 } 
 
vSIpLabelRangeIPMask OBJECT-TYPE 
   SYNTAX InetAddress 
   PIB-ACCESS install 
   STATUS current -- war vorher: mandatory 
   DESCRIPTION "Indicates the subnet's mask address." 
   ::= { vSIpLabelRangeEntry 3 } 
 
--==================================== 
-- END OF VSIpLabelRangeTable   
--==================================== 
 
END 
