ETHER-WIS DEFINITIONS ::= BEGIN

IMPORTS
    MODULE-IDENTITY, OBJECT-TYPE,
    Gauge32, transmission
        FROM SNMPv2-SMI
    ifIndex
        FROM IF-MIB
    MODULE-COMPLIANCE, OBJECT-GROUP
        FROM SNMPv2-CONF
    sonetMediumStuff2, sonetSectionStuff2,
    sonetLineStuff2, sonetFarEndLineStuff2,
    sonetPathStuff2, sonetFarEndPathStuff2,
    sonetMediumType, sonetMediumLineCoding,
    sonetMediumLineType, sonetMediumCircuitIdentifier,
    sonetMediumLoopbackConfig, sonetSESthresholdSet,
    sonetPathCurrentWidth
        FROM SONET-MIB;

etherWisMIB MODULE-IDENTITY
    LAST-UPDATED "200309190000Z"  -- September 19, 2003
        ORGANIZATION "IETF Ethernet Interfaces and Hub MIB
                     Working Group"
        CONTACT-INFO
           "WG charter:
              http://www.ietf.org/html.charters/hubmib-charter.html

            Mailing Lists:
              General Discussion: hubmib@ietf.org
              To Subscribe: hubmib-request@ietf.org
              In Body: subscribe your_email_address

             Chair: Dan Romascanu
            Postal: Avaya Inc.
                    Atidim Technology Park, Bldg. 3
                    Tel Aviv 61131
                    Israel
               Tel: +972 3 645 8414
            E-mail: dromasca@avaya.com

            Editor: C. M. Heard
            Postal: 600 Rainbow Dr. #141
                    Mountain View, CA 94041-2542
                    USA
               Tel: +1 650-964-8391
            E-mail: heard@pobox.com"



    DESCRIPTION
      "The objects in this MIB module are used in conjunction
      with objects in the SONET-MIB and the MAU-MIB to manage
      the Ethernet WAN Interface Sublayer (WIS).

      The following reference is used throughout this MIB module:

      [IEEE 802.3 Std] refers to:
         IEEE Std 802.3, 2000 Edition: 'IEEE Standard for
         Information technology - Telecommunications and
         information exchange between systems - Local and
         metropolitan area networks - Specific requirements -
         Part 3: Carrier sense multiple access with collision
         detection (CSMA/CD) access method and physical layer
         specifications', as amended by IEEE Std 802.3ae-2002,
         'IEEE Standard for Carrier Sense Multiple Access with
         Collision Detection (CSMA/CD) Access Method and
         Physical Layer Specifications - Media Access Control
         (MAC) Parameters, Physical Layer and Management
         Parameters for 10 Gb/s Operation', 30 August 2002.

      Of particular interest are Clause 50, 'WAN Interface
      Sublayer (WIS), type 10GBASE-W', Clause 30, '10Mb/s,
      100Mb/s, 1000Mb/s, and 10Gb/s MAC Control, and Link
      Aggregation Management', and Clause 45, 'Management
      Data Input/Output (MDIO) Interface'.

      Copyright (C) The Internet Society (2003).  This version
      of this MIB module is part of RFC 3637;  see the RFC
      itself for full legal notices."

    REVISION    "200309190000Z"  -- September 19, 2003
    DESCRIPTION "Initial version, published as RFC 3637."

    ::= { transmission 134 }

-- The main sections of the module

etherWisObjects     OBJECT IDENTIFIER ::= { etherWisMIB 1 }

etherWisObjectsPath OBJECT IDENTIFIER ::= { etherWisMIB 2 }

etherWisConformance OBJECT IDENTIFIER ::= { etherWisMIB 3 }








-- groups in the Ethernet WIS MIB module

etherWisDevice      OBJECT IDENTIFIER ::= { etherWisObjects 1 }

etherWisSection     OBJECT IDENTIFIER ::= { etherWisObjects 2 }

etherWisPath        OBJECT IDENTIFIER ::= { etherWisObjectsPath 1 }

etherWisFarEndPath  OBJECT IDENTIFIER ::= { etherWisObjectsPath 2 }


-- The Device group

-- These objects provide WIS extensions to
-- the SONET-MIB Medium Group.

etherWisDeviceTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF EtherWisDeviceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "The table for Ethernet WIS devices"
     ::= { etherWisDevice 1 }

etherWisDeviceEntry OBJECT-TYPE
    SYNTAX  EtherWisDeviceEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "An entry in the Ethernet WIS device table.  For each
       instance of this object there MUST be a corresponding
       instance of sonetMediumEntry."
    INDEX  { ifIndex }
     ::= { etherWisDeviceTable 1 }

EtherWisDeviceEntry ::=
    SEQUENCE {
        etherWisDeviceTxTestPatternMode     INTEGER,
        etherWisDeviceRxTestPatternMode     INTEGER,
        etherWisDeviceRxTestPatternErrors   Gauge32
        }










etherWisDeviceTxTestPatternMode OBJECT-TYPE
    SYNTAX  INTEGER {
                none(1),
                squareWave(2),
                prbs31(3),
                mixedFrequency(4)
            }
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "This variable controls the transmit test pattern mode.
       The value none(1) puts the the WIS transmit path into
       the normal operating mode.  The value squareWave(2) puts
       the WIS transmit path into the square wave test pattern
       mode described in [IEEE 802.3 Std.] subclause 50.3.8.1.
       The value prbs31(3) puts the WIS transmit path into the
       PRBS31 test pattern mode described in [IEEE 802.3 Std.]
       subclause 50.3.8.2.  The value mixedFrequency(4) puts the
       WIS transmit path into the mixed frequency test pattern
       mode described in [IEEE 802.3 Std.] subclause 50.3.8.3.
       Any attempt to set this object to a value other than
       none(1) when the corresponding instance of ifAdminStatus
       has the value up(1) MUST be rejected with the error
       inconsistentValue, and any attempt to set the corresponding
       instance of ifAdminStatus to the value up(1) when an
       instance of this object has a value other than none(1)
       MUST be rejected with the error inconsistentValue."
    REFERENCE
       "[IEEE 802.3 Std.], 50.3.8, WIS test pattern generator and
       checker, 45.2.2.6, 10G WIS control 2 register (2.7), and
       45.2.2.7.2, PRBS31 pattern testing ability (2.8.1)."
     ::= { etherWisDeviceEntry 1 }

etherWisDeviceRxTestPatternMode OBJECT-TYPE
    SYNTAX  INTEGER {
                none(1),
                prbs31(3),
                mixedFrequency(4)
            }
    MAX-ACCESS  read-write
    STATUS  current










    DESCRIPTION
       "This variable controls the receive test pattern mode.
       The value none(1) puts the the WIS receive path into the
       normal operating mode.  The value prbs31(3) puts the WIS
       receive path into the PRBS31 test pattern mode described
       in [IEEE 802.3 Std.] subclause 50.3.8.2.  The value
       mixedFrequency(4) puts the WIS receive path into the mixed
       frequency test pattern mode described in [IEEE 802.3 Std.]
       subclause 50.3.8.3.  Any attempt to set this object to a
       value other than none(1) when the corresponding instance
       of ifAdminStatus has the value up(1) MUST be rejected with
       the error inconsistentValue, and any attempt to set the
       corresponding instance of ifAdminStatus to the value up(1)
       when an instance of this object has a value other than
       none(1) MUST be rejected with the error inconsistentValue."
    REFERENCE
       "[IEEE 802.3 Std.], 50.3.8, WIS test pattern generator and
       checker, 45.2.2.6, 10G WIS control 2 register (2.7), and
       45.2.2.7.2, PRBS31 pattern testing ability (2.8.1)."
     ::= { etherWisDeviceEntry 2 }

etherWisDeviceRxTestPatternErrors OBJECT-TYPE
    SYNTAX  Gauge32 ( 0..65535 )
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "This object counts the number of errors detected when the
       WIS receive path is operating in the PRBS31 test pattern
       mode.  It is reset to zero when the WIS receive path
       initially enters that mode, and it increments each time
       the PRBS pattern checker detects an error as described in
       [IEEE 802.3 Std.] subclause 50.3.8.2 unless its value is
       65535, in which case it remains unchanged.  This object is
       writeable so that it may be reset upon explicit request
       of a command generator application while the WIS receive
       path continues to operate in PRBS31 test pattern mode."
    REFERENCE
       "[IEEE 802.3 Std.], 50.3.8, WIS test pattern generator and
       checker, 45.2.2.7.2, PRBS31 pattern testing ability
       (2.8.1), and 45.2.2.8, 10G WIS test pattern error counter
       register (2.9)."
     ::= { etherWisDeviceEntry 3 }









-- The Section group

-- These objects provide WIS extensions to
-- the SONET-MIB Section Group.

etherWisSectionCurrentTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF EtherWisSectionCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "The table for the current state of Ethernet WIS sections."
     ::= { etherWisSection 1 }

etherWisSectionCurrentEntry OBJECT-TYPE
    SYNTAX  EtherWisSectionCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "An entry in the etherWisSectionCurrentTable.  For each
       instance of this object there MUST be a corresponding
       instance of sonetSectionCurrentEntry."
    INDEX  { ifIndex }
     ::= { etherWisSectionCurrentTable 1 }

EtherWisSectionCurrentEntry ::=
    SEQUENCE {
        etherWisSectionCurrentJ0Transmitted OCTET STRING,
        etherWisSectionCurrentJ0Received    OCTET STRING
        }

etherWisSectionCurrentJ0Transmitted OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (16))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "This is the 16-octet section trace message that
       is transmitted in the J0 byte.  The value SHOULD
       be '89'h followed by fifteen octets of '00'h
       (or some cyclic shift thereof) when the section
       trace function is not used, and the implementation
       SHOULD use that value (or a cyclic shift thereof)
       as a default if no other value has been set."
    REFERENCE
       "[IEEE 802.3 Std.], 30.8.1.1.8, aJ0ValueTX."
     ::= { etherWisSectionCurrentEntry 1 }






etherWisSectionCurrentJ0Received OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "This is the 16-octet section trace message that
       was most recently received in the J0 byte."
    REFERENCE
       "[IEEE 802.3 Std.], 30.8.1.1.9, aJ0ValueRX."
     ::= { etherWisSectionCurrentEntry 2 }


-- The Path group

-- These objects provide WIS extensions to
-- the SONET-MIB Path Group.

etherWisPathCurrentTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF EtherWisPathCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "The table for the current state of Ethernet WIS paths."
     ::= { etherWisPath 1 }

etherWisPathCurrentEntry OBJECT-TYPE
    SYNTAX  EtherWisPathCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "An entry in the etherWisPathCurrentTable.  For each
       instance of this object there MUST be a corresponding
       instance of sonetPathCurrentEntry."
    INDEX  { ifIndex }
     ::= { etherWisPathCurrentTable 1 }

EtherWisPathCurrentEntry ::=
    SEQUENCE {
        etherWisPathCurrentStatus           BITS,
        etherWisPathCurrentJ1Transmitted    OCTET STRING,
        etherWisPathCurrentJ1Received       OCTET STRING
        }









etherWisPathCurrentStatus OBJECT-TYPE
    SYNTAX  BITS {
                etherWisPathLOP(0),
                etherWisPathAIS(1),
                etherWisPathPLM(2),
                etherWisPathLCD(3)
            }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "This variable indicates the current status of the
       path payload with a bit map that can indicate multiple
       defects at once.  The bit positions are assigned as
       follows:

       etherWisPathLOP(0)
          This bit is set to indicate that an
          LOP-P (Loss of Pointer - Path) defect
          is being experienced.  Note:  when this
          bit is set, sonetPathSTSLOP MUST be set
          in the corresponding instance of
          sonetPathCurrentStatus.

       etherWisPathAIS(1)
          This bit is set to indicate that an
          AIS-P (Alarm Indication Signal - Path)
          defect is being experienced.  Note:  when
          this bit is set, sonetPathSTSAIS MUST be
          set in the corresponding instance of
          sonetPathCurrentStatus.

       etherWisPathPLM(1)
          This bit is set to indicate that a
          PLM-P (Payload Label Mismatch - Path)
          defect is being experienced.  Note:  when
          this bit is set, sonetPathSignalLabelMismatch
          MUST be set in the corresponding instance of
          sonetPathCurrentStatus.













       etherWisPathLCD(3)
          This bit is set to indicate that an
          LCD-P (Loss of Codegroup Delination - Path)
          defect is being experienced.  Since this
          defect is detected by the PCS and not by
          the path layer itself, there is no
          corresponding bit in sonetPathCurrentStatus."
    REFERENCE
       "[IEEE 802.3 Std.], 30.8.1.1.18, aPathStatus."
     ::= { etherWisPathCurrentEntry 1 }

etherWisPathCurrentJ1Transmitted OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (16))
    MAX-ACCESS  read-write
    STATUS  current
    DESCRIPTION
       "This is the 16-octet path trace message that
       is transmitted in the J1 byte.  The value SHOULD
       be '89'h followed by fifteen octets of '00'h
       (or some cyclic shift thereof) when the path
       trace function is not used, and the implementation
       SHOULD use that value (or a cyclic shift thereof)
       as a default if no other value has been set."
    REFERENCE
       "[IEEE 802.3 Std.], 30.8.1.1.23, aJ1ValueTX."
     ::= { etherWisPathCurrentEntry 2 }

etherWisPathCurrentJ1Received OBJECT-TYPE
    SYNTAX  OCTET STRING (SIZE (16))
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "This is the 16-octet path trace message that
       was most recently received in the J1 byte."
    REFERENCE
       "[IEEE 802.3 Std.], 30.8.1.1.24, aJ1ValueRX."
     ::= { etherWisPathCurrentEntry 3 }














-- The Far End Path group

-- These objects provide WIS extensions to
-- the SONET-MIB Far End Path Group.

etherWisFarEndPathCurrentTable OBJECT-TYPE
    SYNTAX  SEQUENCE OF EtherWisFarEndPathCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "The table for the current far-end state of Ethernet WIS
       paths."
     ::= { etherWisFarEndPath 1 }

etherWisFarEndPathCurrentEntry OBJECT-TYPE
    SYNTAX  EtherWisFarEndPathCurrentEntry
    MAX-ACCESS  not-accessible
    STATUS  current
    DESCRIPTION
       "An entry in the etherWisFarEndPathCurrentTable.  For each
       instance of this object there MUST be a corresponding
       instance of sonetFarEndPathCurrentEntry."
    INDEX  { ifIndex }
     ::= { etherWisFarEndPathCurrentTable 1 }

EtherWisFarEndPathCurrentEntry ::=
    SEQUENCE {
        etherWisFarEndPathCurrentStatus     BITS
        }

etherWisFarEndPathCurrentStatus OBJECT-TYPE
    SYNTAX  BITS {
                etherWisFarEndPayloadDefect(0),
                etherWisFarEndServerDefect(1)
            }
    MAX-ACCESS  read-only
    STATUS  current
    DESCRIPTION
       "This variable indicates the current status at the
       far end of the path using a bit map that can indicate
       multiple defects at once.  The bit positions are
       assigned as follows:

       etherWisFarEndPayloadDefect(0)
          A far end payload defect (i.e., far end
          PLM-P or LCD-P) is currently being signaled
          in G1 bits 5-7.




       etherWisFarEndServerDefect(1)
          A far end server defect (i.e., far end
          LOP-P or AIS-P) is currently being signaled
          in G1 bits 5-7.  Note:  when this bit is set,
          sonetPathSTSRDI MUST be set in the corresponding
          instance of sonetPathCurrentStatus."
    REFERENCE
       "[IEEE 802.3 Std.], 30.8.1.1.25, aFarEndPathStatus."
     ::= { etherWisFarEndPathCurrentEntry 1 }


--
--     Conformance Statements
--

etherWisGroups      OBJECT IDENTIFIER ::= { etherWisConformance 1 }

etherWisCompliances OBJECT IDENTIFIER ::= { etherWisConformance 2 }

--     Object Groups

etherWisDeviceGroupBasic OBJECT-GROUP
    OBJECTS {
        etherWisDeviceTxTestPatternMode,
        etherWisDeviceRxTestPatternMode
        }
    STATUS  current
    DESCRIPTION
       "A collection of objects that support test
       features required of all WIS devices."
     ::= { etherWisGroups 1 }

etherWisDeviceGroupExtra OBJECT-GROUP
    OBJECTS {
        etherWisDeviceRxTestPatternErrors
        }
    STATUS  current
    DESCRIPTION
       "A collection of objects that support
       optional WIS device test features."
     ::= { etherWisGroups 2 }










etherWisSectionGroup OBJECT-GROUP
    OBJECTS {
        etherWisSectionCurrentJ0Transmitted,
        etherWisSectionCurrentJ0Received
        }
    STATUS  current
    DESCRIPTION
       "A collection of objects that provide
       required information about a WIS section."
     ::= { etherWisGroups 3 }

etherWisPathGroup OBJECT-GROUP
    OBJECTS {
        etherWisPathCurrentStatus,
        etherWisPathCurrentJ1Transmitted,
        etherWisPathCurrentJ1Received
        }
    STATUS  current
    DESCRIPTION
       "A collection of objects that provide
       required information about a WIS path."
     ::= { etherWisGroups 4 }

etherWisFarEndPathGroup OBJECT-GROUP
    OBJECTS {
        etherWisFarEndPathCurrentStatus
        }
    STATUS  current
    DESCRIPTION
       "A collection of objects that provide required
       information about the far end of a WIS path."
     ::= { etherWisGroups 5 }

--     Compliance Statements

etherWisCompliance MODULE-COMPLIANCE
    STATUS  current
    DESCRIPTION
       "The compliance statement for interfaces that include
       the Ethernet WIS.  Compliance with the following
       external compliance statements is prerequisite:

       MIB Module             Compliance Statement
       ----------             --------------------
       IF-MIB                 ifCompliance3
       IF-INVERTED-STACK-MIB  ifInvCompliance
       EtherLike-MIB          dot3Compliance2
       MAU-MIB                mauModIfCompl3"



    MODULE  -- this module
        MANDATORY-GROUPS {
            etherWisDeviceGroupBasic,
            etherWisSectionGroup,
            etherWisPathGroup,
            etherWisFarEndPathGroup
            }

        OBJECT       etherWisDeviceTxTestPatternMode
        SYNTAX       INTEGER {
            none(1),
            squareWave(2),
            mixedFrequency(4)
            }
        DESCRIPTION
            "Support for values other than none(1),
            squareWave(2), and mixedFrequency(4)
            is not required."

        OBJECT       etherWisDeviceRxTestPatternMode
        SYNTAX       INTEGER {
            none(1),
            mixedFrequency(4)
            }
        DESCRIPTION
            "Support for values other than none(1)
            and mixedFrequency(4) is not required."

        GROUP        etherWisDeviceGroupExtra
        DESCRIPTION
            "Implementation of this group, along with support for
            the value prbs31(3) for etherWisDeviceTxTestPatternMode
            and etherWisDeviceRxTestPatternMode, is necessary if the
            optional PRBS31 test pattern mode is to be supported."

        OBJECT       etherWisDeviceRxTestPatternErrors
        WRITE-SYNTAX Gauge32 ( 0 )
        DESCRIPTION
            "An implementation is not required to
            allow values other than zero to be
            written to this object."










    MODULE SONET-MIB
        MANDATORY-GROUPS {
            sonetMediumStuff2,
            sonetSectionStuff2,
            sonetLineStuff2,
            sonetFarEndLineStuff2,
            sonetPathStuff2,
            sonetFarEndPathStuff2
            }

        OBJECT       sonetMediumType
        SYNTAX       INTEGER {
            sonet(1)
            }
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required, nor is support
            for any value other than sonet(1)."

        OBJECT       sonetMediumLineCoding
        SYNTAX       INTEGER {
            sonetMediumNRZ(4)
            }
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required, nor is support
            for any value other than sonetMediumNRZ(4)."

        OBJECT       sonetMediumLineType
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       sonetMediumCircuitIdentifier
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required."

        OBJECT       sonetMediumLoopbackConfig
        SYNTAX       BITS {
            sonetNoLoop(0),
            sonetFacilityLoop(1)
            }
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required, nor is support for values
            other than sonetNoLoop(0) and sonetFacilityLoop(1)."




        OBJECT       sonetSESthresholdSet
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required, and only one
            of the enumerated values need be supported."

        OBJECT       sonetPathCurrentWidth
        SYNTAX       INTEGER {
            sts192cSTM64(6)
            }
        MIN-ACCESS   read-only
        DESCRIPTION
            "Write access is not required, nor is support
            for any value other than sts192cSTM64(6)."

     ::= { etherWisCompliances 1 }

END
