# -*- text -*-
#
#	3GPP2 stuff.
#
#	http://www.3gpp2.org/Public_html/specs/index.cfm
#	http://www.3gpp2.org/public_html/Specs/X.S0011-005-D_v2.0_081103.pdf
#	http://www.3gpp2.org/public_html/specs/X.S0011-005-C_v3.0_061030.pdf
#		"cdma2000 Wireless IP Network Standard: Accounting Services and 3GPP2 Radius VSAs"
#		"3GPP2 X.S0011-005-D"
#		"Version: 2.0"
#		"Version Date: November 2008"
#
#	http://www.3gpp2.org/public_html/X/VSA-VSE.cfm
#
#	http://www.3gpp2.org/public_html/specs/X.S0054-910-A_v1.0_080909.pdf
#	"CAN Data Dictionary "
#		"Revision A"
#
#	$Id$
#
# [wireshark] 2009-07-08 - FreeRadius 2.6.1 dictionary.3gpp2 updated from the 3GPP2 X.S0011-005-D v2.0 spec
#
VENDOR		3GPP2				5535

BEGIN-VENDOR	3GPP2

ATTRIBUTE	3GPP2-Ike-Preshared-Secret-Request	1	integer
ATTRIBUTE	3GPP2-Security-Level			2	integer
ATTRIBUTE	3GPP2-Pre-Shared-Secret			3	string # 16 octets
ATTRIBUTE	3GPP2-Reverse-Tunnel-Spec		4	integer
ATTRIBUTE	3GPP2-Diffserv-Class-Option		5	integer

#  Contains embedded 3GPP2 accounting attributes.
ATTRIBUTE	3GPP2-Accounting-Container		6	octets
ATTRIBUTE	3GPP2-Home-Agent-IP-Address		7	octets ## if 4 octets: ipaddr; if 16: ipv6 address 

# A number formed from the concatenation of the home RADIUS IP address,
# the FA IP address, and a 32-bit Unix timestamp, all encoded as 8 ASCII
#  hex characters.
ATTRIBUTE	3GPP2-KeyID						8	string # 20 octets

ATTRIBUTE	3GPP2-PCF-IP-Address			9	ipaddr
ATTRIBUTE	3GPP2-BSID						10	string
ATTRIBUTE	3GPP2-User-Id					11	integer
ATTRIBUTE	3GPP2-Forward-FCH-Mux-Option	12	integer
ATTRIBUTE	3GPP2-Reverse-FCH-Mux-Option	13	integer
#
# 14-15 ?
#
ATTRIBUTE	3GPP2-Service-Option			16	integer
ATTRIBUTE	3GPP2-Forward-Traffic-Type		17	integer
ATTRIBUTE	3GPP2-Reverse-Traffic-Type		18	integer
ATTRIBUTE	3GPP2-FCH-Frame-Size			19	integer
ATTRIBUTE	3GPP2-Forward-FCH-RC			20	integer
ATTRIBUTE	3GPP2-Reverse-FCH-RC			21	integer
ATTRIBUTE	3GPP2-IP-Technology				22	integer
ATTRIBUTE	3GPP2-Compulsory-Tunnel-Indicator	23	integer
ATTRIBUTE	3GPP2-Release-Indicator			24	integer
ATTRIBUTE	3GPP2-Bad-PPP-Frame-Count		25	integer
#
# 26-29 ?
#
ATTRIBUTE	3GPP2-Number-Active-Transitions		30	integer
ATTRIBUTE	3GPP2-Terminating-SDB-Octet-Count	31	integer
ATTRIBUTE	3GPP2-Originating-SDB-OCtet-Count	32	integer
ATTRIBUTE	3GPP2-Terminating-Number-SDBs		33	integer
ATTRIBUTE	3GPP2-Originating-Number-SDBs		34	integer
# 35 ?
ATTRIBUTE	3GPP2-IP-QoS						36	integer
# 37-38 ?
ATTRIBUTE	3GPP2-Airlink-Priority				39	integer
ATTRIBUTE	3GPP2-Airlink-Record-Type			40	integer
ATTRIBUTE	3GPP2-R-P-Session-ID				41	octets
ATTRIBUTE	3GPP2-Airlink-Sequence-Number		42	integer
ATTRIBUTE	3GPP2-Received-HDLC-Octets			43	integer
ATTRIBUTE	3GPP2-Correlation-Id				44	string
ATTRIBUTE	3GPP2-Module-Orig-Term-Indicator	45	integer
ATTRIBUTE	3GPP2-Inbound-Mobile-IP-Sig-Octets	46	integer
ATTRIBUTE	3GPP2-Outbound-Mobile-IP-Sig-Octets	47	integer
ATTRIBUTE	3GPP2-Session-Continue				48	integer
ATTRIBUTE	3GPP2-Active-Time					49	integer
ATTRIBUTE	3GPP2-DCCH-Frame-Size				50	integer
ATTRIBUTE	3GPP2-Begin-Session					51	integer
ATTRIBUTE	3GPP2-ESN							52	string
# 53 ?
ATTRIBUTE	3GPP2-S-Key							54	octets
ATTRIBUTE	3GPP2-S-Request						55	integer
ATTRIBUTE	3GPP2-S-Lifetime					56	date
ATTRIBUTE	3GPP2-MN-HA-SPI						57	integer
ATTRIBUTE	3GPP2-MN-HA-Shared-Key				58	string encrypt=2

# The next set of attributes contain sub-types
ATTRIBUTE	3GPP2-Remote-IP-Address				59	octets

ATTRIBUTE	3GPP2-HRPD-Access/Terminal-Authentication-and-1x-Access-Authorization 60 integer
ATTRIBUTE	3GPP2-AT-Hardware-Identifier		61	integer
BEGIN-TLV
	ATTRIBUTE	AT-hardware-identifier-type		1	string
	ATTRIBUTE	AT-hardware-identifier-value	2	string
END-TLV

# 62 - 69 are marked "reserved"

ATTRIBUTE	3GPP2-Remote-IPv6-Address				70	octets
ATTRIBUTE	3GPP2-Remote-Address-Table-Index		71	octets
ATTRIBUTE	3GPP2-Remote-IPv4-Addr-Octet-Count		72	octets
ATTRIBUTE	3GPP2-Allowed-Diffserv-Marking			73	tlv
BEGIN-TLV 3GPP2-Allowed-Diffserv-Marking
	ATTRIBUTE	flags-for-Allowed-Diffserv-class	1	string
	ATTRIBUTE	Max-class-selection-marking			2	string
	ATTRIBUTE	Reverse-tunnel-marking				3	string
END-TLV 3GPP2-Allowed-Diffserv-Marking
#contains subtypes
ATTRIBUTE	3GPP2-Service-Option-Profile			74	tlv
BEGIN-TLV 3GPP2-Service-Option-Profile
	ATTRIBUTE	service-option						1	integer
END-TLV 3GPP2-Service-Option-Profile

# the following don't contain subtypes
ATTRIBUTE	3GPP2-DNS-Update-Required				75	integer
# 76 ?
# 77 ?
ATTRIBUTE	3GPP2-Always-On							78	integer
ATTRIBUTE	3GPP2-Foreign-Agent-Address				79	ipaddr
ATTRIBUTE	3GPP2-Last-User-Activity-Time			80	integer
ATTRIBUTE	3GPP2-MN-AAA-Removal-Indication			81	integer
ATTRIBUTE	3GPP2-RN-Packet-Data-Inactivity-Timer	82	integer
ATTRIBUTE	3GPP2-Forward-PDCH-RC					83	integer
ATTRIBUTE	3GPP2-Forward-DCCH-Mux-Option			84	integer
ATTRIBUTE	3GPP2-Reverse-DCCH-Mux-Option			85	integer
ATTRIBUTE	3GPP2-Forward-DCCH-RC					86	integer
ATTRIBUTE	3GPP2-Reverse-DHHC-RC					87	integer
ATTRIBUTE	3GPP2-Session-Termination-Capability	88	integer
ATTRIBUTE	3GPP2-Allowed-Persistent-TFTs			89	integer

# The next set of attributes contain sub-types
ATTRIBUTE	3GPP2-Prepaid-Acct-Quota				90	tlv
BEGIN-TLV 3GPP2-Prepaid-Acct-Quota
	ATTRIBUTE	QID									1	integer
	ATTRIBUTE	VolumeQuota							2	integer
	ATTRIBUTE	VolumeQuotaOverflow					3	m2integer
	ATTRIBUTE	VolumeThreshold						4	integer
	ATTRIBUTE	VolumeThreshouldOverflow			5	integer
	ATTRIBUTE	DurationQuota						6	integer
	ATTRIBUTE	DurationThreshold					7	integer
	ATTRIBUTE	Update-Reason						8	integer
END-TLV 3GPP2-Prepaid-Acct-Quota

#contains sub-types
ATTRIBUTE	3GPP2-Prepaid-acct-Capability			91	tlv
BEGIN-TLV 3GPP2-Prepaid-acct-Capability
	ATTRIBUTE	AvailableInClient					1	integer
	ATTRIBUTE	SelectedForSession					2	integer
END-TLV 3GPP2-Prepaid-acct-Capability
ATTRIBUTE	3GPP2-MIP-Lifetime						92	octets

ATTRIBUTE	3GPP2-Acct-Stop-Trigger					93	integer

# contains subtypes
ATTRIBUTE	3GPP2-Service-Reference-Id				94	octets

ATTRIBUTE	3GPP2-DNS-Update-Capability				95	integer
ATTRIBUTE	3GPP2-Disconnect-Reason					96	integer

# The next set of attributes contain sub-types
ATTRIBUTE	3GPP2-Remote-IPv6-Octet-Count			97	octets
#contains sub-types
ATTRIBUTE	3GPP2-PrePaid-Tariff-Switching			98	tlv
BEGIN-TLV 3GPP2-PrePaid-Tariff-Switching
	ATTRIBUTE	QuotaIDentifier						1	integer
	ATTRIBUTE	VolumeUsedAfterTariffSwitch			2	integer
	ATTRIBUTE	VolumeUsedATSOverflow				3	integer
	ATTRIBUTE	TariffSwitchInterval				4	integer
	ATTRIBUTE	TimeIntervalafterTariffSwitchUpdate	5	integer
END-TLV 3GPP2-PrePaid-Tariff-Switching
#contain sub-types
ATTRIBUTE	3GPP2-Authorization-Parameters			99	tlv
BEGIN-TLV 3GPP2-Authorization-Parameters
	ATTRIBUTE	BAK-Identifier						1	integer
	ATTRIBUTE	Timestamp-long						2	integer
	ATTRIBUTE	Authorization-Signature				3	string
END-TLV 3GPP2-Authorization-Parameters


ATTRIBUTE	3GPP2-BCMCS_FLOW_ID						100	bytes

#contain sub-types
ATTRIBUTE	3GPP2-BCMCS-Capability					101	tlv
BEGIN-TLV 3GPP2-BCMCS-Capability
	ATTRIBUTE	Protocol-Revision					1	integer
END-TLV 3GPP2-BCMCS-Capability

#contain sub-types
ATTRIBUTE	3GPP2-Common-Session-Info				102	tlv
BEGIN-TLV 3GPP2-Common-Session-Info
	ATTRIBUTE	BCMCS_FLOW_ID						1	bytes
	ATTRIBUTE	Program-Start-Time					2	date
	ATTRIBUTE	Program-End-Time					3	date
	ATTRIBUTE	Program-Allowed-Registration-Time(seconds)	4	integer
	ATTRIBUTE	Authorization-Required-Flag			5	string
	ATTRIBUTE	QoS-Parameter						6	integer #??
	ATTRIBUTE	BCMCS_Flow_Priority					7	integer
END-TLV 3GPP2-Common-Session-Info

#contain sub-types
ATTRIBUTE	BSN-Session-Info						103	tlv
BEGIN-TLV BSN-Session-Info
	ATTRIBUTE	BCMCS_FLOW_ID						1	bytes
	ATTRIBUTE	Multicast-IP-Address				2	ipaddr
	ATTRIBUTE	Destination-Port-Number				3	integer
	ATTRIBUTE	Header-Compression-Algorithm		4	string
	ATTRIBUTE	CID									5	string
	ATTRIBUTE	MAX-CID								6	integer
	ATTRIBUTE	Compression-Profile					7	integer
	ATTRIBUTE	MAX-Header-Size						8	integer
	ATTRIBUTE	MRRU								9	integer
	ATTRIBUTE	Content-Server-Source-IP-Address	10	ipaddr
	ATTRIBUTE	Content-Server-Source-IPv6-Address	11	ipv6addr
END-TLV BSN-Session-Info

#contain sub-types
ATTRIBUTE	RAN-Session-Info							104	tlv
BEGIN-TLV RAN-Session-Info
	ATTRIBUTE	BCMCS_FLOW_ID						1	integer
	ATTRIBUTE	Encryption-Mechanism				2	integer
	ATTRIBUTE	BAK-Identifier						3	integer
	ATTRIBUTE	BAK									4	string
	ATTRIBUTE	BAK-Expire-Time						5	string
	ATTRIBUTE	Session-Bandwidth					6	integer
END-TLV RAN-Session-Info
	
ATTRIBUTE	Reason-Code								105	integer
ATTRIBUTE	3GPP2-BCMCS-Flow-Transmission-Time		107	date

#contain sub-types
ATTRIBUTE	3GPP2-Subnet							108	tlv
BEGIN-TLV 3GPP2-Subnet
	ATTRIBUTE	Subnet								1	bytes
	ATTRIBUTE	Sector-ID							2	bytes
END-TLV 3GPP2-Subnet
ATTRIBUTE	3GPP2-Multicast-IP-Address				109	ipaddr
ATTRIBUTE	3GPP2-Port								110	integer

#contain sub-typess
ATTRIBUTE	3GPP2-TK-Info							112	tlv
BEGIN-TLV 3GPP2-TK-Info
	ATTRIBUTE	TK									1	integer
	ATTRIBUTE	TK_RAND								2	integer
END-TLV 3GPP2-TK-Info
#contain sub-types
ATTRIBUTE	3GPP2-BAK-ID							113	tlv
BEGIN-TLV 3GPP2-BAK-ID
	ATTRIBUTE	BAK_ID								1	integer
	ATTRIBUTE	BAK_Expire							2	integer
END-TLV 3GPP2-BAK-ID

ATTRIBUTE	3GPP2-Reverse-PDCH-RC					114	integer
ATTRIBUTE	3GPP2-MEID								116	string
#contain sub-types
ATTRIBUTE	3GPP2-DNS-Server-IP-Address				117	tlv
BEGIN-TLV 3GPP2-DNS-Server-IP-Address
	ATTRIBUTE	Primary-DNS-Server					1	ipaddr
	ATTRIBUTE	Secondary-DNS-Server				2	ipaddr
	ATTRIBUTE	Flag								3	integer
	ATTRIBUTE	Entity-Type							4	integer
END-TLV 3GPP2-DNS-Server-IP-Address

ATTRIBUTE	3GPP2-MIP6-Home-Agent-Address-From-BU	118	ipv6addr
ATTRIBUTE	3GPP2-MIP6-Care-of-Address				119	ipv6addr
ATTRIBUTE	3GPP2-Home-Agent-Not-Authorized			120	integer
ATTRIBUTE	3GPP2-MIP6-Session-Key					121	octets
ATTRIBUTE	3GPP2-Hot-Line-Accounting-Information	122	string
ATTRIBUTE	3GPP2-MIP6-Mesg-ID						123	octets
ATTRIBUTE	3GPP2-Filter-Rule						124	string
ATTRIBUTE	3GPP2-HTTP-Redirection-Rule				125	string
ATTRIBUTE	3GPP2-IP-Redirection-Rule				126	string
ATTRIBUTE	3GPP2-Hot-Line-Capability				127	integer
ATTRIBUTE	3GPP2-MIP6-Home-Link-Prefix-Attr-A		128	octets

ATTRIBUTE	3GPP2-Max-Authorized-Aggr-Bandwidth		130	integer

# The next set of attributes contain sub-types
ATTRIBUTE	3GPP2-Authorized-Flow-Profile-IDs		131	tlv
BEGIN-TLV 3GPP2-Authorized-Flow-Profile-IDs
	ATTRIBUTE	ProfileID_Forward					1	string
	ATTRIBUTE	ProfileID_Reverse					2	string
	ATTRIBUTE	ProfileID_Bi-direction				3	string
END-TLV 3GPP2-Authorized-Flow-Profile-IDs

ATTRIBUTE	3GPP2-Granted-QoS-Parameters			132	tlv
BEGIN-TLV 3GPP2-Granted-QoS-Parameters
	ATTRIBUTE	Direction							1	integer
	ATTRIBUTE	FLOW_ID								2	integer
	ATTRIBUTE	QoS_ATTRIBUTE_SET_ID				3	integer
	ATTRIBUTE	FlowProfileID						4	integer
	ATTRIBUTE	Traffic_Class						5	string
	ATTRIBUTE	Peak_Rate							6	string
	ATTRIBUTE	Bucket_Size							7	string
	ATTRIBUTE	Token_Rate							8	string
	ATTRIBUTE	Max_Latency							9	string
	ATTRIBUTE	Max_IP_Packet_Loss_Rate				10	string
	ATTRIBUTE	Packet_Size							11	string
	ATTRIBUTE	Delay_Var_Sensitive					12	string
END-TLV 3GPP2-Granted-QoS-Parameters

ATTRIBUTE	3GPP2-Maximum-Per-Flow-Priority			133	integer
ATTRIBUTE	3GPP2-MIP6-Authenticator				134	octets

ATTRIBUTE	3GPP2-MIP6-MAC-Mobility-Data			138	octets
ATTRIBUTE	3GPP2-Inter-User-Priority				139	integer
ATTRIBUTE	3GPP2-MIP6-Home-Agent-Address-Attr-B	140	ipv6addr
ATTRIBUTE	3GPP2-MIP6-HOA-Received-From-BU			141	ipv6addr
ATTRIBUTE	3GPP2-Carrier-ID						142	octets
ATTRIBUTE	3GPP2-GMT-Time-Zone-Offset				143	integer

# contains subtypes
ATTRIBUTE	3GPP2-Flow-ID-Parameter					144	octets

ATTRIBUTE	3GPP2-Flow-Status						145	integer
ATTRIBUTE	3GPP2-Filtered-Octet-Count-Terminating	146	integer
ATTRIBUTE	3GPP2-Filtered-Octet-Count-Originating	147	integer

ATTRIBUTE	3GPP2-RSVP-Inbound-Octet-Count			162	integer
ATTRIBUTE	3GPP2-RSVP-Outbound-Octet-Count			163	integer
ATTRIBUTE	3GPP2-RSVP-Inbound-Packet-Count			164	integer
ATTRIBUTE	3GPP2-RSVP-Outbound-Packet-Count		165	integer

ATTRIBUTE	3GPP2-HA-Request						168	integer
ATTRIBUTE	3GPP2-HA-Authorised						169	integer
ATTRIBUTE	3GPP2-IP-Ver-Authorised					172	integer
ATTRIBUTE	3GPP2-MIPv4-Mesg-Id						173	string

ATTRIBUTE	3GPP2-MIP6-HA-Local-Assignment-Capblty	179	integer

ATTRIBUTE	3GPP2-Network-PMIP-NAI					192	string
ATTRIBUTE	3GPP2-PMIP-Based-Mobility-Capability	193	integer
ATTRIBUTE	3GPP2-Accounting-Mode					198	integer ## ??

ATTRIBUTE	3GPP2-HAAA-MIP6-HA-Protocol-Capblty-Ind	203	integer

ATTRIBUTE	3GPP2-VAAA-Assigned-MIP6-HA				205	ipv6addr
ATTRIBUTE	3GPP2-VAAA-Assigned-MIP6-HL				206	octets
ATTRIBUTE	3GPP2-VAAA-MIP6-HA-Protocol-Capblty-Ind	207	integer

ATTRIBUTE	3GPP2-DNS-Server-IPV6-Address			214	tlv
BEGIN-TLV 3GPP2-DNS-Server-IPV6-Address
	ATTRIBUTE	Primary-DNS-Server-IPV6-ADDRESS		1	ipv6addr
	ATTRIBUTE	Secondary-DNS-Server-IPV6-ADDRESS	2	ipv6addr
	ATTRIBUTE	Flag								3	string
	ATTRIBUTE	Entity-Type							4	string
END-TLV 3GPP2-DNS-Server-IPV6-Address

VALUE	3GPP2-Airlink-Record-Type	Connection-Setup	1
VALUE	3GPP2-Airlink-Record-Type	Active-Start		2
VALUE	3GPP2-Airlink-Record-Type	Active-Stop			3
VALUE	3GPP2-Airlink-Record-Type	Short-Data-Burst	4

VALUE	Authorization-Required-Flag	Authorization-is-not-required-for-this-flow				0
VALUE	Authorization-Required-Flag	Authorization-is-required-for-this-flow					1

VALUE	Reason-Code	Reserved																0
VALUE	Reason-Code	Authorization-Only														1
VALUE	Reason-Code	Session-Discovery-Only													2
VALUE	Reason-Code	Authorization-and-Session-Discovery										3


VALUE	Header-Compression-Algorithm	No-Header-Compression								0
VALUE	Header-Compression-Algorithm	ROHC-U-mode											1

VALUE	CID	Small-CID																		0
VALUE	CID	Large-CID																		1

VALUE	Encryption-Mechanism	High-layer-encryption-in-the-Content-Server					0
VALUE	Encryption-Mechanism	Link-layer-encryption-in-the-RAN							1

VALUE	3GPP2-PMIP-Based-Mobility-Capability	AGW-supports-the-Network-PMIP4-only			1
VALUE	3GPP2-PMIP-Based-Mobility-Capability	AGW-supports-the-Network-PMIP6-only			2
VALUE	3GPP2-PMIP-Based-Mobility-Capability	AGW-supports-the-both-Network-PMIP4-and-PMIP6	3

VALUE	Update-Reason	Pre-initializatio													1
VALUE	Update-Reason	Initial-request														2
VALUE	Update-Reason	Threshold-reached													3
VALUE	Update-Reason	Quota-reached														4
VALUE	Update-Reason	Remote-Forced-disconnect											5
VALUE	Update-Reason	Client-Service-termination											6
VALUE	Update-Reason	Main-SI-released													7
VALUE	Update-Reason	Service-Instance-not-established									8
VALUE	Update-Reason	Tariff-Switch-Update												9

VALUE	AvailableInClient	PrePaid-Accounting-for-Volume-supported							1
VALUE	AvailableInClient	PrePaid-Accounting-for-Duration-supported						2
VALUE	AvailableInClient	PrePaid-Accounting-for-Volume-and-Duration-supported			3

VALUE	SelectedForSession	PrePaid	Accounting	not	used									0
VALUE	SelectedForSession	Usage-of-PrePaid-Accounting-for-Volume							1
VALUE	SelectedForSession	Usage-of-PrePaid-Accounting-for-Duration						2
VALUE	SelectedForSession	Usage-of-PrePaid-Accounting-for-Volume-and-Duration				3

VALUE	Flag	DNS-IP-Addresses-Provided-By-HAAA-Forcibly									1
VALUE	Flag	DNS-IP-Addresses-Provided-By-HAAA-Unobtrusively								0

VALUE	Entity-Type		HAAA	1
VALUE	Entity-Type		VAAA	2

END-VENDOR 3GPP2
