# -*- text -*-
#
# Ericsson-AB dictionary.
#
# Version:	1.00  14-Sep-2000  Chris Adams <cmadams@hiwaay.net>
#		1.10  26-Oct-2014  Anish Bhatt <anish@chelsio.com>
#		$Id$
#

VENDOR		Ericsson-AB				2352

#
#	Ericsson-AB Vendor Specific Extensions
#
#	The first set here uses '_' as the separator, as Ericsson-AB has changed
#	their documentation to use '-' vs. '_'.  The older '_' style entries
#	are listed first so that they will still be accepted,
#	yet not preferred.
#
#
#	Ericsson-AB Vendor Specific Extensions  ( older style syntax )
#
#	The names use underscores (_) instead of dashes (-), because
#	that's what Ericsson-AB used in their older documentation and examples.
#
BEGIN-VENDOR	Ericsson-AB

ATTRIBUTE	Client_DNS_Pri				1	ipaddr
ATTRIBUTE	Client_DNS_Sec				2	ipaddr
ATTRIBUTE	DHCP_Max_Leases				3	integer
ATTRIBUTE	Context_Name				4	string
ATTRIBUTE	Bridge_Group				5	string
ATTRIBUTE	BG_Aging_Time				6	string
ATTRIBUTE	BG_Path_Cost				7	string
ATTRIBUTE	BG_Span_Dis				8	string
ATTRIBUTE	BG_Trans_BPDU				9	string
ATTRIBUTE	Rate_Limit_Rate				10	integer
ATTRIBUTE	Rate_Limit_Burst			11	integer
ATTRIBUTE	Police_Rate				12	integer
ATTRIBUTE	Police_Burst				13	integer
ATTRIBUTE	Source_Validation			14	integer
ATTRIBUTE	Tunnel_Domain				15	integer
ATTRIBUTE	Tunnel_Local_Name			16	string
ATTRIBUTE	Tunnel_Remote_Name			17	string
ATTRIBUTE	Tunnel_Function				18	integer
ATTRIBUTE	Tunnel-Flow-Control			19	integer
ATTRIBUTE	Tunnel-Static				20	integer
ATTRIBUTE	Tunnel_Max_Sessions			21	integer
ATTRIBUTE	Tunnel_Max_Tunnels			22	integer
ATTRIBUTE	Tunnel_Session_Auth			23	integer
ATTRIBUTE	Tunnel_Window				24	integer
ATTRIBUTE	Tunnel_Retransmit			25	integer
ATTRIBUTE	Tunnel_Cmd_Timeout			26	integer
ATTRIBUTE	PPPOE_URL				27	string
ATTRIBUTE	PPPOE_MOTM				28	string
ATTRIBUTE	Tunnel_Group				29	integer
ATTRIBUTE	Tunnel_Context				30	string
ATTRIBUTE	Tunnel_Algorithm			31	integer
ATTRIBUTE	Tunnel_Deadtime				32	integer
ATTRIBUTE	Mcast_Send				33	integer
ATTRIBUTE	Mcast_Receive				34	integer
ATTRIBUTE	Mcast_MaxGroups				35	integer
ATTRIBUTE	Ip_Address_Pool_Name			36	string
ATTRIBUTE	Tunnel_DNIS				37	integer
ATTRIBUTE	Medium_Type				38	integer
ATTRIBUTE	PVC_Encapsulation_Type			39	integer
ATTRIBUTE	PVC_Profile_Name			40	string
ATTRIBUTE	PVC_Circuit_Padding			41	integer
ATTRIBUTE	Bind_Type				42	integer
ATTRIBUTE	Bind_Auth_Protocol			43	integer
ATTRIBUTE	Bind_Auth_Max_Sessions			44	integer
ATTRIBUTE	Bind_Bypass_Bypass			45	string
ATTRIBUTE	Bind_Auth_Context			46	string
ATTRIBUTE	Bind_Auth_Service_Grp			47	string
ATTRIBUTE	Bind_Bypass_Context			48	string
ATTRIBUTE	Bind_Int_Context			49	string
ATTRIBUTE	Bind_Tun_Context			50	string
ATTRIBUTE	Bind_Ses_Context			51	string
ATTRIBUTE	Bind_Dot1q_Slot				52	integer
ATTRIBUTE	Bind_Dot1q_Port				53	integer
ATTRIBUTE	Bind_Dot1q_Vlan_Tag_Id			54	integer
ATTRIBUTE	Bind_Int_Interface_Name			55	string
ATTRIBUTE	Bind_L2TP_Tunnel_Name			56	string
ATTRIBUTE	Bind_L2TP_Flow_Control			57	integer
ATTRIBUTE	Bind_Sub_User_At_Context		58	string
ATTRIBUTE	Bind_Sub_Password			59	string
ATTRIBUTE	Ip_Host_Addr				60	string
ATTRIBUTE	IP_TOS_Field				61	integer
ATTRIBUTE	NAS_Real_Port				62	integer
ATTRIBUTE	Tunnel_Session_Auth_Ctx			63	string
ATTRIBUTE	Tunnel_Session_Auth_Service_Grp		64	string
ATTRIBUTE	Tunnel_Rate_Limit_Rate			65	integer
ATTRIBUTE	Tunnel_Rate_Limit_Burst			66	integer
ATTRIBUTE	Tunnel_Police_Rate			67	integer
ATTRIBUTE	Tunnel_Police_Burst			68	integer
ATTRIBUTE	Tunnel_L2F_Second_Password		69	string
ATTRIBUTE	ACL-Definition				70	string
ATTRIBUTE	PPPoE-IP-Route-Add			71	string
ATTRIBUTE	TTY_Level_Max				72	integer
ATTRIBUTE	TTY_Level_Start				73	integer
ATTRIBUTE	Bind-DHCP-Context			76	string
ATTRIBUTE	Tunnel-Mobil-Group			77	string
ATTRIBUTE	Tunnel-Client-VPN			78	string
ATTRIBUTE	Tunnel-Server-VPN			79	string
ATTRIBUTE	PPP-Compression				84	integer
ATTRIBUTE	Tunnel-Hello-Timer			85	integer
ATTRIBUTE	Redback-Reason				86	integer
ATTRIBUTE	Qos-Policy-Policing			87	string
ATTRIBUTE	Qos-Policy-Metering			88	string
ATTRIBUTE	Qos-Policy-Queuing			89	string
ATTRIBUTE	Igmp-Service-Profile			90	string
ATTRIBUTE	Sub-Profile-Name			91	string
ATTRIBUTE	Forward-Policy				92	string
ATTRIBUTE	Remote-Port				93	string
ATTRIBUTE	Reauth-String				94	string
ATTRIBUTE	Reauth-More				95	integer

#
#  These next 2 seem to be copies of the DHCP options...
#
ATTRIBUTE	Agent-Remote-Id				96	octets
ATTRIBUTE	Agent-Circuit-Id			97	octets
ATTRIBUTE	Platform-Type				98	integer
ATTRIBUTE	RB-Client-NBNS-Pri			99	ipaddr
ATTRIBUTE	RB-Client-NBNS-Sec			100	ipaddr
ATTRIBUTE	Shaping-Profile-Name			101	string
ATTRIBUTE	Bridge-Profile				103	string
ATTRIBUTE	IP-Interface				104	string
ATTRIBUTE	NAT-Policy-Name				105	string
ATTRIBUTE	RB-NPM-Service-Id			106	string
ATTRIBUTE	HTTP-Redirect-Profile-Name		107	string
ATTRIBUTE	Bind-Auto-Sub-User			108	string
ATTRIBUTE	Bind-Auto-Sub-Context			109	string
ATTRIBUTE	Bind-Auto-Sub-Password			110	string
ATTRIBUTE	Circuit-Protocol-Encap			111	integer
ATTRIBUTE	OS-Version				112	string
ATTRIBUTE	Session-Traffic-Limit			113	string
ATTRIBUTE	QOS-Reference				114	string
ATTRIBUTE	DHCP-Vendor-Class-ID			125	string
ATTRIBUTE	Qos-Rate				126	string
ATTRIBUTE	DHCP-Vendor-Encap-Option		127	string
ATTRIBUTE	Acct_Input_Octets_64			128	octets
ATTRIBUTE	Acct_Output_Octets_64			129	octets
ATTRIBUTE	Acct_Input_Packets_64			130	octets
ATTRIBUTE	Acct_Output_Packets_64			131	octets
ATTRIBUTE	Assigned_IP_Address			132	ipaddr
ATTRIBUTE	Acct_Mcast_In_Octets			133	integer
ATTRIBUTE	Acct_Mcast_Out_Octets			134	integer
ATTRIBUTE	Acct_Mcast_In_Packets			135	integer
ATTRIBUTE	Acct_Mcast_Out_Packets			136	integer
ATTRIBUTE	LAC_Port				137	integer
ATTRIBUTE	LAC_Real_Port				138	integer
ATTRIBUTE	LAC_Port_Type				139	integer
ATTRIBUTE	LAC_Real_Port_Type			140	integer
ATTRIBUTE	Acct_Dyn_Ac_Ent				141	string
ATTRIBUTE	Session_Error_Code			142	integer
ATTRIBUTE	Session_Error_Msg			143	string

VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_RAW	1
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_ROUTE1483 2
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_AUTO1483	3
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_MULTI	4
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_BRIDGE1483 5
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_PPP	6
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_PPP_SERIAL 7
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_PPP_NLPID 8
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_PPP_AUTO	9
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_PPPOE	10
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_L2TP	11
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ATM_PPP_LLC	12
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_AUTO1490 13
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_MULTI	14
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_BRIDGE1490 15
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_PPP	16
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_PPP_AUTO 17
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_PPPOE	18
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_ROUTE1490 19
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_FRAME_L2TP	20
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_L2TP_VC_MUXED 21
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ETH		22
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ETH_PPPOE	23
VALUE	PVC_Encapsulation_Type		AAA_ENCAPS_ETH_MULTI	24
VALUE	PVC_Circuit_Padding		AAA_CIRCUIT_PADDING	1
VALUE	PVC_Circuit_Padding		AAA_CIRCUIT_NO_PADDING	2
VALUE	Bind_Type			AAA_AUTH_BIND		1
VALUE	Bind_Type			AAA_BYPASS_BIND		2
VALUE	Bind_Type			AAA_INTERFACE_BIND	3
VALUE	Bind_Type			AAA_SUBSCRIBE_BIND	4
VALUE	Bind_Type			AAA_TUNNEL_BIND		5
VALUE	Bind_Type			AAA_SESSION_BIND	6
VALUE	Bind_Type			AAA_Q8021_BIND		7
VALUE	Bind_Type			AAA_MULTI_BIND		8
VALUE	Bind_Auth_Protocol		AAA_PPP_PAP		1
VALUE	Bind_Auth_Protocol		AAA_PPP_CHAP		2
VALUE	Bind_Auth_Protocol		AAA_PPP_CHAP_WAIT	3
VALUE	Bind_Auth_Protocol		AAA_PPP_CHAP_PAP	4
VALUE	Bind_Auth_Protocol		AAA_PPP_CHAP_WAIT_PAP	5

VALUE	Tunnel_Function			LAC-Only		1
VALUE	Tunnel_Function			LNS-Only		2
VALUE	Tunnel_Function			LAC-LNS			3
VALUE	Tunnel_Session_Auth		CHAP			1
VALUE	Tunnel_Session_Auth		PAP			2
VALUE	Tunnel_Session_Auth		CHAP-PAP		3
VALUE	Mcast_Send			NO-SEND			1
VALUE	Mcast_Send			SEND			2
VALUE	Mcast_Send			UNSOLICITED-SEND	3
VALUE	Mcast_Receive			NO-RECEIVE		1
VALUE	Mcast_Receive			RECEIVE			2

VALUE	Tunnel_DNIS			DNIS			1
VALUE	Tunnel_DNIS			DNIS-Only		2

VALUE	LAC_Port_Type			NAS_PORT_TYPE_10BT	40
VALUE	LAC_Port_Type			NAS_PORT_TYPE_100BT	41
VALUE	LAC_Port_Type			NAS_PORT_TYPE_DS3_FR	42
VALUE	LAC_Port_Type			NAS_PORT_TYPE_DS3_ATM	43
VALUE	LAC_Port_Type			NAS_PORT_TYPE_OC3	44
VALUE	LAC_Port_Type			NAS_PORT_TYPE_HSSI	45
VALUE	LAC_Port_Type			NAS_PORT_TYPE_EIA530	46
VALUE	LAC_Port_Type			NAS_PORT_TYPE_T1	47
VALUE	LAC_Port_Type			NAS_PORT_TYPE_CHAN_T3	48
VALUE	LAC_Port_Type			NAS_PORT_TYPE_DS1_FR	49
VALUE	LAC_Port_Type			NAS_PORT_TYPE_E3_ATM	50
VALUE	LAC_Port_Type			NAS_PORT_TYPE_IMA_ATM	51
VALUE	LAC_Port_Type			NAS_PORT_TYPE_DS3_ATM_2	52
VALUE	LAC_Port_Type			NAS_PORT_TYPE_OC3_ATM_2	53
VALUE	LAC_Port_Type			NAS_PORT_TYPE_1000BSX	54
VALUE	LAC_Port_Type			NAS_PORT_TYPE_E1_FR	55
VALUE	LAC_Port_Type			NAS_PORT_TYPE_E1_ATM	56
VALUE	LAC_Port_Type			NAS_PORT_TYPE_E3_FR	57
VALUE	LAC_Port_Type			NAS_PORT_TYPE_OC3_POS	58
VALUE	LAC_Port_Type			NAS_PORT_TYPE_OC12_POS	59
VALUE	LAC_Port_Type			NAS_PORT_TYPE_PPPOE	60
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_10BT	40
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_100BT	41
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_DS3_FR	42
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_DS3_ATM	43
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_OC3	44
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_HSSI	45
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_EIA530	46
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_T1	47
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_CHAN_T3	48
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_DS1_FR	49
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_E3_ATM	50
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_IMA_ATM	51
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_DS3_ATM_2	52
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_OC3_ATM_2	53
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_1000BSX	54
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_E1_FR	55
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_E1_ATM	56
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_E3_FR	57
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_OC3_POS	58
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_OC12_POS	59
VALUE	LAC_Real_Port_Type		NAS_PORT_TYPE_PPPOE	60

#
#	New names.
#
ATTRIBUTE	Client-DNS-Pri				1	ipaddr
ATTRIBUTE	Client-DNS-Sec				2	ipaddr
ATTRIBUTE	DHCP-Max-Leases				3	integer
ATTRIBUTE	Context-Name				4	string
ATTRIBUTE	Bridge-Group				5	string
ATTRIBUTE	BG-Aging-Time				6	string
ATTRIBUTE	BG-Path-Cost				7	string
ATTRIBUTE	BG-Span-Dis				8	string
ATTRIBUTE	BG-Trans-BPDU				9	string
ATTRIBUTE	Rate-Limit-Rate				10	integer
ATTRIBUTE	Rate-Limit-Burst			11	integer
ATTRIBUTE	Police-Rate				12	integer
ATTRIBUTE	Police-Burst				13	integer
ATTRIBUTE	Source-Validation			14	integer
ATTRIBUTE	Tunnel-Domain				15	integer
ATTRIBUTE	Tunnel-Local-Name			16	string
ATTRIBUTE	Tunnel-Remote-Name			17	string
ATTRIBUTE	Tunnel-Function				18	integer
ATTRIBUTE	Tunnel-Flow-Control			19	integer
ATTRIBUTE	Tunnel-Static				20	integer
ATTRIBUTE	Tunnel-Max-Sessions			21	integer
ATTRIBUTE	Tunnel-Max-Tunnels			22	integer
ATTRIBUTE	Tunnel-Session-Auth			23	integer
ATTRIBUTE	Tunnel-Window				24	integer
ATTRIBUTE	Tunnel-Retransmit			25	integer
ATTRIBUTE	Tunnel-Cmd-Timeout			26	integer
ATTRIBUTE	PPPOE-URL				27	string
ATTRIBUTE	PPPOE-MOTM				28	string
ATTRIBUTE	Tunnel-Group				29	integer
ATTRIBUTE	Tunnel-Context				30	string
ATTRIBUTE	Tunnel-Algorithm			31	integer
ATTRIBUTE	Tunnel-Deadtime				32	integer
ATTRIBUTE	Mcast-Send				33	integer
ATTRIBUTE	Mcast-Receive				34	integer
ATTRIBUTE	Mcast-MaxGroups				35	integer
ATTRIBUTE	Ip-Address-Pool-Name			36	string
ATTRIBUTE	Tunnel-DNIS				37	integer
ATTRIBUTE	Medium-Type				38	integer
ATTRIBUTE	PVC-Encapsulation-Type			39	integer
ATTRIBUTE	PVC-Profile-Name			40	string
ATTRIBUTE	PVC-Circuit-Padding			41	integer
ATTRIBUTE	Bind-Type				42	integer
ATTRIBUTE	Bind-Auth-Protocol			43	integer
ATTRIBUTE	Bind-Auth-Max-Sessions			44	integer
ATTRIBUTE	Bind-Bypass-Bypass			45	string
ATTRIBUTE	Bind-Auth-Context			46	string
ATTRIBUTE	Bind-Auth-Service-Grp			47	string
ATTRIBUTE	Bind-Bypass-Context			48	string
ATTRIBUTE	Bind-Int-Context			49	string
ATTRIBUTE	Bind-Tun-Context			50	string
ATTRIBUTE	Bind-Ses-Context			51	string
ATTRIBUTE	Bind-Dot1q-Slot				52	integer
ATTRIBUTE	Bind-Dot1q-Port				53	integer
ATTRIBUTE	Bind-Dot1q-Vlan-Tag-Id			54	integer
ATTRIBUTE	Bind-Int-Interface-Name			55	string
ATTRIBUTE	Bind-L2TP-Tunnel-Name			56	string
ATTRIBUTE	Bind-L2TP-Flow-Control			57	integer
ATTRIBUTE	Bind-Sub-User-At-Context		58	string
ATTRIBUTE	Bind-Sub-Password			59	string
ATTRIBUTE	Ip-Host-Addr				60	string
ATTRIBUTE	IP-TOS-Field				61	integer
ATTRIBUTE	NAS-Real-Port				62	integer
ATTRIBUTE	Tunnel-Session-Auth-Ctx			63	string
ATTRIBUTE	Tunnel-Session-Auth-Service-Grp		64	string
ATTRIBUTE	Tunnel-Rate-Limit-Rate			65	integer
ATTRIBUTE	Tunnel-Rate-Limit-Burst			66	integer
ATTRIBUTE	Tunnel-Police-Rate			67	integer
ATTRIBUTE	Tunnel-Police-Burst			68	integer
ATTRIBUTE	Tunnel-L2F-Second-Password		69	string
ATTRIBUTE	ACL-Definition				70	string
ATTRIBUTE	PPPoE-IP-Route-Add			71	string
ATTRIBUTE	TTY-Level-Max				72	integer
ATTRIBUTE	TTY-Level-Start				73	integer
ATTRIBUTE	Tunnel-Checksum				74	integer
ATTRIBUTE	Tunnel-Profile				75	string
ATTRIBUTE	Tunnel-Client-VPN			78	string
ATTRIBUTE	Tunnel-Server-VPN			79	string
ATTRIBUTE	Tunnel-Client-Rhost			80	string
ATTRIBUTE	Tunnel-Server-Rhost			81	string
ATTRIBUTE	Tunnel-Client-Int-Addr			82	ipaddr
ATTRIBUTE	Tunnel-Server-Int-Addr			83	ipaddr
ATTRIBUTE	PPP-Compression				84	integer
ATTRIBUTE	Tunnel-Hello-Timer			85	integer
ATTRIBUTE	Redback-Reason				86	integer
ATTRIBUTE	Qos-Policing-Profile-Name		87	string
ATTRIBUTE	Qos-Metering-Profile-Name		88	string
ATTRIBUTE	Qos-Policy-Queuing			89	string
ATTRIBUTE	IGMP-Service-Profile-Name		90	string
ATTRIBUTE	Subscriber-Profile-Name			91	string
ATTRIBUTE	Forward-Policy				92	string
ATTRIBUTE	Remote-Port				93	string
ATTRIBUTE	Reauth					94	string
ATTRIBUTE	Reauth-More				95	integer
ATTRIBUTE	Agent-Remote-Id				96	string
ATTRIBUTE	Agent-Circuit-Id			97	string
ATTRIBUTE	Platform-Type				98	integer
ATTRIBUTE	Client-NBNS-Pri				99	ipaddr
ATTRIBUTE	Client-NBNS-Sec				100	ipaddr
ATTRIBUTE	Shaping-Profile-Name			101	string
ATTRIBUTE	BG-Cct-Addr-Max				103	integer
ATTRIBUTE	IP-Interface-Name			104	string
ATTRIBUTE	NAT-Policy-Name				105	string
ATTRIBUTE	RB-NPM-Service-Id			106	string
ATTRIBUTE	HTTP-Redirect-Profile-Name		107	string
ATTRIBUTE	Bind-Auto-Sub-User			108	string
ATTRIBUTE	Bind-Auto-Sub-Context			109	string
ATTRIBUTE	Bind-Auto-Sub-Password			110	string
ATTRIBUTE	Circuit-Protocol-Encap			111	integer
ATTRIBUTE	OS-Version				112	string
ATTRIBUTE	Session-Traffic-Limit			113	string
ATTRIBUTE	QOS-Reference				114	string
ATTRIBUTE	Rate-Limit-Excess-Burst			121	octets
ATTRIBUTE	Police-Excess-Burst			122	octets
ATTRIBUTE	Tunnel-Rate-Limit-Excess-Burst		123	octets
ATTRIBUTE	Tunnel-Police-Excess-Burst		124	octets
ATTRIBUTE	DHCP-Vendor-Class-ID			125	string
ATTRIBUTE	Qos-Rate				126	string
ATTRIBUTE	DHCP-Vendor-Encap-Option		127	string
ATTRIBUTE	Acct-Input-Octets-64			128	octets
ATTRIBUTE	Acct-Output-Octets-64			129	octets
ATTRIBUTE	Acct-Input-Packets-64			130	octets
ATTRIBUTE	Acct-Output-Packets-64			131	octets
ATTRIBUTE	Assigned-IP-Address			132	ipaddr
ATTRIBUTE	Acct-Mcast-In-Octets-64			133	octets
ATTRIBUTE	Acct-Mcast-Out-Octets-64		134	octets
ATTRIBUTE	Acct-Mcast-In-Packets-64		135	octets
ATTRIBUTE	Acct-Mcast-Out-Packets-64		136	octets
ATTRIBUTE	LAC-Port				137	integer
ATTRIBUTE	LAC-Real-Port				138	integer
ATTRIBUTE	LAC-Port-Type				139	integer
ATTRIBUTE	LAC-Real-Port-Type			140	integer
ATTRIBUTE	Acct-Dyn-Ac-Ent				141	string
ATTRIBUTE	Session-Error-Code			142	integer
ATTRIBUTE	Session-Error-Msg			143	string
ATTRIBUTE	Acct-Update-Reason			144	integer
ATTRIBUTE	Mac-Addr				145	string
ATTRIBUTE	Vlan-Source-Info			146	string
ATTRIBUTE	Acct-Mcast-In-Octets			147	integer
ATTRIBUTE	Acct-Mcast-Out-Octets			148	integer
ATTRIBUTE	Acct-Mcast-In-Packets			149	integer
ATTRIBUTE	Acct-Mcast-Out-Packets			150	integer
ATTRIBUTE	Reauth-Session-Id			151	string
ATTRIBUTE	QOS-Rate-Inbound			156	string
ATTRIBUTE	QOS-Rate-Outbound			157	string
ATTRIBUTE	Route-Tag				158	integer
ATTRIBUTE	LI-Id					159	integer
ATTRIBUTE	LI-Md-Address				160	ipaddr
ATTRIBUTE	LI-Md-Port				161	integer
ATTRIBUTE	LI-Action				162	integer
ATTRIBUTE	LI-Profile				163	string
ATTRIBUTE	Dynamic-Policy-Filter			164	string
ATTRIBUTE	HTTP-Redirect-URL			165	string
ATTRIBUTE	DSL-Actual-Rate-Up			166	integer
ATTRIBUTE	DSL-Actual-Rate-Down			167	integer
ATTRIBUTE	DSL-Min-Rate-Up				168	integer
ATTRIBUTE	DSL-Min-Rate-Down			169	integer
ATTRIBUTE	DSL-Attainable-Rate-Up			170	integer
ATTRIBUTE	DSL-Attainable-Rate-Down		171	integer
ATTRIBUTE	DSL-Max-Rate-Up				172	integer
ATTRIBUTE	DSL-Max-Rate-Down			173	integer
ATTRIBUTE	DSL-Min-Low-Power-Rate-Up		174	integer
ATTRIBUTE	DSL-Min-Low-Power-Rate-Down		175	integer
ATTRIBUTE	DSL-Max-Inter-Delay-Up			176	integer
ATTRIBUTE	DSL-Actual-Inter-Delay-Up		177	integer
ATTRIBUTE	DSL-Max-Inter-Delay-Down		178	integer
ATTRIBUTE	DSL-Actual-Inter-Delay-Down		179	integer
ATTRIBUTE	DSL-Line-State				180	integer
ATTRIBUTE	DSL-L2-Encapsulation			181	integer
ATTRIBUTE	DSL-Transmission-System			182	integer
ATTRIBUTE	DSL-PPPOA-PPPOE-Inter-Work-Flag		183	integer
ATTRIBUTE	DSL-Actual-Rate-Down-Factor		185	integer
ATTRIBUTE	DSL-Combined-Line-Info			184	string
ATTRIBUTE	Class-Volume-limit			186	string
ATTRIBUTE	Class-Volume-In-Counter			187	string
ATTRIBUTE	Class-Volume-Out-Counter		188	string
ATTRIBUTE	Flow-FAC-Profile			189	string
ATTRIBUTE	Flow-FAC-Profile			189	string
ATTRIBUTE	Service-Name				190	string
ATTRIBUTE	Service-Action				191	integer
ATTRIBUTE	Service-Parameter			192	string
ATTRIBUTE	Service-Error-Cause			193	integer
ATTRIBUTE	Deactivate-Service-Name			194	string
ATTRIBUTE	Qos-Profile-Overhead			195	string
ATTRIBUTE	Dynamic-QoS-Param			196	string
ATTRIBUTE	Acct-Alt-Session-ID			197	string
ATTRIBUTE	Idle-Timeout-Threshold			198	integer
ATTRIBUTE	Double-Authentication			199	integer
ATTRIBUTE	SBC-Adjacency				200	string
ATTRIBUTE	DHCP-Field				201	octets
ATTRIBUTE	DHCP-Option				202	octets
ATTRIBUTE	Security-Service			203	string
ATTRIBUTE	Reauth-Service-Name			204	string
ATTRIBUTE	Flow-IP-Profile				205	string
ATTRIBUTE	Radius-Throttle-Watermark		206	integer
ATTRIBUTE	RB-IPV6-DNS				207	string
ATTRIBUTE	RB-IPv6-Option				208	string
ATTRIBUTE	Cluster-Partition-ID			209	string
ATTRIBUTE	Circuit-Group-Member			210	string
ATTRIBUTE	Delegated-Max-Prefix			212	integer
ATTRIBUTE	IPv4-Address-Release-Control		213	string
ATTRIBUTE	Acct-Input-IPv4-Octet			214	integer
ATTRIBUTE	Acct-Output-IPv4-Octets			215	integer
ATTRIBUTE	Acct-Input-IPv4-Packets			216	integer
ATTRIBUTE	Acct-Output-IPv4-Packets		217	integer
ATTRIBUTE	Acct-Input-IPv4-Gigawords		218	integer
ATTRIBUTE	Acct-Output-IPv4-Gigawords		219	integer
ATTRIBUTE	Acct-Input-IPv6-Octets			220	integer
ATTRIBUTE	Acct-Output-IPv6-Octets			221	integer
ATTRIBUTE	Acct-Input-IPv6-Packets			222	integer
ATTRIBUTE	Acct-Output-IPv6-Packets		223	integer
ATTRIBUTE	Acct-Input-IPv6-Gigawords		224	integer
ATTRIBUTE	Acct-Output-IPv6-Gigawords		225	integer

VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-RAW	1
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-ROUTE1483 2
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-AUTO1483	3
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-MULTI	4
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-BRIDGE1483 5
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-PPP	6
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-PPP-SERIAL 7
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-PPP-NLPID 8
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-PPP-AUTO	9
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-PPPOE	10
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-L2TP	11
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-PPP-LLC	12
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-AUTO1490 13
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-MULTI	14
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-BRIDGE1490 15
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-PPP	16
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-PPP-AUTO 17
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-PPPOE	18
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-ROUTE1490 19
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-FRAME-L2TP	20
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-L2TP-VC-MUXED 21
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH		22
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH-PPPOE	23
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH-MULTI	24
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH-DOT1Q	25
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH-DOT1Q-PPPOE 26
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-MULTI-PPPOE 27
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-MULTI-IPV6OE 28
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ATM-MULTI-PPPOE-N-IPV6OE 29
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH-DOT1Q-TUNNEL 30
VALUE	PVC-Encapsulation-Type		AAA-ENCAPS-ETH-DOT1Q-TUNNEL-PPPOE 31

VALUE	PVC-Circuit-Padding		AAA-CIRCUIT-PADDING	1
VALUE	PVC-Circuit-Padding		AAA-CIRCUIT-NO-PADDING	2
VALUE	Bind-Type			AAA-AUTH-BIND		1
VALUE	Bind-Type			AAA-BYPASS-BIND		2
VALUE	Bind-Type			AAA-INTERFACE-BIND	3
VALUE	Bind-Type			AAA-SUBSCRIBE-BIND	4
VALUE	Bind-Type			AAA-TUNNEL-BIND		5
VALUE	Bind-Type			AAA-SESSION-BIND	6
VALUE	Bind-Type			AAA-Q8021-BIND		7
VALUE	Bind-Type			AAA-MULTI-BIND		8
VALUE	Bind-Type			AAA-DHCP-BIND		9
VALUE	Bind-Type			AAA-MULTI-BIND-SUB	10
VALUE	Bind-Type			AAA-BRIDGE-GROUP-BIND	11
VALUE	Bind-Type			AAA-VLAN-BIND		12
VALUE	Bind-Type			AAA-VLAN-GROUP-BIND	13
VALUE	Bind-Type			AAA-AUTO-SUBSCRIBER-BIND 14
VALUE	Bind-Auth-Protocol		AAA-PPP-PAP		1
VALUE	Bind-Auth-Protocol		AAA-PPP-CHAP		2
VALUE	Bind-Auth-Protocol		AAA-PPP-CHAP-WAIT	3
VALUE	Bind-Auth-Protocol		AAA-PPP-CHAP-PAP	4
VALUE	Bind-Auth-Protocol		AAA-PPP-CHAP-WAIT-PAP	5
VALUE	Bind-Auth-Protocol		AAA-PPP-EAP		6
VALUE	Bind-Auth-Protocol		AAA-PPP-PAP-CHAP	7
VALUE	Bind-Auth-Protocol		AAA-PPP-PAP-CHAP-WAIT	8

VALUE	Source-Validation		Enabled			1
VALUE	Source-Validation		Disabled		2
VALUE	Tunnel-Domain			Enabled			1
VALUE	Tunnel-Domain			Disabled		2
VALUE	Tunnel-Function			LAC-Only		1
VALUE	Tunnel-Function			LNS-Only		2
VALUE	Tunnel-Function			LAC-LNS			3
VALUE	Tunnel-Session-Auth		CHAP			1
VALUE	Tunnel-Session-Auth		PAP			2
VALUE	Tunnel-Session-Auth		CHAP-PAP		3
VALUE	Tunnel-Group			Enabled			1
VALUE	Tunnel-Group			Disabled		2
VALUE	Tunnel-Algorithm		First			1
VALUE	Tunnel-Algorithm		Load-Balance		2
VALUE	Tunnel-Algorithm		WRR			3
VALUE	Mcast-Send			NO-SEND			1
VALUE	Mcast-Send			SEND			2
VALUE	Mcast-Send			UNSOLICITED-SEND	3
VALUE	Mcast-Receive			NO-RECEIVE		1
VALUE	Mcast-Receive			RECEIVE			2

VALUE	Tunnel-DNIS			DNIS			1
VALUE	Tunnel-DNIS			DNIS-Only		2
VALUE	Tunnel-DNIS			DNIS-Generate		4

VALUE	Platform-Type			SMS			1
VALUE	Platform-Type			SmartEdge-800		2
VALUE	Platform-Type			SE-400			3
VALUE	Platform-Type			SE-100			4

VALUE	Circuit-Protocol-Encap		ENCAPS-PPPOE		27

VALUE	Medium-Type			DSL			11
VALUE	Medium-Type			Cable			12
VALUE	Medium-Type			Wireless		13
VALUE	Medium-Type			Satellite		14

VALUE	IP-TOS-Field			normal			0
VALUE	IP-TOS-Field			min-cost-only		1
VALUE	IP-TOS-Field			max-reliability-only	2
VALUE	IP-TOS-Field			max-reliability-plus-min-cost 3
VALUE	IP-TOS-Field			max-throughput-only	4
VALUE	IP-TOS-Field			max-throughput-plus-min-cost 5
VALUE	IP-TOS-Field			max-throughput-plus-max-reliability 6
VALUE	IP-TOS-Field			max-throughput-plus-max-reliability-plus-min-cost 7
VALUE	IP-TOS-Field			min-delay-only		8
VALUE	IP-TOS-Field			min-delay-plus-min-cost	9
VALUE	IP-TOS-Field			min-delay-plus-max-reliability 10
VALUE	IP-TOS-Field			min-delay-plus-max-reliability-plus-min-cost 11
VALUE	IP-TOS-Field			min-delay-plus-max-throughput 12
VALUE	IP-TOS-Field			min-delay-plus-max-throughput-plus-min-cost 13
VALUE	IP-TOS-Field			min-delay-plus-max-throughput-plus-max-reliability 14
VALUE	IP-TOS-Field			min-delay-plus-max-throughput-plus-max-reliability-plus-min-cost 15

VALUE	LAC-Port-Type			NAS-PORT-TYPE-10BT	40
VALUE	LAC-Port-Type			NAS-PORT-TYPE-100BT	41
VALUE	LAC-Port-Type			NAS-PORT-TYPE-DS3-FR	42
VALUE	LAC-Port-Type			NAS-PORT-TYPE-DS3-ATM	43
VALUE	LAC-Port-Type			NAS-PORT-TYPE-OC3	44
VALUE	LAC-Port-Type			NAS-PORT-TYPE-HSSI	45
VALUE	LAC-Port-Type			NAS-PORT-TYPE-EIA530	46
VALUE	LAC-Port-Type			NAS-PORT-TYPE-T1	47
VALUE	LAC-Port-Type			NAS-PORT-TYPE-CHAN-T3	48
VALUE	LAC-Port-Type			NAS-PORT-TYPE-DS1-FR	49
VALUE	LAC-Port-Type			NAS-PORT-TYPE-E3-ATM	50
VALUE	LAC-Port-Type			NAS-PORT-TYPE-IMA-ATM	51
VALUE	LAC-Port-Type			NAS-PORT-TYPE-DS3-ATM-2	52
VALUE	LAC-Port-Type			NAS-PORT-TYPE-OC3-ATM-2	53
VALUE	LAC-Port-Type			NAS-PORT-TYPE-1000BSX	54
VALUE	LAC-Port-Type			NAS-PORT-TYPE-E1-FR	55
VALUE	LAC-Port-Type			NAS-PORT-TYPE-E1-ATM	56
VALUE	LAC-Port-Type			NAS-PORT-TYPE-E3-FR	57
VALUE	LAC-Port-Type			NAS-PORT-TYPE-OC3-POS	58
VALUE	LAC-Port-Type			NAS-PORT-TYPE-OC12-POS	59
VALUE	LAC-Port-Type			NAS-PORT-TYPE-PPPOE	60
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-10BT	40
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-100BT	41
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-DS3-FR	42
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-DS3-ATM	43
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-OC3	44
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-HSSI	45
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-EIA530	46
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-T1	47
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-CHAN-T3	48
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-DS1-FR	49
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-E3-ATM	50
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-IMA-ATM	51
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-DS3-ATM-2	52
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-OC3-ATM-2	53
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-1000BSX	54
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-E1-FR	55
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-E1-ATM	56
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-E3-FR	57
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-OC3-POS	58
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-OC12-POS	59
VALUE	LAC-Real-Port-Type		NAS-PORT-TYPE-PPPOE	60

# Although Ericsson-AB uses - instead of _ in the Attributes, these values are listed
# with _ in the latest (6.1.4.4) documentation, so I have entered them as so
# graeme

VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_SESSION_UP 1
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_SESSION_DOWN 2
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_PERIODIC	3
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_DYN_AC_ENT_START 4
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_DYN_AC_ENT_STOP 5
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_DYN_AC_ENT_TIMEOUT 6
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_SUBSCRIBER_REAUTHOR 7
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_PPP_IPCP_UP 8
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_PPP_MP_LINK_UP 9
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_DHCP_IP_ADDR_GRANTED 10
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_DHCP_IP_ADDR_RELEASED 11
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_ACL_TIMERED_ACTION 12
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_ACL_ACTION 13
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_CMD	14
VALUE	Acct-Update-Reason		AAA_LOAD_ACCT_TEST	15

VALUE	DSL-Line-State			Showtime		1
VALUE	DSL-Line-State			Idle			2
VALUE	DSL-Line-State			Silent			3

VALUE	DSL-Transmission-System		ADSL1			1
VALUE	DSL-Transmission-System		ADSL2			2
VALUE	DSL-Transmission-System		ADSL2+		3
VALUE	DSL-Transmission-System		VDSL1			4
VALUE	DSL-Transmission-System		VDSL2			5
VALUE	DSL-Transmission-System		SDSL			6
VALUE	DSL-Transmission-System		UNKNOWN			7

VALUE	Service-Action			DE-ACTIVATE		0
VALUE	Service-Action			ACTIVATE-WITH-ACCT	1
VALUE	Service-Action			ACTIVATE-WITHOUT-ACCT	2

END-VENDOR	Ericsson-AB
