# -*- text -*-
# Copyright (C) 2015 The FreeRADIUS Server project and contributors
##############################################################################
#
#	ASN Attributes.
#
#	Taken from http://svn.asn.pl/misc/freeradius/dictionary.asn
#
#	$Id: 97fc9f140da31dd0d6958c5133979dadc12815fd $
#
##############################################################################

VENDOR		ASN				23782

BEGIN-VENDOR	ASN

## Server-side extensions
# dynamic IP pool name
ATTRIBUTE	ASN-IP-Pool-Name			1	string

### 2-99: free ###

## limits
ATTRIBUTE	ASN-Kbps-Down				100	integer
ATTRIBUTE	ASN-Kbps-Down-Localmedia		112	integer
ATTRIBUTE	ASN-Kbps-Up				101	integer
ATTRIBUTE	ASN-Pps-Down				102	integer
ATTRIBUTE	ASN-Pps-Up				103	integer
ATTRIBUTE	ASN-TCP-Connlimit			104	integer

## firewall
ATTRIBUTE	ASN-Firewall-Available			110	integer
VALUE	ASN-Firewall-Available		Yes			1
VALUE	ASN-Firewall-Available		No			2

ATTRIBUTE	ASN-Firewall-State			105	integer
VALUE	ASN-Firewall-State		Enabled			1
VALUE	ASN-Firewall-State		Disabled		2

ATTRIBUTE	ASN-Firewall-Block-Ping			107	integer
VALUE	ASN-Firewall-Block-Ping		Enabled			1
VALUE	ASN-Firewall-Block-Ping		Disabled		2

# hosts to allow "<tcp/udp/sctp> <host> <port1,port2,...>"
ATTRIBUTE	ASN-Firewall-Open			106	string

## QoS
ATTRIBUTE	ASN-QoS-Available			111	integer
VALUE	ASN-QoS-Available		Yes			1
VALUE	ASN-QoS-Available		No			2

ATTRIBUTE	ASN-QoS-State				108	integer
VALUE	ASN-QoS-State			Enabled			1
VALUE	ASN-QoS-State			Disabled		2

# IP redirection, with optional randomness
#  "<tcp/udp/sctp> src/dst [<dsthost[/mask]>:]<port1,port2,...> <host>:<port> [<random%>]"
# where src/dst decides whether to match source or destination ports
#       random is an integer number from 1 to 99, or null - no randomness
ATTRIBUTE	ASN-IP-Redirect				109	string

## web filtering
# decides whether to deny or to allow only the specified web topics
ATTRIBUTE	ASN-Webfilter-Mode			113	integer
VALUE	ASN-Webfilter-Mode		Deny			1
VALUE	ASN-Webfilter-Mode		Allow			2

# where to redirect blocked request
#  "[301:302]<new url>"
#  301/302   - redirect permanently (301) or temporarily (302) (default 302)
#  <new url> - an URL address, with following possible substitutions:
#    %a - IP address of the client
#    %i - user ID (RFC931) or "unknown"
#    %n - domainname of the client or "unknown"
#    %p - REQUEST_URI, ie. the path and the optional
#         query string of %u, but note for convenience
#         without the leading "/".
#    %t - matched destination group or "unknown"
#    %u - requested URL
#    %% - single '%'
#
ATTRIBUTE	ASN-Webfilter-Redirect			114	string

# squidGuard destination group to match
#   destinations available by default: sglists-<tag> - tags:
#   ads adult audioandvideo banks blogs chatandforum finance freemail games
#   home jobsearch keylogger news onlineGames phishing proxies recreation
#   reference science searchengine
ATTRIBUTE	ASN-Webfilter-Destination		115	string

# web domain to match (will match all subdomains, too)
ATTRIBUTE	ASN-Webfilter-Domain			116	string

END-VENDOR                             ASN
